<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="24.13" x2="0" y2="1.27" width="0.254" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="21.59" y2="0" width="0.254" layer="20"/>
<wire x1="21.59" y1="0" x2="22.86" y2="1.27" width="0.254" layer="20" curve="90"/>
<wire x1="22.86" y1="1.27" x2="22.86" y2="24.13" width="0.254" layer="20"/>
<wire x1="22.86" y1="24.13" x2="21.59" y2="25.4" width="0.254" layer="20" curve="90"/>
<wire x1="21.59" y1="25.4" x2="1.27" y2="25.4" width="0.254" layer="20"/>
<wire x1="1.27" y1="25.4" x2="0" y2="24.13" width="0.254" layer="20" curve="90"/>
<text>xlab.stanford.edu</text>
<text>XTB-10</text>
<text>Holliday
2018</text>
<text>LYR1</text>
<text>LYR2</text>
<text>LYR3</text>
<text>LYR4</text>
<text>xlab.stanford.edu</text>
<text>XTB-10</text>
<text>8</text>
<text>15</text>
<text>22</text>
<text>INA188</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="User-Submitted">
<description>&lt;h3&gt;SparkFun User Contributed Parts&lt;/h3&gt;
In this library you'll find submitted parts from SparkFun users everywhere!&lt;br&gt;&lt;br&gt;
These are not necessarily parts we carry, but are parts that other users have determined function well with other parts in our libraries. Please keep in mind that it is the end user's responsibility to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;&lt;br&gt;
If you find these parts useful, please consider helping the open-source community by contributing your own through &lt;a href="https://github.com/sparkfun/SparkFun-Eagle-Libraries"&gt;GitHub.&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="maholli">
<packages>
<package name="RHB0032H">
</package>
<package name="D0008A_N">
</package>
<package name="HVQFN28">
<description>&lt;b&gt;HVQFN28: plastic thermal enhanced very thin quad flat package&lt;/b&gt; SOT788-1&lt;p&gt;
no leads; 28 terminals; body 6 x 6 x 0.85 mm&lt;br&gt;
Source: &lt;a href="http://www.nxp.com/documents/data_sheet/P89LPC933_934_935_936.pdf"&gt; Data sheet&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Max Holliday"/>
<attribute name="VERSION" value="1"/>
</element>
<element name="Q10" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="Q7" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="Q4" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="Q2" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="Q1" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="Q5" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="Q3" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="Q9" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="Q8" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="U1" library="maholli" package="D0008A_N" value="Value">
<attribute name="ALTERNATEPARTNUMBER" value="INA188ID"/>
<attribute name="APPLICATION_BUILDNUMBER" value="*"/>
<attribute name="COMPTYPE" value="IC"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MOUNTTYPE" value="SMT"/>
<attribute name="PACKAGEREFERENCE" value="D0008A"/>
<attribute name="PARTNUMBER" value="INA188IDR"/>
<attribute name="PIN_COUNT" value="8"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="ROHS" value="Y"/>
<attribute name="TYPE" value="TYPE"/>
</element>
<element name="Q6" library="User-Submitted" package="SOT23-3" value="IRLML5103">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="U3" library="maholli" package="RHB0032H" value="Value">
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="NAME"/>
<attribute name="PARTNUMBER" value="ADS124S06IRHBR"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="TYPE" value="TYPE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603-RES" value="47">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value="47">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="47">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="47">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="U2" library="maholli" package="HVQFN28" value="M-QFN28"/>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="0.1UF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="47">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="47">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603" value="0.33uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="0.1UF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603-RES" value="47">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="Q2" pad="3"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="Q4" pad="1"/>
<contactref element="Q6" pad="1"/>
<contactref element="Q8" pad="1"/>
<contactref element="Q10" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="HALL1N">
<contactref element="Q2" pad="2"/>
<contactref element="U2" pad="27"/>
</signal>
<signal name="HALL2N">
<contactref element="Q1" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="HALL2P">
<contactref element="Q7" pad="3"/>
<contactref element="Q9" pad="3"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="HALL1P">
<contactref element="Q8" pad="3"/>
<contactref element="Q10" pad="3"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="HALL_EN2">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U3" pad="21"/>
</signal>
<signal name="GND">
<contactref element="Q6" pad="3"/>
<contactref element="Q5" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="U3" pad="27"/>
<contactref element="U3" pad="17"/>
<contactref element="U3" pad="24"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="28"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="7"/>
<contactref element="C6" pad="1"/>
<contactref element="U3" pad="33"/>
<contactref element="U3" pad="14"/>
<contactref element="U2" pad="28"/>
<contactref element="U2" pad="15"/>
<contactref element="U2" pad="16"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="22"/>
<contactref element="U2" pad="21"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="HALL_EN1">
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="U3" pad="22"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="Q5" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q7" pad="1"/>
<contactref element="Q9" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="HALL_AMP_OUT">
<contactref element="U1" pad="6"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="C3" pad="2"/>
<contactref element="U3" pad="16"/>
<contactref element="U3" pad="15"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="U3" pad="23"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="SPI_MISO">
<contactref element="U3" pad="12"/>
</signal>
<signal name="SPI_SCK">
<contactref element="U3" pad="11"/>
</signal>
<signal name="SPI_SS2">
<contactref element="U3" pad="9"/>
</signal>
<signal name="HALL_PWR">
<contactref element="R5" pad="2"/>
<contactref element="Q10" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="Q9" pad="2"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="U3" pad="10"/>
</signal>
<signal name="ADC_START">
<contactref element="U3" pad="8"/>
</signal>
<signal name="ADC_RST">
<contactref element="U3" pad="18"/>
</signal>
<signal name="N$12">
</signal>
<signal name="REF0_P">
<contactref element="U3" pad="30"/>
</signal>
<signal name="REF0_N">
<contactref element="U3" pad="29"/>
</signal>
<signal name="GPIO2">
<contactref element="U3" pad="20"/>
</signal>
<signal name="GPIO3">
<contactref element="U3" pad="19"/>
</signal>
<signal name="AIN2">
<contactref element="R8" pad="2"/>
<contactref element="U2" pad="24"/>
</signal>
<signal name="HALL_OUTN">
<contactref element="R10" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="HALL_OUTP">
<contactref element="R11" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q8" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="IDAC1">
<contactref element="U3" pad="32"/>
<contactref element="U2" pad="25"/>
</signal>
<signal name="IDAC2">
<contactref element="U3" pad="31"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R11" pad="1"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="1"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="R7" pad="1"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="U3" pad="7"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="AIN0">
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="AIN3">
<contactref element="R9" pad="1"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="U2" pad="20"/>
</signal>
<signal name="N$22">
<contactref element="U2" pad="19"/>
</signal>
<signal name="N$23">
<contactref element="U2" pad="18"/>
</signal>
<signal name="N$24">
<contactref element="U2" pad="17"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND2">
</signal>
<signal name="GND3">
</signal>
<signal name="GND5">
</signal>
<signal name="N$25">
<contactref element="U2" pad="23"/>
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$43">
</signal>
<signal name="N$6">
<contactref element="U3" pad="5"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U3" pad="4"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R12" pad="2"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="AVDD">
<contactref element="U3" pad="26"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="INA_VDD">
<contactref element="U1" pad="7"/>
<contactref element="C2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
