<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="24.384" y2="0" width="0" layer="20"/>
<wire x1="24.384" y1="0" x2="24.384" y2="22.86" width="0" layer="20"/>
<wire x1="24.384" y1="22.86" x2="0" y2="22.86" width="0" layer="20"/>
<wire x1="0" y1="22.86" x2="0" y2="0" width="0" layer="20"/>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>PPMI</text>
<text>VRF</text>
<text>GND</text>
<text>PPMO</text>
<text>VENC</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
</package>
<package name="VERTICAL_DIODE">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_NO_SILK">
</package>
<package name="1X03_NO_SILK">
</package>
</packages>
</library>
<library name="adafruit_08-30-2015">
<packages>
<package name="0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="v-reg-2">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Misc Passives">
<packages>
<package name="L_0.2_IN_SPACING">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit_08-30-2015" package="0309V" value="2.2k">
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit_08-30-2015" package="0309V" value="10k">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit_08-30-2015" package="0309V" value="220">
<attribute name="NAME"/>
</element>
<element name="R4" library="adafruit_08-30-2015" package="0309V" value="5.6k">
<attribute name="NAME"/>
</element>
<element name="R5" library="adafruit_08-30-2015" package="0309V" value="5.6k">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="100u">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="VERTICAL_DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L" library="Misc Passives" package="L_0.2_IN_SPACING" value="L">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="v-reg-2" package="78XXS" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="CAP-PTH-SMALL" value="330n">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Passives" package="CAP-PTH-SMALL" value="100n">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="OUT"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="D1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="L" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="IN"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="IC1" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="VENC">
<contactref element="Q1" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="PPMIN">
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="PPMRF">
<contactref element="R5" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="VRF">
<contactref element="L" pad="2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
