<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="124.46" y2="0" width="0" layer="20"/>
<wire x1="124.46" y1="0" x2="124.46" y2="20.31" width="0" layer="20"/>
<wire x1="124.46" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<text>resistors: 1k</text>
<text>VinoTemp v1 - Jul 2015</text>
</plain>
<libraries>
<library name="Dek">
<packages>
<package name="CAP-PTH-SMALL2">
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
<package name="STAND-OFF-#2">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="AXIAL-0.3">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="7-SEGMENT-DISPLAY-2-DIGIT-KINGBRIGHT-DA04">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_TALL">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X4">
</package>
<package name="MOLEX-1X2">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C14" library="Dek" package="CAP-PTH-SMALL2" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="C15" library="Dek" package="CAP-PTH-SMALL2" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C9" library="Dek" package="CAP-PTH-SMALL2" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="CTRL_HDR" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="IC4" library="Dek" package="DIL28-3" value="ATMEGA328">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="Dek" package="STAND-OFF-#2" value="STAND-OFF#2"/>
<element name="JP6" library="Dek" package="STAND-OFF-#2" value="STAND-OFF#2"/>
<element name="R1" library="Dek" package="AXIAL-0.3" value="5k5">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="VALUE"/>
</element>
<element name="TEMP" library="SparkFun-Connectors" package="MOLEX-1X2" value=""/>
<element name="Y1" library="Dek" package="HC49US" value="16MHz">
<attribute name="VALUE"/>
</element>
<element name="COMP" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Dek" package="7-SEGMENT-DISPLAY-2-DIGIT-KINGBRIGHT-DA04" value="7-SEGMENT-DISPLAY-2-DIGITPTH"/>
<element name="R4" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="UP" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_TALL" value="SWITCH-MOMENTARY-2SMD-4">
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DOWN" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_TALL" value="SWITCH-MOMENTARY-2SMD-4">
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C15" pad="1"/>
<contactref element="IC4" pad="22"/>
<contactref element="IC4" pad="8"/>
<contactref element="C14" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="CTRL_HDR" pad="3"/>
<contactref element="R1" pad="P$1"/>
<contactref element="COMP" pad="K"/>
<contactref element="DOWN" pad="A2"/>
<contactref element="UP" pad="A2"/>
</signal>
<signal name="VCC">
<contactref element="R3" pad="2"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC4" pad="20"/>
<contactref element="C15" pad="2"/>
<contactref element="IC4" pad="21"/>
<contactref element="CTRL_HDR" pad="4"/>
<contactref element="TEMP" pad="2"/>
<contactref element="U$1" pad="1COMM"/>
<contactref element="U$1" pad="2COMM"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="D6">
<contactref element="IC4" pad="12"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="Y1" pad="2"/>
<contactref element="IC4" pad="10"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="XTAL1">
<contactref element="IC4" pad="9"/>
<contactref element="Y1" pad="1"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="A1">
<contactref element="IC4" pad="24"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="A2">
<contactref element="IC4" pad="25"/>
<contactref element="UP" pad="B2"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="RST">
<contactref element="R3" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="TX">
<contactref element="IC4" pad="3"/>
</signal>
<signal name="RX">
<contactref element="IC4" pad="2"/>
</signal>
<signal name="A0">
<contactref element="IC4" pad="23"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="D4">
<contactref element="IC4" pad="6"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="D9">
<contactref element="IC4" pad="15"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="D10">
<contactref element="IC4" pad="16"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="D11">
<contactref element="IC4" pad="17"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="D12">
<contactref element="IC4" pad="18"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="D2">
<contactref element="IC4" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="A4">
<contactref element="IC4" pad="27"/>
<contactref element="TEMP" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="D5">
<contactref element="IC4" pad="11"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="D13">
<contactref element="IC4" pad="19"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="D7">
<contactref element="IC4" pad="13"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="D3">
<contactref element="IC4" pad="5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="A3">
<contactref element="IC4" pad="26"/>
<contactref element="DOWN" pad="B2"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="D8">
<contactref element="IC4" pad="14"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="A5">
<contactref element="IC4" pad="28"/>
<contactref element="CTRL_HDR" pad="2"/>
<contactref element="CTRL_HDR" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="COMP" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="1A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="1B"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="1C"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="1D"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="1E"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="1F"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="1G"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="2A"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="2B"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="2C"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="2D"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="2E"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="2F"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="2G"/>
<contactref element="R17" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
