<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="26.595225" y1="34.02" x2="3.44828125" y2="34.02" width="0" layer="20"/>
<wire x1="3.44828125" y1="34.02" x2="0" y2="30.57171875" width="0" layer="20" curve="90"/>
<wire x1="0" y1="30.57171875" x2="0" y2="14.713471875" width="0" layer="20"/>
<wire x1="0" y1="14.713471875" x2="14.713471875" y2="0" width="0" layer="20" curve="90"/>
<wire x1="14.713471875" y1="0" x2="29.94" y2="15.226528125" width="0" layer="20" curve="90"/>
<wire x1="29.94" y1="15.226528125" x2="29.94" y2="30.675225" width="0" layer="20"/>
<wire x1="29.94" y1="30.675225" x2="26.595225" y2="34.02" width="0" layer="20" curve="90"/>
<text>LT</text>
<text>RT</text>
<text>VCC</text>
<text>Switch Side</text>
<text>LT</text>
<text>RT</text>
<text>VCC</text>
<text>RV-Project.Com
Turn Switch
V1.1 3/4/21</text>
</plain>
<libraries>
<library name="a-lib">
<description>Archive Library (for old designs) - do not use for new components.</description>
<packages>
<package name="MO1-22AWG-SMALL">
</package>
<package name="DIODE-1N400X(NEW)">
<description>Pitch: 0.4"</description>
</package>
</packages>
</library>
<library name="a-lib_Switches">
<description>Thru-Hole Switches, Relays</description>
<packages>
<package name="ESWITCH-KC58">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="a-lib_Switches" package="ESWITCH-KC58" value=""/>
<element name="JP1" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="JP2" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="JP3" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value=""/>
<element name="JP4" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="JP5" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="D3" library="a-lib" package="DIODE-1N400X(NEW)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="a-lib" package="DIODE-1N400X(NEW)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="S1" pad="P$7"/>
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="S1" pad="P$4"/>
<contactref element="JP4" pad="P$1"/>
<contactref element="JP1" pad="P$1"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="S1" pad="P$10"/>
<contactref element="JP2" pad="P$1"/>
<contactref element="JP5" pad="P$1"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="S1" pad="P$A"/>
<contactref element="JP3" pad="P$1"/>
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
