<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="69.83" y2="0" width="0" layer="20"/>
<wire x1="69.83" y1="0" x2="69.83" y2="41.58" width="0" layer="20"/>
<wire x1="69.83" y1="41.58" x2="0" y2="41.58" width="0" layer="20"/>
<wire x1="0" y1="41.58" x2="0" y2="0" width="0" layer="20"/>
<text>POS</text>
<text>SIG</text>
<text>NEG</text>
<text>OUT</text>
<text>GND</text>
<text>PWR</text>
<text>GND</text>
<text>NC</text>
<text>NEG</text>
<text>SIG</text>
<text>POS</text>
<text>Feedback connect v002 03-05-2014</text>
</plain>
<libraries>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MKDSN1,5/3-5,08">
<description>&lt;b&gt;MKDSN 1,5/ 3-5,08&lt;/b&gt; Printklemme&lt;p&gt;
Nennstrom: 13,5 A&lt;br&gt;
Nennspannung: 250 V&lt;br&gt;
Rastermaß: 5,08 mm&lt;br&gt;
Polzahl: 3&lt;br&gt;
Anschlussart: Schraubanschluss&lt;br&gt;
Montage: Löten&lt;br&gt;
Anschlussrichtung Leiter/Platine: 0 °&lt;br&gt;
Artikelnummer: 1729131&lt;br&gt;
Source: http://eshop.phoenixcontact.com .. 1729131.pdf</description>
</package>
<package name="MKDSN1,5/2-5,08">
<description>&lt;b&gt;MKDSN 1,5/ 2-5,08&lt;/b&gt; Printklemme&lt;p&gt;
Nennstrom: 13,5 A&lt;br&gt;
Nennspannung: 250 V&lt;br&gt;
Rastermaß: 5,08 mm&lt;br&gt;
Polzahl: 2&lt;br&gt;
Anschlussart: Schraubanschluss&lt;br&gt;
Montage: Löten&lt;br&gt;
Anschlussrichtung Leiter/Platine: 0 °&lt;br&gt;
Artikelnummer: 1729128&lt;br&gt;
Source: http://eshop.phoenixcontact.com .. 1729128.pdf</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3223W">
<description>&lt;b&gt;3 mm SMD Trimming Potentiometer&lt;/b&gt; Top Adjust&lt;p&gt;
Source: http://www.bourns.com/data/global/PDFs/3223.PDF</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="EIA3216-KIT">
<description>&lt;h3&gt;EIA3216-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-3-2-07">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FEEDBACK" library="con-phoenix-508" package="MKDSN1,5/3-5,08" value="MKDSN1,5/3-5,08">
<attribute name="OC_NEWARK" value="70R0299"/>
<attribute name="MPN" value="SMKDSN1,5/3-5,08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792904"/>
<attribute name="NAME"/>
</element>
<element name="OUTPUT" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="OC_NEWARK" value="30M2397"/>
<attribute name="MPN" value="MKDSN 1,5/2-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792903"/>
<attribute name="NAME"/>
</element>
<element name="MANUAL" library="con-phoenix-508" package="MKDSN1,5/3-5,08" value="MKDSN1,5/3-5,08">
<attribute name="OC_NEWARK" value="70R0299"/>
<attribute name="MPN" value="SMKDSN1,5/3-5,08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792904"/>
<attribute name="NAME"/>
</element>
<element name="POWER" library="con-phoenix-508" package="MKDSN1,5/3-5,08" value="MKDSN1,5/3-5,08">
<attribute name="OC_NEWARK" value="70R0299"/>
<attribute name="MPN" value="SMKDSN1,5/3-5,08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792904"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="pot" package="3223W" value=""/>
<element name="R2" library="pot" package="3223W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="DIL08" value="LM358N"/>
<element name="R3" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="EIA3216-KIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="EIA3216-KIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+15" library="SparkFun-3-2-07" package="LED-1206" value=""/>
<element name="-15" library="SparkFun-3-2-07" package="LED-1206" value=""/>
<element name="R8" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL1" library="con-amp-quick" package="03P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SL2" library="con-amp-quick" package="03P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SL3" library="con-amp-quick" package="03P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL4" library="con-amp-quick" package="03P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+7V">
<contactref element="R1" pad="2"/>
<contactref element="FEEDBACK" pad="1"/>
<contactref element="MANUAL" pad="1"/>
<contactref element="SL2" pad="3"/>
<contactref element="SL3" pad="3"/>
</signal>
<signal name="-8V">
<contactref element="R2" pad="2"/>
<contactref element="FEEDBACK" pad="3"/>
<contactref element="MANUAL" pad="3"/>
<contactref element="SL2" pad="1"/>
<contactref element="SL3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="7"/>
<contactref element="R7" pad="2"/>
<contactref element="OUTPUT" pad="1"/>
<contactref element="SL4" pad="1"/>
</signal>
<signal name="-15V">
<contactref element="IC1" pad="4"/>
<contactref element="C2" pad="C"/>
<contactref element="POWER" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="-15" pad="A"/>
<contactref element="SL1" pad="3"/>
</signal>
<signal name="+15V">
<contactref element="IC1" pad="8"/>
<contactref element="C1" pad="A"/>
<contactref element="POWER" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="+15" pad="C"/>
<contactref element="SL1" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="OUTPUT" pad="2"/>
<contactref element="POWER" pad="2"/>
<contactref element="C2" pad="A"/>
<contactref element="C1" pad="C"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="SL1" pad="2"/>
<contactref element="SL4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="FEEDBACK" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="SL2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="MANUAL" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="SL3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R8" pad="2"/>
<contactref element="+15" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R9" pad="2"/>
<contactref element="-15" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
