<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.514" y2="0" width="0" layer="20"/>
<wire x1="21.514" y1="0" x2="21.514" y2="22.85" width="0" layer="20"/>
<wire x1="21.514" y1="22.85" x2="0" y2="22.85" width="0" layer="20"/>
<wire x1="0" y1="22.85" x2="0" y2="0" width="0" layer="20"/>
<text>Order Switcher</text>
<text>Quantum Effects 2016</text>
</plain>
<libraries>
<library name="Eigene_Kreationen">
<packages>
<package name="OCTO-PAD">
</package>
<package name="ROUND-PAD">
</package>
<package name="GND-PAD">
</package>
</packages>
</library>
<library name="switches">
<packages>
<package name="4PDT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IN1" library="Eigene_Kreationen" package="OCTO-PAD" value="In1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="IN2" library="Eigene_Kreationen" package="OCTO-PAD" value="In2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="OUT1" library="Eigene_Kreationen" package="OCTO-PAD" value="Out1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="OUT2" library="Eigene_Kreationen" package="OCTO-PAD" value="Out2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="RETURN1" library="Eigene_Kreationen" package="ROUND-PAD" value="Return1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="RETURN2" library="Eigene_Kreationen" package="ROUND-PAD" value="Return2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SEND1" library="Eigene_Kreationen" package="ROUND-PAD" value="Send1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SEND2" library="Eigene_Kreationen" package="ROUND-PAD" value="Send2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="switches" package="4PDT" value=""/>
<element name="U$1" library="Eigene_Kreationen" package="GND-PAD" value="GND-PAD"/>
<element name="U$2" library="Eigene_Kreationen" package="GND-PAD" value="GND-PAD"/>
<element name="U$3" library="Eigene_Kreationen" package="GND-PAD" value="GND-PAD"/>
<element name="U$4" library="Eigene_Kreationen" package="GND-PAD" value="GND-PAD"/>
<element name="U$5" library="Eigene_Kreationen" package="GND-PAD" value="GND-PAD"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="SW1" pad="P$1"/>
<contactref element="SEND1" pad="P$1"/>
<contactref element="SW1" pad="P$9"/>
</signal>
<signal name="N$3">
<contactref element="SW1" pad="P$5"/>
<contactref element="OUT1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="SW1" pad="P$8"/>
<contactref element="IN2" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="SW1" pad="P$11"/>
<contactref element="OUT2" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="RETURN1" pad="P$1"/>
<contactref element="SW1" pad="P$4"/>
<contactref element="SW1" pad="P$12"/>
</signal>
<signal name="N$7">
<contactref element="SEND2" pad="P$1"/>
<contactref element="SW1" pad="P$3"/>
<contactref element="SW1" pad="P$7"/>
</signal>
<signal name="N$8">
<contactref element="SW1" pad="P$10"/>
<contactref element="RETURN2" pad="P$1"/>
<contactref element="SW1" pad="P$6"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="SW1" pad="P$2"/>
<contactref element="IN1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
