<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="11.3032" y2="0" width="0" layer="20"/>
<wire x1="11.3032" y1="0" x2="11.3032" y2="15.4332" width="0" layer="20"/>
<wire x1="11.3032" y1="15.4332" x2="0" y2="15.4332" width="0" layer="20"/>
<wire x1="0" y1="15.4332" x2="0" y2="0" width="0" layer="20"/>
<text>3.3V</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<text>ALR</text>
<text>RST</text>
<text>TMP102</text>
<text>MPL115A2</text>
<text>U1</text>
<text>U2</text>
<text>Barom Sensor Board</text>
<text>Rev. 1.3</text>
<text>2013</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT563">
</package>
<package name="LGA8">
<description>&lt;h4&gt;LGA8 Package&lt;/h4&gt; &lt;B&gt;**UNPROVEN**&lt;/b&gt;
&lt;ul&gt;&lt;li&gt; 5.0x3.0x1.2mm&lt;/li&gt;
&lt;li&gt;8-pad&lt;/li&gt;&lt;br&gt;&lt;/ul&gt;
Used in MPL115A1 -</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TMP102" library="SparkFun-Sensors" package="SOT563" value="TMP102"/>
<element name="JP1" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-Sensors" package="LGA8" value="MPL115A"/>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="TMP102" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="TMP102" pad="4"/>
</signal>
<signal name="3.3V">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="TMP102" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="4"/>
<contactref element="TMP102" pad="6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="3"/>
<contactref element="TMP102" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="MPL_RST">
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="ALERT">
<contactref element="TMP102" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
