<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="17.1" x2="0" y2="4.95" width="0" layer="20"/>
<wire x1="0" y1="4.95" x2="4.95" y2="0" width="0" layer="20"/>
<wire x1="4.95" y1="0" x2="9.3" y2="0" width="0" layer="20"/>
<wire x1="9.3" y1="0" x2="14.3" y2="5" width="0" layer="20"/>
<wire x1="14.3" y1="5" x2="14.3" y2="17" width="0" layer="20"/>
<wire x1="14.3" y1="17" x2="9.5" y2="21.8" width="0" layer="20"/>
<wire x1="9.5" y1="21.8" x2="4.7" y2="21.8" width="0" layer="20"/>
<wire x1="4.7" y1="21.8" x2="0" y2="17.1" width="0" layer="20"/>
<hole x="7.1" y="20" drill="2.2"/>
<hole x="7.1" y="2" drill="2.2"/>
<text>V</text>
<text>G</text>
<text>S</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SKQUCAA010">
<description>&lt;Alps, SKQUCAA010, 2 Way Joystick Switch Plunger, Momentary, 12V dc&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SKQUCAA010">
<description>&lt;b&gt;SKQUCAA010-3&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="S2" library="SKQUCAA010" package="SKQUCAA010" value="SKQUCAA010">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="Alps, SKQUCAA010, 2 Way Joystick Switch Plunger, Momentary, 12V dc"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="MANUFACTURER_NAME" value="ALPS"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SKQUCAA010"/>
<attribute name="MOUSER_PART_NUMBER" value="688-SKQUCA"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/ALPS/SKQUCAA010?qs=N5Jky1br14PIN8L1H%2F2niA%3D%3D"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
</elements>
<signals>
<signal name="3.3V">
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="S2" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="S2" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="S2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
