<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="55.88" y1="59.69" x2="91.44" y2="59.69" width="0.1524" layer="20"/>
<wire x1="91.44" y1="59.69" x2="91.44" y2="29.21" width="0.1524" layer="20"/>
<wire x1="91.44" y1="29.21" x2="55.88" y2="29.21" width="0.1524" layer="20"/>
<wire x1="55.88" y1="29.21" x2="55.88" y2="59.69" width="0.1524" layer="20"/>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>1uf</text>
<text>100uf</text>
<text>10k</text>
<text>4.7k</text>
<text>1M</text>
<text>9014</text>
<text>9014</text>
<text>mic</text>
<text>Audio Act. Leds</text>
<text>CMX Solutions</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Transistor">
<description>BJT | JFET | MOSFET | UJT | Darlington</description>
<packages>
<package name="TO92">
<description>TO-92</description>
</package>
</packages>
</library>
<library name="Rembrandt Electronics - JST XH Connectors v1-0">
<packages>
<package name="JST-XH-02-PACKAGE-LONG-PAD">
<description>&lt;b&gt;JST XH Connector Long Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;2&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICROPHONE-PTH-9.7MM">
<description>&lt;h3&gt;Microphone - 9.7 mm Diameter, PTH&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Sensors/Sound/CEM-C9745JAD462P2.54R.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 2&lt;/li&gt;
&lt;li&gt;Diameter: 9.7 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;MIC&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="Tinkercad">
<packages>
<package name="CAPPRD254W65D500H1150B">
<description>Radial Polarized Capacitor, 2.54 mm pitch, 5.00 mm body diameter, 11.50 mm body height
 &lt;p&gt;Radial Polarized Capacitor package with 2.54 mm pitch (lead spacing), 0.65 mm lead diameter, 5.00 mm body diameter and 11.50 mm body height&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$2" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$3" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$4" library="Transistor" package="TO92" value="">
<attribute name="VALUE"/>
</element>
<element name="E$5" library="Transistor" package="TO92" value="">
<attribute name="VALUE"/>
</element>
<element name="E$6" library="Rembrandt Electronics - JST XH Connectors v1-0" package="JST-XH-02-PACKAGE-LONG-PAD" value="">
<attribute name="VALUE"/>
</element>
<element name="E$7" library="Rembrandt Electronics - JST XH Connectors v1-0" package="JST-XH-02-PACKAGE-LONG-PAD" value="">
<attribute name="VALUE"/>
</element>
<element name="MIC" library="SparkFun-Sensors" package="MICROPHONE-PTH-9.7MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$9" library="Tinkercad" package="CAPPRD254W65D500H1150B" value="">
<attribute name="VALUE"/>
</element>
<element name="E$10" library="Tinkercad" package="CAPPRD254W65D500H1150B" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$2">
<contactref element="E$3" pad="P$2"/>
<contactref element="E$9" pad="1"/>
<contactref element="E$1" pad="P$2"/>
<contactref element="E$6" pad="2"/>
<contactref element="E$7" pad="1"/>
<contactref element="E$2" pad="P$2"/>
</signal>
<signal name="S$6">
<contactref element="E$7" pad="2"/>
</signal>
<signal name="S$5">
<contactref element="E$10" pad="2"/>
<contactref element="E$5" pad="3"/>
</signal>
<signal name="S$8">
<contactref element="E$5" pad="1"/>
<contactref element="E$4" pad="1"/>
<contactref element="E$9" pad="2"/>
<contactref element="E$6" pad="1"/>
</signal>
<signal name="S$4">
<contactref element="E$1" pad="P$1"/>
<contactref element="E$10" pad="1"/>
<contactref element="E$2" pad="P$1"/>
</signal>
<signal name="S$1">
<contactref element="E$3" pad="P$1"/>
<contactref element="E$4" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
