<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="-2.54" y1="38.1" x2="-2.54" y2="-1.27" width="0.4064" layer="20"/>
<wire x1="-2.54" y1="-1.27" x2="20.32" y2="-1.27" width="0.4064" layer="20"/>
<wire x1="20.32" y1="-1.27" x2="20.32" y2="38.1" width="0.4064" layer="20"/>
<wire x1="20.32" y1="38.1" x2="-2.54" y2="38.1" width="0.4064" layer="20"/>
<text>WIFI AUX BOARD
</text>
<text>REV 1.0 |  BE</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216-KIT">
<description>&lt;h3&gt;EIA3216-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="esp8266modules">
<packages>
<package name="ESP-12-E">
<description>ESP8266 Module ESP-12-E</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BOARD_CONNECTOR" library="SparkFun-Connectors" package="AVR_ICSP" value="M05X2PTH"/>
<element name="C1" library="SparkFun-Passives" package="EIA3216-KIT" value="100uF"/>
<element name="C2" library="SparkFun-Passives" package="EIA3216-KIT" value="22uF"/>
<element name="FLASH" library="SparkFun-Electromechanical" package="TACTILE-PTH" value=""/>
<element name="IC1" library="SparkFun-PowerIC" package="SOT223" value="AMS1117-3.3v"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="RESET" library="SparkFun-Electromechanical" package="TACTILE-PTH" value=""/>
<element name="U$1" library="esp8266modules" package="ESP-12-E" value="ESP-12-E">
<attribute name="DIMENSIONS" value="24.0 x 16.0 mm"/>
<attribute name="PITCH" value="0.078&quot; / 2 mm"/>
<attribute name="PINS" value="22"/>
</element>
<element name="CONNECTOR" library="SparkFun-Connectors" package="1X04_NO_SILK" value="GND|RX|TX|V">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="FLASH" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="RESET" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="FLASH" pad="1"/>
<contactref element="RESET" pad="1"/>
<contactref element="C1" pad="C"/>
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="C"/>
<contactref element="U$1" pad="GND"/>
<contactref element="R4" pad="2"/>
<contactref element="CONNECTOR" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="C2" pad="A"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="RESET"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="FLASH">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="GPIO0"/>
</signal>
<signal name="+5V">
<contactref element="C1" pad="A"/>
<contactref element="IC1" pad="3"/>
<contactref element="CONNECTOR" pad="4"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="TX"/>
<contactref element="CONNECTOR" pad="3"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="RX"/>
<contactref element="CONNECTOR" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="CH_PD"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="GPIO15"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
