<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0.0508" y1="24.12" x2="0" y2="24.0692" width="0" layer="20" curve="90"/>
<circle x="16.51" y="11.43" radius="14.480225" width="0.1524" layer="20"/>
<text>RUSS-BUTTON
         v1</text>
</plain>
<libraries>
<library name="bt_avr">
<description>&lt;b&gt;AVR Microcontrollers&lt;/b&gt;
&lt;p&gt;Created by Michael Shimniok &lt;a href="http://www.bot-thoughts.com/"&gt;www.bot-thoughts.com&lt;/a&gt;&lt;/b&gt;</description>
<packages>
<package name="SOIC14N">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
<package name="LED5MMRGB">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="BATHLD001">
<description>&lt;b&gt;BAT-HLD-001&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="bt_avr" package="SOIC14N" value="ATTINY441/841-SSU"/>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="JP1" library="pinhead" package="1X02" value=""/>
<element name="R1" library="SparkFun-Resistors" package="0603" value="100">
<attribute name="PROD_ID" value="RES-12438"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="100">
<attribute name="PROD_ID" value="RES-12438"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="100">
<attribute name="PROD_ID" value="RES-12438"/>
</element>
<element name="U$1" library="adafruit" package="LED5MMRGB" value="5MMRGBLED"/>
<element name="U1" library="SamacSys_Parts" package="BATHLD001" value="BAT-HLD-001">
<attribute name="DESCRIPTION" value="Coin Cell Battery Holders Linx CR2032 Battery Holder"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="MANUFACTURER_NAME" value="Linx Technologies"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="BAT-HLD-001"/>
<attribute name="MOUSER_PART_NUMBER" value="712-BAT-HLD-001"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=712-BAT-HLD-001"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="ISP1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="ISP1" pad="6"/>
<contactref element="IC1" pad="14"/>
<contactref element="U$1" pad="3"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="MISO2">
<contactref element="ISP1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="SCK2">
<contactref element="ISP1" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="RST2">
<contactref element="ISP1" pad="5"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="MOSI2">
<contactref element="ISP1" pad="4"/>
<contactref element="IC1" pad="7"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="RGB">
<contactref element="IC1" pad="6"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
