<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="-0.2794" y1="-0.0508" x2="11.3478" y2="-0.0254" width="0" layer="20"/>
<wire x1="11.3478" y1="-0.0254" x2="11.3478" y2="22.6246" width="0" layer="20"/>
<wire x1="11.3478" y1="22.6246" x2="-0.2794" y2="22.5992" width="0" layer="20"/>
<wire x1="-0.2794" y1="22.5992" x2="-0.2794" y2="-0.0508" width="0" layer="20"/>
<text>SDO</text>
<text>SDI</text>
<text>CSX</text>
<text>D/CX</text>
<text>SCL</text>
<text>RST</text>
<text>GND</text>
<text>VCC</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="ili9341">
<packages>
<package name="ILI9341-2.8">
<description>connector for ili9341 screens with SPI interface</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="5-2,5">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="ili9341" package="ILI9341-2.8" value="ILI9341-2.8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="XL" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5"/>
<element name="YU" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5"/>
<element name="XR" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5"/>
<element name="YD" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="P$9"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="P$10"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="P$3"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$4"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="P$5"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="P$6"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="P$7"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$18"/>
<contactref element="YD" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$17"/>
<contactref element="XR" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$16"/>
<contactref element="YU" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P$15"/>
<contactref element="XL" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$8"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="J1" pad="2"/>
<contactref element="U$1" pad="P$14"/>
<contactref element="U$1" pad="P$13"/>
<contactref element="U$1" pad="P$12"/>
<contactref element="U$1" pad="P$11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
