<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>GND</text>
<hole x="68.58" y="15.875" drill="0.6"/>
<hole x="35.56" y="15.875" drill="0.6"/>
<wire x1="20.32" y1="48.895" x2="83.82" y2="48.895" width="0.4064" layer="20"/>
<wire x1="20.32" y1="48.895" x2="20.32" y2="13.97" width="0.4064" layer="20"/>
<wire x1="20.32" y1="13.97" x2="83.82" y2="13.97" width="0.4064" layer="20"/>
<wire x1="83.82" y1="13.97" x2="83.82" y2="48.895" width="0.4064" layer="20"/>
<hole x="22.86" y="46.99" drill="0.6"/>
<hole x="81.28" y="46.99" drill="0.6"/>
<text>CLK</text>
<text>LCH</text>
<text>SER</text>
<text>VCC</text>
<text>WEYLAND-YUTANI</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>3</text>
<text>8</text>
<text>9</text>
<text>22k</text>
<text>22k</text>
<text>HVDC-IN</text>
<text>HVDC-O</text>
<text>HVDC-O</text>
<text>BUILDING BETTER WORLDS</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10_LOCK">
</package>
<package name="1X01">
</package>
<package name="1X05_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="IC1" library="74xx-eu" package="DIL16" value="74HC595N">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="74xx-us" package="DIL16" value="74141N">
<attribute name="VALUE"/>
</element>
<element name="IC3" library="74xx-us" package="DIL16" value="74141N">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X10_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X10_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X05_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC3" pad="12"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="16"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC3" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="15"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="4"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="5"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="6"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="7"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="1"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="2"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$11">
<contactref element="J2" pad="3"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="4"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="N$13">
<contactref element="J2" pad="5"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$14">
<contactref element="J2" pad="6"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="N$15">
<contactref element="J2" pad="7"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="N$16">
<contactref element="J2" pad="8"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$17">
<contactref element="J2" pad="9"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="J2" pad="10"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="J3" pad="1"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="N$20">
<contactref element="J3" pad="2"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="N$21">
<contactref element="J3" pad="3"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="N$22">
<contactref element="J3" pad="4"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="N$23">
<contactref element="J3" pad="5"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="N$24">
<contactref element="J3" pad="6"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="N$25">
<contactref element="J3" pad="7"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="N$26">
<contactref element="J3" pad="8"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="N$27">
<contactref element="J3" pad="9"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="J3" pad="10"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="J5" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$30">
<contactref element="J6" pad="1"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$33">
<contactref element="IC1" pad="14"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$34">
<contactref element="IC1" pad="11"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$35">
<contactref element="IC1" pad="12"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="VCC-ISO">
<contactref element="R1" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="J4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
