<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="26.3" y2="0" width="0" layer="20"/>
<wire x1="26.3" y1="0" x2="26.3" y2="15.4" width="0" layer="20"/>
<wire x1="26.3" y1="15.4" x2="0" y2="15.4" width="0" layer="20"/>
<wire x1="0" y1="15.4" x2="0" y2="0" width="0" layer="20"/>
<text>Aaron Sirken, Jessica McWilliams
radio_v1.0
2/26/16</text>
</plain>
<libraries>
<library name="SmartPrj">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="latch">
<packages>
<package name="1051330001">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="chipcon-ti-v2">
<description>&lt;B&gt;Chipcon / Texas-Instruments RF  Devices&lt;/b&gt;&lt;p&gt;
&lt;B&gt; The Devices for ISM 2,4GHz, and 300MHz ... 1000MHz &lt;/b&gt;&lt;p&gt;
&lt;B&gt; Revision 0.1&lt;/b&gt;&lt;p&gt;
http://www.ti.com&lt;p&gt;
&lt;author&gt;Created by  S.Hofmann  mc_sho@gmx.de&lt;/author&gt;</description>
<packages>
<package name="QFN50P600X600X100-41N">
<description>&lt;b&gt;QFN,0.50mm pitch,square;40 pin,6.00mm L X 6.00mm W X 1.00mm H body (w/thermal tab)&lt;/b&gt;&lt;p&gt;
&lt;i&gt;IPC7351A for VQFN40&lt;/i&gt;</description>
</package>
</packages>
</library>
<library name="Base">
<description>Generated from &lt;b&gt;Base.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="ABM12-32.000MHZ-B2X-T-----CRYSTAL">
</package>
<package name="JOANTENNA">
</package>
<package name="MICROBUILDER_BALUN0805">
</package>
</packages>
</library>
<library name="pel_hdr">
<packages>
<package name="PH005-1-2">
<description>Standard 0.05" (1.27mm) pitch pin header.</description>
</package>
<package name="PH005-1-5">
<description>Standard 0.05" (1.27mm) pitch pin header.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C31" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0402-RES" value="56K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="SparkFun-Capacitors" package="0402-CAP" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="SparkFun-Capacitors" package="0402-CAP" value="15pF"/>
<element name="U$4" library="Base" package="ABM12-32.000MHZ-B2X-T-----CRYSTAL" value="ABRACON-ABM12-32MHZ-CRYSTAL"/>
<element name="U$5" library="Base" package="JOANTENNA" value="JONTENNA"/>
<element name="B1" library="Base" package="MICROBUILDER_BALUN0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="chipcon-ti-v2" package="QFN50P600X600X100-41N" value="CC2531">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="SparkFun-Capacitors" package="0402-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="SparkFun-Capacitors" package="0402-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="SparkFun-Capacitors" package="0402-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="SparkFun-Capacitors" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="latch" package="1051330001" value=""/>
<element name="R11" library="SparkFun-Passives" package="0402-RES" value="27">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Passives" package="0402-RES" value="27">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SmartPrj" package="C0402" value="47pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SmartPrj" package="C0402" value="47pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC" library="pel_hdr" package="PH005-1-2" value="PH1X2-05"/>
<element name="SPI" library="pel_hdr" package="PH005-1-5" value="PH1X5-05"/>
<element name="PH1" library="pel_hdr" package="PH005-1-2" value="PH1X2-05"/>
<element name="PRG" library="pel_hdr" package="PH005-1-2" value="PH1X2-05"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C31" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="B1" pad="5"/>
<contactref element="B1" pad="2"/>
<contactref element="B1" pad="6"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="U$4" pad="P$4"/>
<contactref element="R1" pad="1"/>
<contactref element="U$6" pad="41"/>
<contactref element="U$6" pad="1"/>
<contactref element="C41" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="VCC" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U$6" pad="37"/>
<contactref element="SPI" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U$6" pad="38"/>
<contactref element="SPI" pad="4"/>
</signal>
<signal name="SPCK">
<contactref element="U$6" pad="5"/>
<contactref element="SPI" pad="3"/>
</signal>
<signal name="PWM3">
<contactref element="U$6" pad="20"/>
<contactref element="PH1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="C31" pad="1"/>
<contactref element="U$6" pad="40"/>
</signal>
<signal name="N$17">
<contactref element="R1" pad="2"/>
<contactref element="U$6" pad="30"/>
</signal>
<signal name="N$19">
<contactref element="C36" pad="1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$6" pad="22"/>
</signal>
<signal name="N$20">
<contactref element="C37" pad="1"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="U$6" pad="23"/>
</signal>
<signal name="N$10">
<contactref element="B1" pad="1"/>
<contactref element="U$5" pad="FEED"/>
</signal>
<signal name="N$13">
<contactref element="B1" pad="3"/>
<contactref element="U$6" pad="26"/>
</signal>
<signal name="N$14">
<contactref element="B1" pad="4"/>
<contactref element="U$6" pad="25"/>
</signal>
<signal name="DP">
<contactref element="U$6" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="DN">
<contactref element="U$6" pad="3"/>
<contactref element="C12" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="SS0">
<contactref element="U$6" pad="6"/>
<contactref element="SPI" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="C41" pad="1"/>
<contactref element="U$6" pad="29"/>
<contactref element="C39" pad="1"/>
<contactref element="U$6" pad="28"/>
<contactref element="U$6" pad="31"/>
<contactref element="U$6" pad="27"/>
<contactref element="U$6" pad="24"/>
<contactref element="U$6" pad="39"/>
<contactref element="C40" pad="1"/>
<contactref element="U$6" pad="10"/>
<contactref element="U$6" pad="21"/>
<contactref element="C38" pad="1"/>
<contactref element="VCC" pad="2"/>
</signal>
<signal name="DPP">
<contactref element="U3" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="DNN">
<contactref element="U3" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="VUSB">
<contactref element="U3" pad="1"/>
<contactref element="U$6" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$6" pad="34"/>
<contactref element="PRG" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$6" pad="35"/>
<contactref element="PRG" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
