<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.42" y2="0" width="0" layer="20"/>
<wire x1="31.42" y1="0" x2="31.42" y2="60.95" width="0" layer="20"/>
<wire x1="31.42" y1="60.95" x2="0" y2="60.95" width="0" layer="20"/>
<wire x1="0" y1="60.95" x2="0" y2="0" width="0" layer="20"/>
<hole x="7.62" y="2.54" drill="3.2"/>
<hole x="29.21" y="2.54" drill="3.2"/>
<hole x="29.21" y="58.42" drill="3.2"/>
<text>Flimshaw
Industries</text>
<text>24bit BCD Clock
HV passthrough</text>
<text>Charlie Hoey
1.19.2016</text>
<text>REV1</text>
<text>CLOCK</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,54/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,17/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="GeekAmmo">
<description>&lt;h3&gt;GeekAmmo  Library&lt;/h3&gt;

These are parts used by the GeekAmmo company (now part of SparkFun Electronics)!

 If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TAC-SWITCH-PTH">
</package>
</packages>
</library>
<library name="Custom-Parts-2">
<packages>
<package name="NIXIE_MODULE_CONNECTOR">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="22pf">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="22pf">
<attribute name="VALUE"/>
</element>
<element name="HOURS" library="74xx-eu" package="SO16" value="74HCT595D">
<attribute name="NAME"/>
</element>
<element name="HRS_G" library="wirepad" package="2,54/1,1" value="">
<attribute name="VALUE"/>
</element>
<element name="HRS_SCL" library="wirepad" package="2,54/1,1" value="">
<attribute name="VALUE"/>
</element>
<element name="HV-IN" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MINS_G" library="wirepad" package="2,54/1,1" value="">
<attribute name="VALUE"/>
</element>
<element name="MINS_SCL" library="wirepad" package="2,54/1,1" value="">
<attribute name="VALUE"/>
</element>
<element name="MINUTES" library="74xx-eu" package="SO16" value="74HCT595D">
<attribute name="NAME"/>
</element>
<element name="Q1" library="crystal" package="HC49U-V" value="4mhz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="1666969"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="10K"/>
<element name="SECONDS" library="74xx-eu" package="SO16" value="74HCT595D">
<attribute name="NAME"/>
</element>
<element name="SECS_G" library="wirepad" package="2,54/1,1" value="">
<attribute name="VALUE"/>
</element>
<element name="SECS_SCL" library="wirepad" package="2,54/1,1" value="">
<attribute name="VALUE"/>
</element>
<element name="SET" library="GeekAmmo" package="TAC-SWITCH-PTH" value="TACTILE-SWITCH-PTH">
<attribute name="NAME"/>
</element>
<element name="U$1" library="Custom-Parts-2" package="NIXIE_MODULE_CONNECTOR" value="NIXIE_MODULE"/>
<element name="U$2" library="Custom-Parts-2" package="NIXIE_MODULE_CONNECTOR" value="NIXIE_MODULE"/>
<element name="U$3" library="Custom-Parts-2" package="NIXIE_MODULE_CONNECTOR" value="NIXIE_MODULE"/>
<element name="U$4" library="Custom-Parts-2" package="NIXIE_MODULE_CONNECTOR" value="NIXIE_MODULE"/>
<element name="U$5" library="Custom-Parts-2" package="NIXIE_MODULE_CONNECTOR" value="NIXIE_MODULE"/>
<element name="U$6" library="Custom-Parts-2" package="NIXIE_MODULE_CONNECTOR" value="NIXIE_MODULE"/>
<element name="U1" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="IC1" library="linear" package="TO220V" value="786TV"/>
<element name="C3" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="10uf"/>
<element name="C4" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="10uf"/>
<element name="V+" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V-" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
</elements>
<signals>
<signal name="GND">
<contactref element="SECONDS" pad="8"/>
<contactref element="MINUTES" pad="8"/>
<contactref element="HOURS" pad="8"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="GND"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$4" pad="GND"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$6" pad="GND"/>
<contactref element="U$5" pad="GND"/>
<contactref element="IC1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="V-" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="SECONDS" pad="16"/>
<contactref element="MINUTES" pad="16"/>
<contactref element="HOURS" pad="16"/>
<contactref element="U1" pad="8"/>
<contactref element="SET" pad="3"/>
<contactref element="U$1" pad="5V"/>
<contactref element="U$2" pad="5V"/>
<contactref element="U$3" pad="5V"/>
<contactref element="U$4" pad="5V"/>
<contactref element="U$5" pad="5V"/>
<contactref element="U$6" pad="5V"/>
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="3"/>
<contactref element="Q1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="SECONDS" pad="9"/>
<contactref element="MINUTES" pad="14"/>
</signal>
<signal name="N$4">
<contactref element="MINUTES" pad="9"/>
<contactref element="HOURS" pad="14"/>
</signal>
<signal name="N$5">
<contactref element="SECONDS" pad="12"/>
<contactref element="MINUTES" pad="12"/>
<contactref element="HOURS" pad="12"/>
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="SECONDS" pad="11"/>
<contactref element="MINUTES" pad="11"/>
<contactref element="HOURS" pad="11"/>
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="SECONDS" pad="14"/>
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="SECONDS" pad="15"/>
<contactref element="U$1" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="SECONDS" pad="1"/>
<contactref element="U$1" pad="B"/>
</signal>
<signal name="N$11">
<contactref element="SECONDS" pad="2"/>
<contactref element="U$1" pad="C"/>
</signal>
<signal name="N$12">
<contactref element="SECONDS" pad="3"/>
<contactref element="U$1" pad="D"/>
</signal>
<signal name="N$13">
<contactref element="SECONDS" pad="4"/>
<contactref element="U$2" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="SECONDS" pad="5"/>
<contactref element="U$2" pad="B"/>
</signal>
<signal name="N$15">
<contactref element="SECONDS" pad="6"/>
<contactref element="U$2" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="SECONDS" pad="7"/>
<contactref element="U$2" pad="D"/>
</signal>
<signal name="N$17">
<contactref element="U$3" pad="A"/>
<contactref element="MINUTES" pad="15"/>
</signal>
<signal name="N$18">
<contactref element="MINUTES" pad="1"/>
<contactref element="U$3" pad="B"/>
</signal>
<signal name="N$19">
<contactref element="MINUTES" pad="2"/>
<contactref element="U$3" pad="C"/>
</signal>
<signal name="N$20">
<contactref element="MINUTES" pad="3"/>
<contactref element="U$3" pad="D"/>
</signal>
<signal name="N$21">
<contactref element="MINUTES" pad="4"/>
<contactref element="U$4" pad="A"/>
</signal>
<signal name="N$22">
<contactref element="MINUTES" pad="5"/>
<contactref element="U$4" pad="B"/>
</signal>
<signal name="N$23">
<contactref element="MINUTES" pad="6"/>
<contactref element="U$4" pad="C"/>
</signal>
<signal name="N$24">
<contactref element="MINUTES" pad="7"/>
<contactref element="U$4" pad="D"/>
</signal>
<signal name="N$25">
<contactref element="HOURS" pad="15"/>
<contactref element="U$5" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="U$5" pad="B"/>
<contactref element="HOURS" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="HOURS" pad="2"/>
<contactref element="U$5" pad="C"/>
</signal>
<signal name="N$28">
<contactref element="U$5" pad="D"/>
<contactref element="HOURS" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="HOURS" pad="4"/>
<contactref element="U$6" pad="A"/>
</signal>
<signal name="N$30">
<contactref element="HOURS" pad="5"/>
<contactref element="U$6" pad="B"/>
</signal>
<signal name="N$31">
<contactref element="HOURS" pad="6"/>
<contactref element="U$6" pad="C"/>
</signal>
<signal name="N$32">
<contactref element="HOURS" pad="7"/>
<contactref element="U$6" pad="D"/>
</signal>
<signal name="HV">
<contactref element="U$1" pad="HV"/>
<contactref element="U$2" pad="HV"/>
<contactref element="U$3" pad="HV"/>
<contactref element="U$4" pad="HV"/>
<contactref element="HV-IN" pad="1"/>
<contactref element="U$5" pad="HV"/>
<contactref element="U$6" pad="HV"/>
</signal>
<signal name="N$33">
<contactref element="HRS_SCL" pad="1"/>
<contactref element="HOURS" pad="10"/>
</signal>
<signal name="N$34">
<contactref element="HRS_G" pad="1"/>
<contactref element="HOURS" pad="13"/>
</signal>
<signal name="N$35">
<contactref element="MINS_SCL" pad="1"/>
<contactref element="MINUTES" pad="10"/>
</signal>
<signal name="N$36">
<contactref element="MINS_G" pad="1"/>
<contactref element="MINUTES" pad="13"/>
</signal>
<signal name="N$37">
<contactref element="SECS_G" pad="1"/>
<contactref element="SECONDS" pad="13"/>
</signal>
<signal name="N$38">
<contactref element="SECS_SCL" pad="1"/>
<contactref element="SECONDS" pad="10"/>
</signal>
<signal name="N$39">
<contactref element="V+" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="J1" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="SET" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
