<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="28.067" y1="17.78" x2="28.067" y2="45.72" width="0" layer="20"/>
<wire x1="28.067" y1="45.72" x2="0" y2="45.72" width="0" layer="20"/>
<wire x1="0" y1="45.72" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="17.907" y2="0" width="0" layer="20"/>
<wire x1="17.907" y1="0" x2="17.907" y2="17.78" width="0" layer="20"/>
<wire x1="17.907" y1="17.78" x2="28.067" y2="17.78" width="0" layer="20"/>
<hole x="2.54" y="3.81" drill="3.048"/>
<hole x="2.54" y="41.91" drill="3.048"/>
<text>RV-Project.Com</text>
<text>Display Board</text>
<text>Water Alarm</text>
<text>Rev C    
5/24/2018</text>
<text>GND</text>
<text>9V</text>
<text>Reset</text>
<text>CH1A</text>
<text>CH1B</text>
<text>CH2A</text>
<text>CH2B</text>
<text>CH3A</text>
<text>CH3B</text>
<text>Alarm</text>
<text>5V</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="1X01_HEADER">
</package>
<package name="BI-LEDCOMMONANODE">
</package>
<package name="1206-RES">
</package>
<package name="TACTILE-PTH-EZ">
</package>
<package name="ART_CHEROKEE_MEDIUM">
</package>
<package name="BUZZER_SMALL">
</package>
<package name="SOT23-3">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP3" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="a-lib" package="BI-LEDCOMMONANODE" value="LED_BI-COLOR_CA"/>
<element name="LED2" library="a-lib" package="BI-LEDCOMMONANODE" value="LED_BI-COLOR_CA"/>
<element name="LED3" library="a-lib" package="BI-LEDCOMMONANODE" value="LED_BI-COLOR_CA"/>
<element name="Q1" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="VALUE" value="MMBT2222A"/>
</element>
<element name="R8" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R10" library="a-lib" package="1206-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R12" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R14" library="a-lib" package="1206-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R6" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="a-lib" package="TACTILE-PTH-EZ" value="SWITCH-MOMENTARY-2PTH_EZ"/>
<element name="U$1" library="a-lib" package="ART_CHEROKEE_MEDIUM" value=""/>
<element name="JP11" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="BZ1" library="a-lib" package="BUZZER_SMALL" value="BUZZERMALLORY_PT1140PEQ">
<attribute name="VOLTAGE" value="9-20V"/>
</element>
<element name="Q2" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q3" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q4" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q5" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q6" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q7" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="a-lib" package="SOD-323" value="3.3V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-11284"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R4" pad="2"/>
<contactref element="LED1" pad="C1"/>
</signal>
<signal name="N$2">
<contactref element="R6" pad="2"/>
<contactref element="LED1" pad="C2"/>
</signal>
<signal name="N$3">
<contactref element="R8" pad="2"/>
<contactref element="LED2" pad="C1"/>
</signal>
<signal name="N$4">
<contactref element="R10" pad="2"/>
<contactref element="LED2" pad="C2"/>
</signal>
<signal name="N$5">
<contactref element="R12" pad="2"/>
<contactref element="LED3" pad="C1"/>
</signal>
<signal name="N$6">
<contactref element="R14" pad="2"/>
<contactref element="LED3" pad="C2"/>
</signal>
<signal name="9V">
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="JP9" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$14">
<contactref element="R2" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="JP10" pad="1"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q6" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="Q1" pad="3"/>
<contactref element="BZ1" pad="-"/>
</signal>
<signal name="N$13">
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="R2" pad="2"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R8" pad="1"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R10" pad="1"/>
<contactref element="Q5" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="R12" pad="1"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R14" pad="1"/>
<contactref element="Q7" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="Q2" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="Q3" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="Q4" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="Q5" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="Q6" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="Q7" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="R13" pad="1"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R11" pad="1"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R9" pad="1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R7" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R5" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R3" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="BZ1" pad="+"/>
<contactref element="D1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
