<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="58.42" y2="0" width="0" layer="20"/>
<wire x1="58.42" y1="0" x2="58.42" y2="58.42" width="0" layer="20"/>
<wire x1="58.42" y1="58.42" x2="0" y2="58.42" width="0" layer="20"/>
<wire x1="0" y1="58.42" x2="0" y2="0" width="0" layer="20"/>
<text>set my sensor to
catch digital butterflies
a tsunami rings</text>
<text>www.netChimes.org</text>
<text>netChimes Sensor ver. C jeg2015</text>
<text>Place outdoor on a level surface.
Power via USB wall (mains) adapter.
Keep surface free of debris.</text>
<text>CHIME 1</text>
<text>CHIME 2</text>
<text>CHIME 3</text>
<text>CHIME 6</text>
<text>CHIME 5</text>
<text>CHIME 4</text>
</plain>
<libraries>
<library name="HALL_EFFECT_BM">
<packages>
<package name="AH180-PG-A">
</package>
</packages>
</library>
<library name="Particle_Photon">
<packages>
<package name="SPARK_PHOTON">
<description>This is a footprint for plugging the Particle Photon IoT
board into your projects using a few female headers. Have
fun!!!</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CHIME1" library="HALL_EFFECT_BM" package="AH180-PG-A" value="AH180-PG-A"/>
<element name="CHIME2" library="HALL_EFFECT_BM" package="AH180-PG-A" value="AH180-PG-A"/>
<element name="CHIME3" library="HALL_EFFECT_BM" package="AH180-PG-A" value="AH180-PG-A"/>
<element name="CHIME4" library="HALL_EFFECT_BM" package="AH180-PG-A" value="AH180-PG-A"/>
<element name="CHIME5" library="HALL_EFFECT_BM" package="AH180-PG-A" value="AH180-PG-A"/>
<element name="CHIME6" library="HALL_EFFECT_BM" package="AH180-PG-A" value="AH180-PG-A"/>
<element name="U$1" library="Particle_Photon" package="SPARK_PHOTON" value="PARTICLE_PHOTON"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="D0"/>
<contactref element="CHIME1" pad="PIN"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="D1"/>
<contactref element="CHIME2" pad="PIN"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="D2"/>
<contactref element="CHIME3" pad="PIN"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="D4"/>
<contactref element="CHIME5" pad="PIN"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="3.3V"/>
<contactref element="CHIME6" pad="VIN"/>
<contactref element="CHIME5" pad="VIN"/>
<contactref element="CHIME4" pad="VIN"/>
<contactref element="CHIME3" pad="VIN"/>
<contactref element="CHIME2" pad="VIN"/>
<contactref element="CHIME1" pad="VIN"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="CHIME1" pad="GND"/>
<contactref element="CHIME5" pad="GND"/>
<contactref element="CHIME6" pad="GND"/>
<contactref element="CHIME3" pad="GND"/>
<contactref element="CHIME2" pad="GND"/>
<contactref element="CHIME4" pad="GND"/>
<contactref element="U$1" pad="GND*"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="D3"/>
<contactref element="CHIME4" pad="PIN"/>
</signal>
<signal name="N$13">
<contactref element="CHIME6" pad="PIN"/>
<contactref element="U$1" pad="D5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
