<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="99" width="0" layer="20"/>
<wire x1="160" y1="99" x2="0" y2="99" width="0" layer="20"/>
<wire x1="0" y1="99" x2="0" y2="0" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>EARTH</text>
<text>ACOPIAN EL-10, 13, 20 LINEAR POWER SUPPLY </text>
<text>M8-3 
RECEPTACLE</text>
<text>SCHURTER DD22</text>
<text>HAMMOND 1455N1601  ENCLOSURE</text>
<text>20190716</text>
<text>J007874A LINEAR POWER SUPPLY </text>
<text>S</text>
<text>S</text>
<text>-</text>
<text>+</text>
</plain>
<libraries>
<library name="STEVES_BU">
<packages>
<package name="ACOPIAN_ES-10">
</package>
<package name="DD22">
<description>Power Entry Module PCB</description>
</package>
<package name="M8-3_RA">
<description>3 Position Circular Connector Receptacle, Female Sockets Solder Gold 
Phoenix M8-3 1456145</description>
</package>
<package name="LOGO_BMP_OP">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PS1" library="STEVES_BU" package="ACOPIAN_ES-10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PE1" library="STEVES_BU" package="DD22" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="STEVES_BU" package="M8-3_RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="STEVES_BU" package="LOGO_BMP_OP" value="JFRC-LOGOLOGO_OP"/>
<element name="J2" library="STEVES_BU" package="M8-3_RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="PS1" pad="AC2"/>
<contactref element="PE1" pad="N"/>
</signal>
<signal name="N$2">
<contactref element="PS1" pad="AC1"/>
<contactref element="PE1" pad="L"/>
</signal>
<signal name="N$3">
<contactref element="PE1" pad="PE"/>
<contactref element="JP1" pad="2"/>
<contactref element="J1" pad="P1"/>
<contactref element="J1" pad="P2"/>
<contactref element="J2" pad="P2"/>
<contactref element="J2" pad="P1"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="4"/>
<contactref element="PS1" pad="TRIM"/>
<contactref element="JP1" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="PS1" pad="-"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="3"/>
<contactref element="PS1" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
