<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0.254" layer="20"/>
<wire x1="0" y1="1.27" x2="0" y2="26.67" width="0.254" layer="20"/>
<wire x1="0" y1="26.67" x2="1.27" y2="27.94" width="0.254" layer="20"/>
<wire x1="1.27" y1="27.94" x2="21.59" y2="27.94" width="0.254" layer="20"/>
<wire x1="21.59" y1="27.94" x2="22.86" y2="26.67" width="0.254" layer="20"/>
<wire x1="22.86" y1="26.67" x2="22.86" y2="19.05" width="0.254" layer="20"/>
<wire x1="22.86" y1="19.05" x2="24.003" y2="17.907" width="0.254" layer="20"/>
<wire x1="46.863" y1="8.001" x2="41.91" y2="8.001" width="0.254" layer="20"/>
<wire x1="41.91" y1="8.001" x2="40.894" y2="6.985" width="0.254" layer="20"/>
<wire x1="40.894" y1="6.985" x2="40.132" y2="6.985" width="0.254" layer="20"/>
<wire x1="40.132" y1="6.985" x2="39.624" y2="7.493" width="0.254" layer="20"/>
<wire x1="39.624" y1="7.493" x2="37.846" y2="7.493" width="0.254" layer="20"/>
<wire x1="37.846" y1="7.493" x2="37.338" y2="6.985" width="0.254" layer="20"/>
<wire x1="46.99" y1="17.907" x2="46.863" y2="8.001" width="0.254" layer="20"/>
<wire x1="46.99" y1="17.907" x2="24.003" y2="17.907" width="0.254" layer="20"/>
<wire x1="37.211" y1="6.985" x2="23.876" y2="6.985" width="0.254" layer="20"/>
<wire x1="1.27" y1="0" x2="21.59" y2="0" width="0.254" layer="20"/>
<wire x1="21.59" y1="0" x2="22.86" y2="1.27" width="0.254" layer="20"/>
<wire x1="22.86" y1="1.27" x2="22.86" y2="5.969" width="0.254" layer="20"/>
<wire x1="22.86" y1="5.969" x2="23.876" y2="6.985" width="0.254" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>CMD</text>
<text>CD</text>
<text>DAT2</text>
<text>CLK</text>
<text>DAT0</text>
<text>DAT1</text>
<text>V10</text>
<text>Revised by: Patrick Alberts</text>
<text>PCB must be no thicker than 0.75mm</text>
<text>Tim Holmberg </text>
<text>microSD Sniffer </text>
<text>DAT2</text>
<text>CD</text>
<text>CMD</text>
<text>GND</text>
<text>VCC</text>
<text>CLK</text>
<text>DAT0</text>
<text>DAT1</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X08">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
<package name="OSHW-LOGO-M">
</package>
<package name="SFE_LOGO_FLAME_.2">
</package>
<package name="SFE_LOGO_NAME_FLAME_.1">
</package>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICRO-SDCARD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICROSD_1:1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X08" value=""/>
<element name="U2" library="SparkFun-Connectors" package="MICROSD_1:1" value="microSD Socket">
<attribute name="PROD_ID" value="CONN-07820"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="">
<attribute name="VERSION" value="v01"/>
<attribute name="DESIGNER" value="NAME"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="SFE_LOGO_FLAME_.2" value="SFE_LOGO_FLAME.2_INCH"/>
<element name="LOGO3" library="SparkFun-Aesthetics" package="SFE_LOGO_NAME_FLAME_.1" value="SFE_LOGO_NAME_FLAME.1_INCH"/>
<element name="U1" library="SparkFun-Boards" package="MICRO-SDCARD" value="MICRO-SDCARD"/>
<element name="FID1" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FID2" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="GND1"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="CD1"/>
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="GND"/>
<contactref element="U2" pad="GND3"/>
<contactref element="U2" pad="CD2"/>
</signal>
<signal name="VCC">
<contactref element="U2" pad="4"/>
<contactref element="JP1" pad="5"/>
<contactref element="U1" pad="VCC"/>
</signal>
<signal name="DAT1">
<contactref element="U2" pad="8"/>
<contactref element="JP1" pad="8"/>
<contactref element="U1" pad="DAT1"/>
</signal>
<signal name="DAT0">
<contactref element="JP1" pad="7"/>
<contactref element="U2" pad="7"/>
<contactref element="U1" pad="DAT0"/>
</signal>
<signal name="CLK">
<contactref element="U2" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="U1" pad="CLK"/>
</signal>
<signal name="CMD">
<contactref element="U2" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="CMD"/>
</signal>
<signal name="CD/DAT3">
<contactref element="U2" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="CD/DAT3"/>
</signal>
<signal name="DAT2">
<contactref element="U2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="DAT2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
