<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="35.56" width="0.1524" layer="20"/>
<wire x1="0" y1="35.56" x2="53.34" y2="35.56" width="0.1524" layer="20"/>
<wire x1="53.34" y1="35.56" x2="53.34" y2="-0.15875" width="0.1524" layer="20"/>
<wire x1="53.34" y1="-0.15875" x2="0" y2="0" width="0.1524" layer="20"/>
<text>PB12</text>
<text>GND</text>
<text>PB13</text>
<text>PB14</text>
<text>PB15</text>
<text>PA8</text>
<text>PA9</text>
<text>PA10</text>
<text>PA11</text>
<text>PA12</text>
<text>GND</text>
<text>PA15</text>
<text>PB3</text>
<text>PB4</text>
<text>PB5</text>
<text>PB6</text>
<text>PB7</text>
<text>PB8</text>
<text>PB9</text>
<text>5V0</text>
<text>3V3</text>
<text>GND</text>
<text>3V3</text>
<text>RST</text>
<text>PB11</text>
<text>PB10</text>
<text>PB1</text>
<text>PB0</text>
<text>PA7</text>
<text>PA6</text>
<text>PA5</text>
<text>PA4</text>
<text>PA3</text>
<text>PA2</text>
<text>PA1</text>
<text>PA0</text>
<text>PC15</text>
<text>PC14</text>
<text>PC13</text>
<text>VBAT</text>
<text>BluePill Breakout Board</text>
<text>(c) 2019 Harry H. Arends
BLUE-PILL Breakout V0.1</text>
</plain>
<libraries>
<library name="BluePill">
<packages>
<package name="BLUE_PILL_MIN">
</package>
</packages>
</library>
<library name="con-phoenix-254">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 2.54 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="10POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="kunstmanen">
<description>Components used in Werkgroep Kunstmanen designs</description>
<packages>
<package name="LOGO_KM_BIG">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="BluePill" package="BLUE_PILL_MIN" value=""/>
<element name="X1" library="con-phoenix-254" package="10POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-phoenix-254" package="10POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="con-phoenix-254" package="10POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="con-phoenix-254" package="10POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="kunstmanen" package="LOGO_KM_BIG" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$21"/>
<contactref element="X2" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$40"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$39"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$38"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$37"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$36"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P$35"/>
<contactref element="X1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$34"/>
<contactref element="X1" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$33"/>
<contactref element="X1" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="P$32"/>
<contactref element="X1" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$31"/>
<contactref element="X1" pad="10"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="P$30"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="P$29"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="P$28"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="P$27"/>
<contactref element="X2" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="P$26"/>
<contactref element="X2" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="P$22"/>
<contactref element="X2" pad="9"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="P$23"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="P$24"/>
<contactref element="X2" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="P$25"/>
<contactref element="X2" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="P$20"/>
<contactref element="X4" pad="1"/>
</signal>
<signal name="PB12">
<contactref element="U$1" pad="P$1"/>
<contactref element="X3" pad="10"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="P$19"/>
<contactref element="X4" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="P$18"/>
<contactref element="X4" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="P$17"/>
<contactref element="X4" pad="4"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="P$16"/>
<contactref element="X4" pad="5"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="P$15"/>
<contactref element="X4" pad="6"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="P$14"/>
<contactref element="X4" pad="7"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="P$13"/>
<contactref element="X4" pad="8"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="P$12"/>
<contactref element="X4" pad="9"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="P$11"/>
<contactref element="X4" pad="10"/>
</signal>
<signal name="N$32">
<contactref element="U$1" pad="P$10"/>
<contactref element="X3" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="U$1" pad="P$9"/>
<contactref element="X3" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="P$8"/>
<contactref element="X3" pad="3"/>
</signal>
<signal name="N$35">
<contactref element="U$1" pad="P$7"/>
<contactref element="X3" pad="4"/>
</signal>
<signal name="N$36">
<contactref element="U$1" pad="P$6"/>
<contactref element="X3" pad="5"/>
</signal>
<signal name="N$37">
<contactref element="U$1" pad="P$5"/>
<contactref element="X3" pad="6"/>
</signal>
<signal name="PB15">
<contactref element="U$1" pad="P$4"/>
<contactref element="X3" pad="7"/>
</signal>
<signal name="PB14">
<contactref element="U$1" pad="P$3"/>
<contactref element="X3" pad="8"/>
</signal>
<signal name="PB13">
<contactref element="U$1" pad="P$2"/>
<contactref element="X3" pad="9"/>
</signal>
<signal name="GND">
</signal>
</signals>
</board>
</drawing>
</eagle>
