<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="39.7512" y2="0" width="0" layer="20"/>
<wire x1="39.7512" y1="0" x2="39.7512" y2="46.5736" width="0" layer="20"/>
<wire x1="39.7512" y1="46.5736" x2="0" y2="46.5736" width="0" layer="20"/>
<wire x1="0" y1="46.5736" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.3368" y="44.0436" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<hole x="37.1348" y="2.54" drill="3.2"/>
<hole x="37.1348" y="43.8404" drill="3.2"/>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>3.3V</text>
</plain>
<libraries>
<library name="yc">
<packages>
<package name="SDP600">
</package>
</packages>
</library>
<library name="Teensy_3_Series_Board_v1.0">
<packages>
<package name="TEENSY_3.1_BASIC">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="yc" package="SDP600" value="SDP600"/>
<element name="U$2" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1_BASIC" value="TEENSY_3.1_BASIC">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value=""/>
</elements>
<signals>
<signal name="AGND">
<contactref element="U$2" pad="AGND"/>
</signal>
<signal name="VBAT">
<contactref element="U$2" pad="VBAT"/>
</signal>
<signal name="VIN">
<contactref element="U$2" pad="VIN"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$2" pad="19/A5"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="P$4"/>
<contactref element="U$2" pad="18/A4"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$2" pad="3.3V"/>
<contactref element="U$2" pad="3.3V1"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$3"/>
<contactref element="U$2" pad="GND1"/>
<contactref element="U$2" pad="GND"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
