<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="10.795" y1="17.8308" x2="12.279778125" y2="17.8308" width="0" layer="20"/>
<wire x1="12.279778125" y1="17.8308" x2="12.476815625" y2="17.749184375" width="0" layer="20" curve="-45"/>
<wire x1="12.476815625" y1="17.749184375" x2="13.01563125" y2="17.526" width="0" layer="20" curve="45"/>
<wire x1="13.01563125" y1="17.526" x2="27.432" y2="17.526" width="0" layer="20"/>
<wire x1="27.432" y1="17.526" x2="28.194" y2="16.764" width="0" layer="20" curve="-90"/>
<wire x1="28.194" y1="16.764" x2="28.194" y2="8.636" width="0" layer="20"/>
<wire x1="28.194" y1="8.636" x2="27.432" y2="7.874" width="0" layer="20" curve="-90"/>
<wire x1="27.432" y1="7.874" x2="13.01563125" y2="7.874" width="0" layer="20"/>
<wire x1="13.01563125" y1="7.874" x2="12.476815625" y2="7.650815625" width="0" layer="20" curve="45"/>
<wire x1="12.476815625" y1="7.650815625" x2="12.279778125" y2="7.5692" width="0" layer="20" curve="-45"/>
<wire x1="12.279778125" y1="7.5692" x2="10.795" y2="7.5692" width="0" layer="20"/>
<wire x1="10.795" y1="7.5692" x2="10.033" y2="8.3312" width="0" layer="20" curve="-90"/>
<wire x1="10.033" y1="8.3312" x2="10.033" y2="17.0688" width="0" layer="20"/>
<wire x1="10.033" y1="17.0688" x2="10.795" y2="17.8308" width="0" layer="20" curve="-90"/>
<text>10k</text>
<text>4.7k</text>
<text>4.7k</text>
<text>0.1uF</text>
<text>2.2uF</text>
<text>G</text>
<text>3V</text>
<text>SD</text>
<text>SC</text>
</plain>
<libraries>
<library name="BRETTAN">
<packages>
<package name="QDSP-6064-SLIM">
</package>
<package name="0402_RES">
</package>
<package name="0402_CAP">
</package>
<package name="FALKLOGOSMALL">
</package>
<package name="QFN-24">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$6" library="BRETTAN" package="QDSP-6064-SLIM" value="QDSP-6064"/>
<element name="U$1" library="BRETTAN" package="0402_CAP" value="2.2uF"/>
<element name="RSET" library="BRETTAN" package="0402_RES" value="10k"/>
<element name="C1" library="BRETTAN" package="0402_CAP" value="0.1uF"/>
<element name="PU1" library="BRETTAN" package="0402_RES" value="4.7k"/>
<element name="PU2" library="BRETTAN" package="0402_RES" value="4.7k"/>
<element name="U$2" library="BRETTAN" package="FALKLOGOSMALL" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="BRETTAN" package="QFN-24" value="AS1117QFN24"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$3" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="C1">
<contactref element="U$6" pad="1"/>
<contactref element="U$3" pad="23"/>
</signal>
<signal name="C2">
<contactref element="U$6" pad="10"/>
<contactref element="U$3" pad="24"/>
</signal>
<signal name="C3">
<contactref element="U$6" pad="4"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="C4">
<contactref element="U$6" pad="6"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="SEGA">
<contactref element="U$6" pad="12"/>
<contactref element="U$3" pad="12"/>
</signal>
<signal name="SEGC">
<contactref element="U$6" pad="3"/>
<contactref element="U$3" pad="17"/>
</signal>
<signal name="SEGE">
<contactref element="U$6" pad="2"/>
<contactref element="U$3" pad="18"/>
</signal>
<signal name="SEGG">
<contactref element="U$6" pad="7"/>
<contactref element="U$3" pad="15"/>
</signal>
<signal name="SEGDP">
<contactref element="U$6" pad="5"/>
<contactref element="U$3" pad="19"/>
</signal>
<signal name="SEGB">
<contactref element="U$6" pad="11"/>
<contactref element="U$3" pad="14"/>
</signal>
<signal name="SEGD">
<contactref element="U$6" pad="8"/>
<contactref element="U$3" pad="20"/>
</signal>
<signal name="SEGF">
<contactref element="U$6" pad="9"/>
<contactref element="U$3" pad="13"/>
</signal>
<signal name="SDA">
<contactref element="PU2" pad="2"/>
<contactref element="U$3" pad="22"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="PU1" pad="2"/>
<contactref element="U$3" pad="11"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="PU1" pad="1"/>
<contactref element="PU2" pad="1"/>
<contactref element="U$3" pad="16"/>
<contactref element="RSET" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="ISET">
<contactref element="RSET" pad="2"/>
<contactref element="U$3" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
