<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="40.64" width="0.2032" layer="20"/>
<wire x1="0" y1="40.64" x2="40.64" y2="40.64" width="0.2032" layer="20"/>
<wire x1="40.64" y1="40.64" x2="40.64" y2="0" width="0.2032" layer="20"/>
<wire x1="40.64" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>Load-</text>
<text>Load+</text>
<text>BLEON</text>
<text>JUICE</text>
<text>BT STATUS</text>
<text>GND</text>
<text>VCC</text>
<text>mjl</text>
<text>2017</text>
<text>GND</text>
<text>VCC</text>
<text>ID</text>
<text>D+</text>
<text>D-</text>
<text>B</text>
<text>C</text>
<text>E</text>
<text>HI</text>
<text>LO</text>
<text>150Ω</text>
<text>150Ω</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_3MM">
<description>&lt;h3&gt;LED 3MM PTH&lt;/h3&gt;

3 mm, round.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4001">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_PTH_LOCK">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH Locking Footprint&lt;/h3&gt;
5.5mm jack, 2.1mm center pole diameter.
&lt;br&gt; Holes are offset from center 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STANDOFF-ELECTRICAL">
<description>&lt;h3&gt;Standoff (#4 Screw) - w/ Electrical Connection&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw.&lt;/p&gt;
&lt;p&gt;The drill is surrounded by a copper ring, which can be connected to any net.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED-BLEON" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
</element>
<element name="LED-BT" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
</element>
<element name="LED-LD" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
</element>
<element name="DIODE-FLYBK" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="1A/50V/1.1V">
<attribute name="PROD_ID" value="DIO-09176"/>
</element>
<element name="TR" library="SparkFun-DiscreteSemi" package="TO-92" value="200mA/40V">
<attribute name="PROD_ID" value="TRANS-08447"/>
</element>
<element name="BLE3" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="BLE2" library="SparkFun-Connectors" package="1X06_LOCK" value=""/>
<element name="BLE1" library="SparkFun-Connectors" package="1X06_LOCK" value=""/>
<element name="R-BLEON" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R-BT" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="USB-B" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="JUICER" library="SparkFun-Connectors" package="POWER_JACK_PTH_LOCK" value="POWER_JACKPTH_LOCK">
<attribute name="PROD_ID" value="CONN-08197"/>
<attribute name="SF_ID" value="PRT-00119"/>
</element>
<element name="SWITCH" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="GNDMOUNT1" library="SparkFun-Hardware" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="GNDMOUNT2" library="SparkFun-Hardware" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
</elements>
<signals>
<signal name="N$3">
<contactref element="TR" pad="1"/>
<contactref element="DIODE-FLYBK" pad="A"/>
<contactref element="JUICER" pad="PWR"/>
<contactref element="SWITCH" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="DIODE-FLYBK" pad="C"/>
<contactref element="TR" pad="3"/>
<contactref element="BLE2" pad="1"/>
<contactref element="USB-B" pad="1"/>
<contactref element="SWITCH" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED-BLEON" pad="A"/>
<contactref element="R-BLEON" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="LED-BT" pad="A"/>
<contactref element="R-BT" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="BLE1" pad="1"/>
<contactref element="R-BLEON" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="BLE3" pad="2"/>
<contactref element="R-BT" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="BLE3" pad="1"/>
<contactref element="TR" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="LED-LD" pad="A"/>
<contactref element="JUICER" pad="GND"/>
</signal>
<signal name="GND">
<contactref element="LED-LD" pad="K"/>
<contactref element="LED-BT" pad="K"/>
<contactref element="LED-BLEON" pad="K"/>
<contactref element="BLE2" pad="2"/>
<contactref element="USB-B" pad="5"/>
<contactref element="GNDMOUNT1" pad="P1"/>
<contactref element="GNDMOUNT2" pad="P1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
