<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="181.59" y2="0" width="0" layer="20"/>
<wire x1="181.59" y1="0" x2="181.59" y2="61.595" width="0" layer="20"/>
<wire x1="181.59" y1="61.595" x2="0" y2="61.595" width="0" layer="20"/>
<wire x1="0" y1="61.595" x2="0" y2="0" width="0" layer="20"/>
<text>LED Matrix V1.0</text>
<text>-  +</text>
</plain>
<libraries>
<library name="max7219">
<packages>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="LED">
<packages>
<package name="MATRIX_8X8_38MM">
<description>CPD-15088 LED Matrix 8x8 38mm Green</description>
</package>
</packages>
</library>
<library name="teensy">
<packages>
<package name="TEENSY2.0">
<description>Teensy 2.0</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="con-haxn">
<packages>
<package name="2,8-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, round</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="max7219" package="DIL24-3" value="MAX7219CNG">
<attribute name="MF" value="MAXIM"/>
<attribute name="MPN" value="MAX7219CNG"/>
<attribute name="OC_FARNELL" value="1523914"/>
<attribute name="OC_NEWARK" value="34C4018"/>
</element>
<element name="SA" library="LED" package="MATRIX_8X8_38MM" value="LED_8X8_MATRIXYGD2/A"/>
<element name="_1" library="teensy" package="TEENSY2.0" value="TEENSY2.0"/>
<element name="IC2" library="max7219" package="DIL24-3" value="MAX7219CNG">
<attribute name="MF" value="MAXIM"/>
<attribute name="MPN" value="MAX7219CNG"/>
<attribute name="OC_FARNELL" value="1523914"/>
<attribute name="OC_NEWARK" value="34C4018"/>
</element>
<element name="SB" library="LED" package="MATRIX_8X8_38MM" value="LED_8X8_MATRIXYGD2/A"/>
<element name="IC3" library="max7219" package="DIL24-3" value="MAX7219CNG">
<attribute name="MF" value="MAXIM"/>
<attribute name="MPN" value="MAX7219CNG"/>
<attribute name="OC_FARNELL" value="1523914"/>
<attribute name="OC_NEWARK" value="34C4018"/>
</element>
<element name="SC" library="LED" package="MATRIX_8X8_38MM" value="LED_8X8_MATRIXYGD2/A"/>
<element name="IC4" library="max7219" package="DIL24-3" value="MAX7219CNG">
<attribute name="MF" value="MAXIM"/>
<attribute name="MPN" value="MAX7219CNG"/>
<attribute name="OC_FARNELL" value="1523914"/>
<attribute name="OC_NEWARK" value="34C4018"/>
</element>
<element name="SD" library="LED" package="MATRIX_8X8_38MM" value="LED_8X8_MATRIXYGD2/A"/>
<element name="R1" library="adafruit" package="0204/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0204/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0204/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0204/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="con-haxn" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="H2" library="con-haxn" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="H3" library="con-haxn" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="H4" library="con-haxn" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="H5" library="con-haxn" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="H6" library="con-haxn" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="JP1" library="jumper" package="JP1" value=""/>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="S2" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="9"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC4" pad="9"/>
<contactref element="_1" pad="GND"/>
<contactref element="_1" pad="GRND1"/>
<contactref element="H1" pad="B2,8"/>
<contactref element="H2" pad="B2,8"/>
<contactref element="H3" pad="B2,8"/>
<contactref element="H4" pad="B2,8"/>
<contactref element="H5" pad="B2,8"/>
<contactref element="H6" pad="B2,8"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SA13">
<contactref element="SA" pad="13"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="SA3">
<contactref element="SA" pad="3"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="SA4">
<contactref element="SA" pad="4"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="SA10">
<contactref element="SA" pad="10"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="SA6">
<contactref element="SA" pad="6"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="SA11">
<contactref element="SA" pad="11"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="SA15">
<contactref element="SA" pad="15"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="SA16">
<contactref element="SA" pad="16"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="SB9">
<contactref element="SB" pad="9"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="SC14">
<contactref element="SC" pad="14"/>
<contactref element="IC3" pad="17"/>
</signal>
<signal name="SC8">
<contactref element="SC" pad="8"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="SC12">
<contactref element="SC" pad="12"/>
<contactref element="IC3" pad="21"/>
</signal>
<signal name="SC1">
<contactref element="SC" pad="1"/>
<contactref element="IC3" pad="23"/>
</signal>
<signal name="SC7">
<contactref element="SC" pad="7"/>
<contactref element="IC3" pad="20"/>
</signal>
<signal name="SC2">
<contactref element="SC" pad="2"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="SC5">
<contactref element="SC" pad="5"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="SC9">
<contactref element="SC" pad="9"/>
<contactref element="IC3" pad="22"/>
</signal>
<signal name="SB13">
<contactref element="SB" pad="13"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="SB3">
<contactref element="SB" pad="3"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="SB4">
<contactref element="SB" pad="4"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="SB10">
<contactref element="SB" pad="10"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="SB6">
<contactref element="SB" pad="6"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="SB11">
<contactref element="SB" pad="11"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="SB15">
<contactref element="SB" pad="15"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="SB16">
<contactref element="SB" pad="16"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="SB14">
<contactref element="SB" pad="14"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="SB8">
<contactref element="SB" pad="8"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="SB12">
<contactref element="SB" pad="12"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="SB1">
<contactref element="SB" pad="1"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="SB7">
<contactref element="SB" pad="7"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="SB2">
<contactref element="SB" pad="2"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="SB5">
<contactref element="SB" pad="5"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="SC3">
<contactref element="SC" pad="3"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="SC4">
<contactref element="SC" pad="4"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="SC6">
<contactref element="SC" pad="6"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="SC10">
<contactref element="SC" pad="10"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="SC11">
<contactref element="SC" pad="11"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="SC13">
<contactref element="SC" pad="13"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="SC15">
<contactref element="SC" pad="15"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="SC16">
<contactref element="SC" pad="16"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="SD9">
<contactref element="SD" pad="9"/>
<contactref element="IC4" pad="22"/>
</signal>
<signal name="SD14">
<contactref element="SD" pad="14"/>
<contactref element="IC4" pad="17"/>
</signal>
<signal name="SD8">
<contactref element="SD" pad="8"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="SD12">
<contactref element="SD" pad="12"/>
<contactref element="IC4" pad="21"/>
</signal>
<signal name="SD1">
<contactref element="SD" pad="1"/>
<contactref element="IC4" pad="23"/>
</signal>
<signal name="SD7">
<contactref element="SD" pad="7"/>
<contactref element="IC4" pad="20"/>
</signal>
<signal name="SD2">
<contactref element="SD" pad="2"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="SD5">
<contactref element="SD" pad="5"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="SD13">
<contactref element="SD" pad="13"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="SD3">
<contactref element="SD" pad="3"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="SD4">
<contactref element="SD" pad="4"/>
<contactref element="IC4" pad="10"/>
</signal>
<signal name="SD10">
<contactref element="SD" pad="10"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="SD6">
<contactref element="SD" pad="6"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="SD11">
<contactref element="SD" pad="11"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="SD15">
<contactref element="SD" pad="15"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="SD16">
<contactref element="SD" pad="16"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="SA9">
<contactref element="SA" pad="9"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="SA14">
<contactref element="SA" pad="14"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="SA8">
<contactref element="SA" pad="8"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="SA12">
<contactref element="SA" pad="12"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="SA1">
<contactref element="SA" pad="1"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="SA7">
<contactref element="SA" pad="7"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="SA2">
<contactref element="SA" pad="2"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="SA5">
<contactref element="SA" pad="5"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC3" pad="13"/>
<contactref element="IC4" pad="13"/>
<contactref element="_1" pad="B1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC3" pad="12"/>
<contactref element="IC4" pad="12"/>
<contactref element="_1" pad="B2"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="24"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC4" pad="24"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC3" pad="24"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="N$12">
<contactref element="IC2" pad="18"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC3" pad="18"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC4" pad="18"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R4" pad="2"/>
<contactref element="IC4" pad="19"/>
<contactref element="R3" pad="2"/>
<contactref element="IC3" pad="19"/>
<contactref element="R2" pad="2"/>
<contactref element="IC2" pad="19"/>
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="19"/>
<contactref element="JP1" pad="1"/>
<contactref element="_1" pad="5V2"/>
</signal>
<signal name="N$6">
<contactref element="IC4" pad="1"/>
<contactref element="_1" pad="B0"/>
</signal>
<signal name="N$7">
<contactref element="S1" pad="1"/>
<contactref element="_1" pad="F0"/>
</signal>
<signal name="N$8">
<contactref element="_1" pad="F1"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="S2" pad="1"/>
<contactref element="_1" pad="F4"/>
</signal>
<signal name="N$15">
<contactref element="S2" pad="3"/>
<contactref element="_1" pad="F5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
