<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="21.59" x2="5.08" y2="8.89" width="0.1524" layer="20"/>
<wire x1="5.08" y1="8.89" x2="19.05" y2="8.89" width="0.1524" layer="20"/>
<wire x1="19.05" y1="8.89" x2="19.05" y2="21.59" width="0.1524" layer="20"/>
<wire x1="19.05" y1="21.59" x2="5.08" y2="21.59" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-B-MICRO-SMD">
<description>&lt;h3&gt;USB - microB SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Micro-USB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_MICRO-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="SparkFun-Connectors" package="USB-B-MICRO-SMD" value="">
<attribute name="VALUE"/>
</element>
<element name="E$2" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$2">
<contactref element="E$1" pad="VBUS"/>
<contactref element="E$2" pad="5"/>
</signal>
<signal name="S$3">
<contactref element="E$1" pad="D-"/>
<contactref element="E$2" pad="4"/>
</signal>
<signal name="S$4">
<contactref element="E$1" pad="D+"/>
<contactref element="E$2" pad="3"/>
</signal>
<signal name="S$5">
<contactref element="E$1" pad="ID"/>
<contactref element="E$2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="E$1" pad="GND"/>
<contactref element="E$2" pad="1"/>
<contactref element="E$1" pad="SHIELD3"/>
<contactref element="E$1" pad="SHIELD1"/>
<contactref element="E$1" pad="SHIELD2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
