<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="-0.635" y1="19.685" x2="2.54" y2="23.495" width="0.1524" layer="20" curve="-90"/>
<wire x1="2.54" y1="23.495" x2="5.08" y2="23.495" width="0.1524" layer="20"/>
<wire x1="13.97" y1="23.495" x2="16.51" y2="23.495" width="0.1524" layer="20"/>
<wire x1="16.51" y1="23.495" x2="19.685" y2="20.32" width="0.1524" layer="20" curve="-90"/>
<wire x1="19.685" y1="20.32" x2="19.685" y2="5.08" width="0.1524" layer="20"/>
<wire x1="19.685" y1="5.08" x2="16.51" y2="1.27" width="0.1524" layer="20" curve="-90"/>
<wire x1="16.51" y1="1.27" x2="13.97" y2="1.27" width="0.1524" layer="20"/>
<wire x1="5.08" y1="1.27" x2="2.54" y2="1.27" width="0.1524" layer="20"/>
<wire x1="2.54" y1="1.27" x2="-0.635" y2="4.445" width="0.1524" layer="20" curve="-90"/>
<wire x1="-0.635" y1="4.445" x2="-0.635" y2="19.685" width="0.1524" layer="20"/>
<wire x1="5.08" y1="23.495" x2="5.08" y2="24.765" width="0.1524" layer="20"/>
<wire x1="5.08" y1="24.765" x2="9.525" y2="29.21" width="0.1524" layer="20" curve="-90"/>
<wire x1="9.525" y1="29.21" x2="13.97" y2="24.765" width="0.1524" layer="20" curve="-90"/>
<wire x1="13.97" y1="24.765" x2="13.97" y2="23.495" width="0.1524" layer="20"/>
<wire x1="5.08" y1="1.27" x2="5.08" y2="0.635" width="0.1524" layer="20"/>
<wire x1="5.08" y1="0.635" x2="9.525" y2="-3.81" width="0.1524" layer="20" curve="90"/>
<wire x1="9.525" y1="-3.81" x2="13.97" y2="0.635" width="0.1524" layer="20" curve="90"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="1.27" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="Circular Micro-D 5 Pin">
<packages>
<package name="MD15">
</package>
</packages>
</library>
<library name="Micro-D 25">
<packages>
<package name="MD09">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CMD1" library="Circular Micro-D 5 Pin" package="MD15" value="MD15"/>
<element name="CMD2" library="Circular Micro-D 5 Pin" package="MD15" value="MD15"/>
<element name="CMD3" library="Circular Micro-D 5 Pin" package="MD15" value="MD15"/>
<element name="CMD4" library="Circular Micro-D 5 Pin" package="MD15" value="MD15"/>
<element name="CMD5" library="Circular Micro-D 5 Pin" package="MD15" value="MD15"/>
<element name="CMD6" library="Circular Micro-D 5 Pin" package="MD15" value="MD15"/>
<element name="U$1" library="Micro-D 25" package="MD09" value="MD09"/>
<element name="U$2" library="holes" package="2,8" value=""/>
<element name="U$3" library="holes" package="2,8" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="CMD1" pad="P1"/>
<contactref element="U$1" pad="P1"/>
</signal>
<signal name="N$2">
<contactref element="CMD1" pad="P5"/>
<contactref element="U$1" pad="P2"/>
</signal>
<signal name="N$3">
<contactref element="CMD1" pad="P3"/>
<contactref element="U$1" pad="P3"/>
</signal>
<signal name="N$4">
<contactref element="CMD1" pad="P4"/>
<contactref element="U$1" pad="P4"/>
</signal>
<signal name="N$5">
<contactref element="CMD2" pad="P1"/>
<contactref element="U$1" pad="P5"/>
</signal>
<signal name="N$6">
<contactref element="CMD2" pad="P5"/>
<contactref element="U$1" pad="P6"/>
</signal>
<signal name="N$7">
<contactref element="CMD2" pad="P3"/>
<contactref element="U$1" pad="P7"/>
</signal>
<signal name="N$8">
<contactref element="CMD2" pad="P4"/>
<contactref element="U$1" pad="P8"/>
</signal>
<signal name="N$9">
<contactref element="CMD3" pad="P1"/>
<contactref element="U$1" pad="P9"/>
</signal>
<signal name="N$10">
<contactref element="CMD3" pad="P5"/>
<contactref element="U$1" pad="P10"/>
</signal>
<signal name="N$11">
<contactref element="CMD3" pad="P3"/>
<contactref element="U$1" pad="P11"/>
</signal>
<signal name="N$12">
<contactref element="CMD3" pad="P4"/>
<contactref element="U$1" pad="P12"/>
</signal>
<signal name="N$13">
<contactref element="CMD4" pad="P1"/>
<contactref element="U$1" pad="P13"/>
</signal>
<signal name="N$14">
<contactref element="CMD4" pad="P5"/>
<contactref element="U$1" pad="P14"/>
</signal>
<signal name="N$15">
<contactref element="CMD4" pad="P3"/>
<contactref element="U$1" pad="P15"/>
</signal>
<signal name="N$16">
<contactref element="CMD4" pad="P4"/>
<contactref element="U$1" pad="P16"/>
</signal>
<signal name="N$17">
<contactref element="CMD5" pad="P1"/>
<contactref element="U$1" pad="P17"/>
</signal>
<signal name="N$18">
<contactref element="CMD5" pad="P5"/>
<contactref element="U$1" pad="P18"/>
</signal>
<signal name="N$19">
<contactref element="CMD5" pad="P3"/>
<contactref element="U$1" pad="P19"/>
</signal>
<signal name="N$20">
<contactref element="CMD5" pad="P4"/>
<contactref element="U$1" pad="P20"/>
</signal>
<signal name="N$21">
<contactref element="CMD6" pad="P1"/>
<contactref element="U$1" pad="P21"/>
</signal>
<signal name="N$22">
<contactref element="CMD6" pad="P5"/>
<contactref element="U$1" pad="P22"/>
</signal>
<signal name="N$23">
<contactref element="CMD6" pad="P3"/>
<contactref element="U$1" pad="P23"/>
</signal>
<signal name="N$24">
<contactref element="CMD6" pad="P4"/>
<contactref element="U$1" pad="P24"/>
</signal>
<signal name="GND">
<contactref element="CMD2" pad="P2"/>
<contactref element="CMD3" pad="P2"/>
<contactref element="CMD4" pad="P2"/>
<contactref element="CMD5" pad="P2"/>
<contactref element="CMD6" pad="P2"/>
<contactref element="CMD1" pad="P2"/>
<contactref element="U$1" pad="P25"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
