<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="89.84" y2="0" width="0" layer="20"/>
<wire x1="89.84" y1="0" x2="89.84" y2="58.41" width="0" layer="20"/>
<wire x1="89.84" y1="58.41" x2="0" y2="58.41" width="0" layer="20"/>
<wire x1="0" y1="58.41" x2="0" y2="0" width="0" layer="20"/>
<text>www.sergiomorales.me</text>
<text>I.A.S</text>
<text>CONTROLS PORT A</text>
<text>B0</text>
<text>I.A.S</text>
<text>Integrated
Appliance
System</text>
<text>www.sergiomorales.me</text>
<text>Revision 6
04/01/16</text>
<text>CONTROLS PORT B</text>
<text>ISP CONTROLS</text>
<text>CONTROLS EXT</text>
<text>BLUETOOTH</text>
<text>16 VDC MAX IN
5V REGULATED</text>
<text>LEVEL SHIFTER</text>
<text>SHIFT REGISTER</text>
<text>16x2 LCD</text>
<text>NOKIA 5110 LCD</text>
<text>DHT22 SENSOR</text>
<text>DSB18B20 SENSOR</text>
<text>ISP INTERFACE</text>
<text>INTERFACE EXT</text>
<text>8x8 KEYPAD</text>
<text>PIR SENSOR/EXT</text>
<text>CONTROLS PORT C</text>
<text>LCD EN</text>
<text>B1</text>
<text>...</text>
<text>...</text>
<text>B7</text>
<text>GND</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>RESET</text>
<text>VCC</text>
<text>GND</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>RESET</text>
<text>VCC</text>
<text>B6</text>
<text>A7</text>
<text>D7</text>
<text>D6</text>
<text>D5</text>
<text>D4</text>
<text>D3</text>
<text>D2</text>
<text>RESET</text>
<text>ENABLE</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>DQ</text>
<text>VCC</text>
<text>GND</text>
<text>DQ</text>
<text>VCC</text>
<text>UIAREF</text>
<text>XTAL2</text>
<text>XTAL1</text>
<text>AREF</text>
<text>D7</text>
<text>D6</text>
<text>D5</text>
<text>D4</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>VCC</text>
<text>A0</text>
<text>A7</text>
<text>...</text>
<text>...</text>
<text>A1</text>
<text>C7</text>
<text>C1</text>
<text>...</text>
<text>...</text>
<text>R4</text>
<text>C1</text>
<text>C2</text>
<text>R3</text>
<text>GND</text>
<text>DQ</text>
<text>VCC</text>
<text>XTAL2</text>
<text>XTAL1</text>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>VIN</text>
<text>VCC</text>
<text>GND</text>
<text>SCE</text>
<text>RESET</text>
<text>DC</text>
<text>DN</text>
<text>CLK</text>
<text>DB0</text>
<text>DB1</text>
<text>...</text>
<text>...</text>
<text>DB7</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_ROUND">
</package>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
<package name="1X06">
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P1524X483-40">
</package>
</packages>
</library>
<library name="sergio">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SPC4077">
<description>&lt;b&gt;DC POWER JACK 2mm&lt;/b&gt;&lt;br&gt; Right Angle, Through Hole, Rated 5A at 16VDC, PC Terminals&lt;p&gt;
Source: www.spctechnology.com .. 84N1161.pdf&lt;br&gt;
Distributor: &lt;b&gt;Farnell (www.Farnell.de)&lt;/b&gt;&lt;br&gt;
Created by Robert Siegler</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="IAS">
<description>Contains the parts to the Integrated Appliance System PCB, revision .06.</description>
<packages>
<package name="DIL16">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="16X2_LCD" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="16X2_LCD_ENABLE" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="74LS595D_SHIFT_REGISTER" library="74xx-us" package="DIL16" value="74LS595N">
<attribute name="OC_NEWARK" value="34R8835"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="SN74LS595D"/>
<attribute name="VALUE"/>
</element>
<element name="8X8_KEYPAD" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="BLUETOOTH_MODULE" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1206" value="1uF">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="1206" value="1uF">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONTROLS" library="Atmel_By_element14_Batch_1-00" package="DIP254P1524X483-40" value="ATMEGA1284P-PU">
<attribute name="OC_NEWARK" value="15R0264"/>
<attribute name="MF" value=""/>
<attribute name="PACKAGE" value="PDIP-40"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="MPN" value="ATMEGA1284P-PU"/>
<attribute name="OC_FARNELL" value="1715481"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CTRLS_EXT" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="CTRLS_PORT_A" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="CTRLS_PORT_B" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="CTRLS_PORT_C" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="DHT22_SENSOR" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="DSB18B20_SENSOR" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="sergio" package="SOT223" value="REG1117">
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="REG1117"/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INTERFACE" library="Atmel_By_element14_Batch_1-00" package="DIP254P1524X483-40" value="ATMEGA1284P-PU">
<attribute name="OC_NEWARK" value="15R0264"/>
<attribute name="MF" value=""/>
<attribute name="PACKAGE" value="PDIP-40"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="MPN" value="ATMEGA1284P-PU"/>
<attribute name="OC_FARNELL" value="1715481"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP_ADAPTER_CTRLS" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="ISP_ADAPTER_UI" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-jack" package="SPC4077" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NOKIA_5110_LCD" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="PIR_SENSOR_ETC" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="1206" value="10k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="1206" value="10k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="1206" value="2k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="1206" value="1k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="1206" value="1k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UI_EXT" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LEVEL_SHIFTER_3P3V" library="IAS" package="DIL16" value="CD74HC4050EDIL16">
<attribute name="MANUFACTURER_PART_NUMBER" value="CD74HC4050EE4"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2015 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="RSPARTNUMBER" value="7092573"/>
<attribute name="FAMILY" value="Buffer and Line Driver"/>
<attribute name="SECTION" value="Standard and Speciality Logic"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="74LS595D_SHIFT_REGISTER" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="DSB18B20_SENSOR" pad="1"/>
<contactref element="DHT22_SENSOR" pad="1"/>
<contactref element="BLUETOOTH_MODULE" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="ISP_ADAPTER_UI" pad="6"/>
<contactref element="ISP_ADAPTER_CTRLS" pad="6"/>
<contactref element="PIR_SENSOR_ETC" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="74LS595D_SHIFT_REGISTER" pad="13"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="16X2_LCD_ENABLE" pad="4"/>
<contactref element="R5" pad="2"/>
<contactref element="INTERFACE" pad="11"/>
<contactref element="INTERFACE" pad="31"/>
<contactref element="CONTROLS" pad="11"/>
<contactref element="CONTROLS" pad="31"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="8"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="14"/>
</signal>
<signal name="VCC">
<contactref element="74LS595D_SHIFT_REGISTER" pad="16"/>
<contactref element="INTERFACE" pad="10"/>
<contactref element="INTERFACE" pad="30"/>
<contactref element="C1" pad="1"/>
<contactref element="CONTROLS" pad="30"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="DSB18B20_SENSOR" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="DHT22_SENSOR" pad="4"/>
<contactref element="BLUETOOTH_MODULE" pad="1"/>
<contactref element="ISP_ADAPTER_UI" pad="5"/>
<contactref element="ISP_ADAPTER_CTRLS" pad="5"/>
<contactref element="PIR_SENSOR_ETC" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="16X2_LCD_ENABLE" pad="3"/>
<contactref element="POWER" pad="A"/>
<contactref element="CONTROLS" pad="10"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="1"/>
</signal>
<signal name="NLCD_SCLK">
<contactref element="INTERFACE" pad="40"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="3"/>
</signal>
<signal name="NLCD_DN">
<contactref element="INTERFACE" pad="39"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="5"/>
</signal>
<signal name="NLCD_DC">
<contactref element="INTERFACE" pad="38"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="7"/>
</signal>
<signal name="NLCD_RST">
<contactref element="INTERFACE" pad="37"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="9"/>
</signal>
<signal name="SER">
<contactref element="74LS595D_SHIFT_REGISTER" pad="14"/>
<contactref element="INTERFACE" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="74LS595D_SHIFT_REGISTER" pad="11"/>
<contactref element="INTERFACE" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="74LS595D_SHIFT_REGISTER" pad="10"/>
<contactref element="INTERFACE" pad="4"/>
</signal>
<signal name="RCK">
<contactref element="74LS595D_SHIFT_REGISTER" pad="12"/>
<contactref element="INTERFACE" pad="2"/>
</signal>
<signal name="DB0">
<contactref element="74LS595D_SHIFT_REGISTER" pad="15"/>
<contactref element="16X2_LCD" pad="8"/>
</signal>
<signal name="DB1">
<contactref element="74LS595D_SHIFT_REGISTER" pad="1"/>
<contactref element="16X2_LCD" pad="7"/>
</signal>
<signal name="DB2">
<contactref element="74LS595D_SHIFT_REGISTER" pad="2"/>
<contactref element="16X2_LCD" pad="6"/>
</signal>
<signal name="DB3">
<contactref element="74LS595D_SHIFT_REGISTER" pad="3"/>
<contactref element="16X2_LCD" pad="5"/>
</signal>
<signal name="DB4">
<contactref element="74LS595D_SHIFT_REGISTER" pad="4"/>
<contactref element="16X2_LCD" pad="4"/>
</signal>
<signal name="DB5">
<contactref element="74LS595D_SHIFT_REGISTER" pad="5"/>
<contactref element="16X2_LCD" pad="3"/>
</signal>
<signal name="DB6">
<contactref element="74LS595D_SHIFT_REGISTER" pad="6"/>
<contactref element="16X2_LCD" pad="2"/>
</signal>
<signal name="DB7">
<contactref element="74LS595D_SHIFT_REGISTER" pad="7"/>
<contactref element="16X2_LCD" pad="1"/>
</signal>
<signal name="ROW4">
<contactref element="INTERFACE" pad="22"/>
<contactref element="8X8_KEYPAD" pad="8"/>
</signal>
<signal name="ROW3">
<contactref element="INTERFACE" pad="23"/>
<contactref element="8X8_KEYPAD" pad="7"/>
</signal>
<signal name="ROW2">
<contactref element="INTERFACE" pad="24"/>
<contactref element="8X8_KEYPAD" pad="6"/>
</signal>
<signal name="ROW1">
<contactref element="INTERFACE" pad="25"/>
<contactref element="8X8_KEYPAD" pad="5"/>
</signal>
<signal name="COL4">
<contactref element="INTERFACE" pad="26"/>
<contactref element="8X8_KEYPAD" pad="4"/>
</signal>
<signal name="COL3">
<contactref element="INTERFACE" pad="27"/>
<contactref element="8X8_KEYPAD" pad="3"/>
</signal>
<signal name="COL2">
<contactref element="INTERFACE" pad="28"/>
<contactref element="8X8_KEYPAD" pad="2"/>
</signal>
<signal name="COL1">
<contactref element="INTERFACE" pad="29"/>
<contactref element="8X8_KEYPAD" pad="1"/>
</signal>
<signal name="DS18B20_DQ">
<contactref element="INTERFACE" pad="34"/>
<contactref element="DSB18B20_SENSOR" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="DHT22_DQ">
<contactref element="INTERFACE" pad="35"/>
<contactref element="DHT22_SENSOR" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="USART_D0">
<contactref element="INTERFACE" pad="14"/>
<contactref element="CONTROLS" pad="15"/>
</signal>
<signal name="USART_D1">
<contactref element="INTERFACE" pad="15"/>
<contactref element="CONTROLS" pad="14"/>
</signal>
<signal name="BT_TX">
<contactref element="BLUETOOTH_MODULE" pad="3"/>
<contactref element="CONTROLS" pad="16"/>
</signal>
<signal name="N$7">
<contactref element="BLUETOOTH_MODULE" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="BT_RX">
<contactref element="R4" pad="1"/>
<contactref element="CONTROLS" pad="17"/>
</signal>
<signal name="LCD_RS">
<contactref element="INTERFACE" pad="5"/>
<contactref element="16X2_LCD_ENABLE" pad="1"/>
</signal>
<signal name="LCD_EN">
<contactref element="INTERFACE" pad="6"/>
<contactref element="ISP_ADAPTER_UI" pad="1"/>
<contactref element="16X2_LCD_ENABLE" pad="2"/>
</signal>
<signal name="PIR_DQ">
<contactref element="INTERFACE" pad="7"/>
<contactref element="ISP_ADAPTER_UI" pad="2"/>
<contactref element="PIR_SENSOR_ETC" pad="5"/>
</signal>
<signal name="NSCLK">
<contactref element="NOKIA_5110_LCD" pad="5"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="2"/>
</signal>
<signal name="NDN">
<contactref element="NOKIA_5110_LCD" pad="4"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="4"/>
</signal>
<signal name="NDC">
<contactref element="NOKIA_5110_LCD" pad="3"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="6"/>
</signal>
<signal name="NRST">
<contactref element="NOKIA_5110_LCD" pad="2"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="10"/>
</signal>
<signal name="NSCE">
<contactref element="NOKIA_5110_LCD" pad="1"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="12"/>
</signal>
<signal name="NLCD_SCE">
<contactref element="INTERFACE" pad="36"/>
<contactref element="LEVEL_SHIFTER_3P3V" pad="11"/>
</signal>
<signal name="UI_PB7">
<contactref element="INTERFACE" pad="8"/>
<contactref element="ISP_ADAPTER_UI" pad="3"/>
<contactref element="UI_EXT" pad="8"/>
</signal>
<signal name="UI_PA7">
<contactref element="INTERFACE" pad="33"/>
<contactref element="UI_EXT" pad="7"/>
</signal>
<signal name="UI_PD2">
<contactref element="INTERFACE" pad="16"/>
<contactref element="UI_EXT" pad="1"/>
</signal>
<signal name="UI_PD3">
<contactref element="INTERFACE" pad="17"/>
<contactref element="UI_EXT" pad="2"/>
</signal>
<signal name="UI_PD4">
<contactref element="INTERFACE" pad="18"/>
<contactref element="UI_EXT" pad="3"/>
</signal>
<signal name="UI_PD5">
<contactref element="INTERFACE" pad="19"/>
<contactref element="UI_EXT" pad="4"/>
</signal>
<signal name="UI_PD6">
<contactref element="INTERFACE" pad="20"/>
<contactref element="UI_EXT" pad="5"/>
</signal>
<signal name="UI_PD7">
<contactref element="INTERFACE" pad="21"/>
<contactref element="UI_EXT" pad="6"/>
</signal>
<signal name="CTRLS_PD4">
<contactref element="CONTROLS" pad="18"/>
<contactref element="CTRLS_EXT" pad="1"/>
</signal>
<signal name="CTRLS_PD5">
<contactref element="CONTROLS" pad="19"/>
<contactref element="CTRLS_EXT" pad="2"/>
</signal>
<signal name="CTRLS_PD6">
<contactref element="CONTROLS" pad="20"/>
<contactref element="CTRLS_EXT" pad="3"/>
</signal>
<signal name="CTRLS_PD7">
<contactref element="CONTROLS" pad="21"/>
<contactref element="CTRLS_EXT" pad="4"/>
</signal>
<signal name="CTRLS_PA0">
<contactref element="CONTROLS" pad="40"/>
<contactref element="CTRLS_PORT_A" pad="1"/>
</signal>
<signal name="CTRLS_PA1">
<contactref element="CONTROLS" pad="39"/>
<contactref element="CTRLS_PORT_A" pad="2"/>
</signal>
<signal name="CTRLS_PA2">
<contactref element="CONTROLS" pad="38"/>
<contactref element="CTRLS_PORT_A" pad="3"/>
</signal>
<signal name="CTRLS_PA3">
<contactref element="CONTROLS" pad="37"/>
<contactref element="CTRLS_PORT_A" pad="4"/>
</signal>
<signal name="CTRLS_PA4">
<contactref element="CONTROLS" pad="36"/>
<contactref element="CTRLS_PORT_A" pad="5"/>
</signal>
<signal name="CTRLS_PA5">
<contactref element="CONTROLS" pad="35"/>
<contactref element="CTRLS_PORT_A" pad="6"/>
</signal>
<signal name="CTRLS_PA6">
<contactref element="CONTROLS" pad="34"/>
<contactref element="CTRLS_PORT_A" pad="7"/>
</signal>
<signal name="CTRLS_PA7">
<contactref element="CONTROLS" pad="33"/>
<contactref element="CTRLS_PORT_A" pad="8"/>
</signal>
<signal name="CTRLS_PB0">
<contactref element="CONTROLS" pad="1"/>
<contactref element="CTRLS_PORT_B" pad="1"/>
</signal>
<signal name="CTRLS_PB1">
<contactref element="CONTROLS" pad="2"/>
<contactref element="CTRLS_PORT_B" pad="2"/>
</signal>
<signal name="CTRLS_PB2">
<contactref element="CONTROLS" pad="3"/>
<contactref element="CTRLS_PORT_B" pad="3"/>
</signal>
<signal name="CTRLS_PB3">
<contactref element="CONTROLS" pad="4"/>
<contactref element="CTRLS_PORT_B" pad="4"/>
</signal>
<signal name="CTRLS_PB4">
<contactref element="CONTROLS" pad="5"/>
<contactref element="CTRLS_PORT_B" pad="5"/>
</signal>
<signal name="CTRLS_PB5">
<contactref element="ISP_ADAPTER_CTRLS" pad="1"/>
<contactref element="CONTROLS" pad="6"/>
<contactref element="CTRLS_PORT_B" pad="6"/>
</signal>
<signal name="CTRLS_PB6">
<contactref element="ISP_ADAPTER_CTRLS" pad="2"/>
<contactref element="CONTROLS" pad="7"/>
<contactref element="CTRLS_PORT_B" pad="7"/>
</signal>
<signal name="CTRLS_PB7">
<contactref element="ISP_ADAPTER_CTRLS" pad="3"/>
<contactref element="CONTROLS" pad="8"/>
<contactref element="CTRLS_PORT_B" pad="8"/>
</signal>
<signal name="UI_RST">
<contactref element="INTERFACE" pad="9"/>
<contactref element="ISP_ADAPTER_UI" pad="4"/>
</signal>
<signal name="CTRLS_RST">
<contactref element="CONTROLS" pad="9"/>
<contactref element="ISP_ADAPTER_CTRLS" pad="4"/>
</signal>
<signal name="CTRLS_PC0">
<contactref element="CONTROLS" pad="22"/>
<contactref element="CTRLS_PORT_C" pad="1"/>
</signal>
<signal name="CTRLS_PC1">
<contactref element="CTRLS_PORT_C" pad="2"/>
<contactref element="CONTROLS" pad="23"/>
</signal>
<signal name="CTRLS_PC2">
<contactref element="CONTROLS" pad="24"/>
<contactref element="CTRLS_PORT_C" pad="3"/>
</signal>
<signal name="CTRLS_PC3">
<contactref element="CTRLS_PORT_C" pad="4"/>
<contactref element="CONTROLS" pad="25"/>
</signal>
<signal name="CTRLS_PC4">
<contactref element="CONTROLS" pad="26"/>
<contactref element="CTRLS_PORT_C" pad="5"/>
</signal>
<signal name="CTRLS_PC5">
<contactref element="CTRLS_PORT_C" pad="6"/>
<contactref element="CONTROLS" pad="27"/>
</signal>
<signal name="CTRLS_PC6">
<contactref element="CONTROLS" pad="28"/>
<contactref element="CTRLS_PORT_C" pad="7"/>
</signal>
<signal name="CTRLS_PC7">
<contactref element="CONTROLS" pad="29"/>
<contactref element="CTRLS_PORT_C" pad="8"/>
</signal>
<signal name="UI_AREF">
<contactref element="INTERFACE" pad="32"/>
<contactref element="CTRLS_EXT" pad="8"/>
</signal>
<signal name="CTRLS_AREF">
<contactref element="CONTROLS" pad="32"/>
<contactref element="CTRLS_EXT" pad="5"/>
</signal>
<signal name="CTRLS_XTAL1">
<contactref element="CONTROLS" pad="13"/>
<contactref element="CTRLS_EXT" pad="6"/>
</signal>
<signal name="CTRLS_XTAL2">
<contactref element="CONTROLS" pad="12"/>
<contactref element="CTRLS_EXT" pad="7"/>
</signal>
<signal name="UI_XTAL2">
<contactref element="INTERFACE" pad="12"/>
<contactref element="PIR_SENSOR_ETC" pad="3"/>
</signal>
<signal name="UI_XTAL1">
<contactref element="INTERFACE" pad="13"/>
<contactref element="PIR_SENSOR_ETC" pad="4"/>
</signal>
<signal name="VIN">
<contactref element="J1" pad="3"/>
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="POWER" pad="K"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VCC_2">
</signal>
<signal name="VCC_3">
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
