<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="33.147" x2="49.581" y2="33.147" width="0" layer="20"/>
<wire x1="49.581" y1="33.147" x2="49.581" y2="80" width="0" layer="20"/>
<wire x1="49.581" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="33.147" width="0" layer="20"/>
<text>+</text>
<text>PWR</text>
<text>DTR</text>
<text>RI</text>
<text>DCD</text>
<text>CTS</text>
<text>RTS</text>
<text>TXD</text>
<text>RXD</text>
<text>RST</text>
<text>BrK 2015</text>
<text>BT</text>
<text>DATA</text>
<text>CLK</text>
<text>RST</text>
<text>SCL</text>
<text>SDA</text>
<text>GND</text>
<text>NC</text>
<text>3.4-4.4V</text>
<text>+</text>
<text>3.4-4.4V</text>
<text>GPIO6</text>
<text>GPIO5</text>
<text>PWM1</text>
<text>PWM2</text>
<text>ADC2</text>
<text>ADC1</text>
<text>+</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="TESTPOINT_ROUND_2MM">
<description>Testpoint - Round 2mm</description>
</package>
<package name="RESPACK_4X0603">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="1210">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="U.FL">
</package>
<package name="SIM900_SMT">
</package>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
<package name="1X09_LOCK">
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="Speicherkarten-SockelWR-CRD">
<description>&lt;BR&gt;Würth Elektronik -- Electronic Interconnect &amp; Electromechanical Solutions&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Version 6,  January 13th 2015
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="693023010811">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ANTENNA-CHIP5">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="ANARCHY_LOGO">
<description>Anarchy Logo by BrK</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="logo">
<description>&lt;b&gt;Electronic logos&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="ESD_10.00">
<description>&lt;b&gt;Logo ESD 10 mm&lt;/b&gt;</description>
</package>
<package name="MUELLTONNE_10.00">
<description>&lt;b&gt;Logo trash / Mülltonne 10 mm&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD.03X.03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="2.8V" library="microbuilder" package="TESTPOINT_ROUND_2MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="microbuilder" package="RESPACK_4X0603" value="33pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="microbuilder" package="RESPACK_4X0603" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="microbuilder" package="RESPACK_4X0603" value="33pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="microbuilder" package="RESPACK_4X0603" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="1210" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="GND" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK">
<attribute name="NAME"/>
</element>
<element name="GPS" library="adafruit" package="U.FL" value=""/>
<element name="GSM" library="adafruit" package="U.FL" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="JP4" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="K1" library="Speicherkarten-SockelWR-CRD" package="693023010811" value="693023010811"/>
<element name="MIC" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK">
<attribute name="NAME"/>
</element>
<element name="NET" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-ARV" value=""/>
<element name="SPK" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK">
<attribute name="NAME"/>
</element>
<element name="STS" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$23" library="SparkFun-RF" package="ANTENNA-CHIP5" value="ANTENNA2SMD5"/>
<element name="SIM808" library="adafruit" package="SIM900_SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB" library="adafruit" package="USB-MINIB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK">
<attribute name="NAME"/>
</element>
<element name="VIN" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="0.1uF"/>
<element name="!ON!" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$31" library="dp_devices" package="ANARCHY_LOGO" value=""/>
<element name="U$32" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="U$33" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="U$35" library="logo" package="ESD_10.00" value=""/>
<element name="U$34" library="logo" package="MUELLTONNE_10.00" value=""/>
<element name="TP1" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="TP2" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="TP3" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="TP4" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="TP5" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="TP6" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
</elements>
<signals>
<signal name="GND">
<contactref element="SIM808" pad="P$40"/>
<contactref element="GSM" pad="1"/>
<contactref element="GSM" pad="2"/>
<contactref element="SIM808" pad="P$3"/>
<contactref element="CN1" pad="2"/>
<contactref element="SIM808" pad="P$2"/>
<contactref element="SIM808" pad="P$1"/>
<contactref element="C1" pad="8"/>
<contactref element="C2" pad="8"/>
<contactref element="C1" pad="5"/>
<contactref element="C2" pad="4"/>
<contactref element="C3" pad="8"/>
<contactref element="C4" pad="8"/>
<contactref element="C3" pad="5"/>
<contactref element="C4" pad="4"/>
<contactref element="GPS" pad="1"/>
<contactref element="GPS" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="NET" pad="C"/>
<contactref element="STS" pad="C"/>
<contactref element="GND" pad="1"/>
<contactref element="GND" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="JP4" pad="4"/>
<contactref element="K1" pad="C5"/>
<contactref element="SIM808" pad="P$18"/>
<contactref element="SIM808" pad="P$34"/>
<contactref element="SIM808" pad="P$52"/>
<contactref element="SIM808" pad="P$51"/>
<contactref element="SIM808" pad="P$36"/>
<contactref element="SIM808" pad="P$54"/>
<contactref element="SIM808" pad="P$67"/>
<contactref element="SIM808" pad="P$68"/>
<contactref element="SIM808" pad="P$64"/>
<contactref element="SIM808" pad="P$65"/>
<contactref element="SIM808" pad="P$28"/>
<contactref element="USB" pad="GND"/>
<contactref element="C8" pad="2"/>
<contactref element="VIN" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="!ON!" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="VCC" pad="1"/>
<contactref element="VCC" pad="2"/>
<contactref element="SIM808" pad="P$6"/>
<contactref element="SIM808" pad="P$4"/>
<contactref element="SIM808" pad="P$5"/>
<contactref element="CN1" pad="1"/>
<contactref element="VIN" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="2.8V" pad="P$1"/>
<contactref element="SIM808" pad="P$7"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="9"/>
<contactref element="SIM808" pad="P$8"/>
<contactref element="!ON!" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="8"/>
<contactref element="SIM808" pad="P$9"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="7"/>
<contactref element="SIM808" pad="P$10"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="6"/>
<contactref element="SIM808" pad="P$11"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="5"/>
<contactref element="SIM808" pad="P$12"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="4"/>
<contactref element="SIM808" pad="P$13"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="3"/>
<contactref element="SIM808" pad="P$14"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="2"/>
<contactref element="SIM808" pad="P$15"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="1"/>
<contactref element="SIM808" pad="P$16"/>
</signal>
<signal name="N$13">
<contactref element="GPS" pad="3"/>
<contactref element="SIM808" pad="P$35"/>
</signal>
<signal name="MICP">
<contactref element="SIM808" pad="P$19"/>
<contactref element="C1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="MIC" pad="1"/>
</signal>
<signal name="MICM">
<contactref element="SIM808" pad="P$20"/>
<contactref element="C1" pad="7"/>
<contactref element="C1" pad="4"/>
<contactref element="C1" pad="6"/>
<contactref element="C2" pad="7"/>
<contactref element="C2" pad="5"/>
<contactref element="C2" pad="6"/>
<contactref element="C2" pad="3"/>
<contactref element="C1" pad="3"/>
<contactref element="MIC" pad="2"/>
</signal>
<signal name="SPKP">
<contactref element="SIM808" pad="P$21"/>
<contactref element="C3" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="SPK" pad="1"/>
</signal>
<signal name="SPKM">
<contactref element="SIM808" pad="P$22"/>
<contactref element="C3" pad="7"/>
<contactref element="C3" pad="4"/>
<contactref element="C3" pad="6"/>
<contactref element="C4" pad="7"/>
<contactref element="C4" pad="5"/>
<contactref element="C4" pad="6"/>
<contactref element="C4" pad="3"/>
<contactref element="C3" pad="3"/>
<contactref element="SPK" pad="2"/>
</signal>
<signal name="SIM_VDD">
<contactref element="SIM808" pad="P$29"/>
<contactref element="K1" pad="C1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="SIM_DATA">
<contactref element="SIM808" pad="P$30"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="SIM_CLK">
<contactref element="SIM808" pad="P$31"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SIM_RST">
<contactref element="SIM808" pad="P$32"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="JP4" pad="2"/>
<contactref element="SIM808" pad="P$39"/>
</signal>
<signal name="SDA">
<contactref element="JP4" pad="3"/>
<contactref element="SIM808" pad="P$38"/>
</signal>
<signal name="N$28">
<contactref element="R1" pad="4"/>
<contactref element="SIM808" pad="P$50"/>
</signal>
<signal name="N$29">
<contactref element="R1" pad="1"/>
<contactref element="SIM808" pad="P$49"/>
</signal>
<signal name="N$11">
<contactref element="C5" pad="1"/>
<contactref element="SIM808" pad="P$17"/>
</signal>
<signal name="N$14">
<contactref element="R1" pad="8"/>
<contactref element="STS" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="R1" pad="5"/>
<contactref element="NET" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="SIM808" pad="P$53"/>
<contactref element="U$23" pad="FEED"/>
</signal>
<signal name="N$12">
<contactref element="GSM" pad="3"/>
<contactref element="SIM808" pad="P$66"/>
</signal>
<signal name="N$18">
<contactref element="SIM808" pad="P$25"/>
<contactref element="USB" pad="VBUS"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="SIM808" pad="P$26"/>
<contactref element="USB" pad="D+"/>
</signal>
<signal name="N$20">
<contactref element="SIM808" pad="P$27"/>
<contactref element="USB" pad="D-"/>
</signal>
<signal name="N$17">
<contactref element="K1" pad="C2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="K1" pad="C3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="K1" pad="C7"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="TP1" pad="P$1"/>
<contactref element="SIM808" pad="P$23"/>
</signal>
<signal name="N$24">
<contactref element="TP2" pad="P$1"/>
<contactref element="SIM808" pad="P$24"/>
</signal>
<signal name="N$25">
<contactref element="SIM808" pad="P$44"/>
<contactref element="TP3" pad="P$1"/>
</signal>
<signal name="N$26">
<contactref element="SIM808" pad="P$43"/>
<contactref element="TP4" pad="P$1"/>
</signal>
<signal name="N$27">
<contactref element="SIM808" pad="P$42"/>
<contactref element="TP5" pad="P$1"/>
</signal>
<signal name="N$30">
<contactref element="SIM808" pad="P$41"/>
<contactref element="TP6" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
