<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="15.24" x2="15.24" y2="0" width="0" layer="20" curve="90"/>
<wire x1="15.24" y1="0" x2="16.51" y2="0" width="0" layer="20"/>
<wire x1="16.51" y1="0" x2="30.48" y2="13.97" width="0" layer="20" curve="90"/>
<wire x1="30.48" y1="13.97" x2="30.48" y2="44.45" width="0" layer="20"/>
<wire x1="30.48" y1="44.45" x2="22.86" y2="53.34" width="0" layer="20" curve="90"/>
<wire x1="22.86" y1="53.34" x2="6.35" y2="53.34" width="0" layer="20"/>
<wire x1="6.35" y1="53.34" x2="0" y2="45.72" width="0" layer="20" curve="90"/>
<wire x1="0" y1="45.72" x2="0" y2="15.24" width="0" layer="20"/>
<text>Jeremy Hong
Hong's Electronics, LLC
Melbourne, FL
Gomdori SAO Rev A.
MADE IN THE USA</text>
<text>Jeremy Hong
Hong's Electronics, LLC
Melbourne, FL
Gomdori SAO Rev A.
MADE IN THE USA</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="2x3_conn">
<packages>
<package name="CONN6_3020-06-0300-00_CNC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="2x3_conn" package="CONN6_3020-06-0300-00_CNC" value="3020-06-0300-00">
<attribute name="COPYRIGHT" value="Copyright (C) 2022 Ultra Librarian. All rights reserved."/>
<attribute name="DIGI-KEY_PART_NUMBER_1" value="1175-1864-ND"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="3020-06-0300-00"/>
<attribute name="MFR_NAME" value="CNC Tech"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
