<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.9715" y2="0" width="0" layer="20"/>
<wire x1="25.9715" y1="0" x2="25.9715" y2="9.5885" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="9.5885" width="0" layer="20"/>
<wire x1="0" y1="9.5885" x2="25.9715" y2="9.5885" width="0" layer="20"/>
<text>620</text>
<text>1</text>
<text>9</text>
<text>1K</text>
<text>620</text>
<text>1K</text>
<text>rev5wR5</text>
<text>grips03
Gen&gt;78</text>
<text>.</text>
<text>1</text>
<text>9</text>
<text>db9 here</text>
<text>1</text>
<text>1</text>
<text>6</text>
<text>6</text>
<text>9</text>
<text>9</text>
<text>5</text>
</plain>
<libraries>
<library name="ref-packages-longpad-dave">
<description>&lt;b&gt;Reference Package&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ATARI_CONNECTOR">
</package>
<package name="1X09">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CMXT3906" library="ref-packages-longpad-dave" package="SOT23-6" value="3DIODE-SOT23-6"/>
<element name="R1" library="SparkFun-Resistors" package="1206" value=""/>
<element name="R2" library="SparkFun-Resistors" package="1206" value=""/>
<element name="R3" library="SparkFun-Resistors" package="1206" value=""/>
<element name="R4" library="SparkFun-Resistors" package="1206" value=""/>
<element name="GEN" library="SparkFun-Connectors" package="ATARI_CONNECTOR" value="ATARI_CONNECTOR"/>
<element name="JP2" library="SparkFun-Connectors" package="1X09" value="M09"/>
</elements>
<signals>
<signal name="C1">
<contactref element="CMXT3906" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="B1">
<contactref element="CMXT3906" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="COM">
<contactref element="CMXT3906" pad="1"/>
<contactref element="CMXT3906" pad="4"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="B">
<contactref element="R3" pad="2"/>
<contactref element="GEN" pad="P$1"/>
</signal>
<signal name="C">
<contactref element="R4" pad="2"/>
<contactref element="GEN" pad="P$4"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="GEN" pad="P$3"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="UP">
<contactref element="GEN" pad="P$5"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="DOWN">
<contactref element="GEN" pad="P$6"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="LEFT">
<contactref element="GEN" pad="P$7"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="C2">
<contactref element="CMXT3906" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="B2">
<contactref element="CMXT3906" pad="5"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="RIGHT">
<contactref element="GEN" pad="P$8"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="5V">
<contactref element="GEN" pad="P$9"/>
<contactref element="GEN" pad="P$2"/>
<contactref element="JP2" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
