<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.86" y2="0" width="0" layer="20"/>
<wire x1="22.86" y1="0" x2="22.86" y2="67.31" width="0" layer="20"/>
<wire x1="22.86" y1="67.31" x2="0" y2="67.31" width="0" layer="20"/>
<wire x1="0" y1="67.31" x2="0" y2="0" width="0" layer="20"/>
<text>G15</text>
<text>G14</text>
<text>G13</text>
<text>G12</text>
<text>5V</text>
<text>G11</text>
<text>GND</text>
<text>G10</text>
<text>G9</text>
<text>G8</text>
<text>G7</text>
<text>G6</text>
<text>G5</text>
<text>G4</text>
<text>G3</text>
<text>G2</text>
<text>G1</text>
<text>3V3</text>
<text>G46</text>
<text>G43</text>
<text>G42</text>
<text>G44</text>
<text>G41</text>
<text>EN</text>
<text>G40</text>
<text>G0</text>
<text>G39</text>
<text>GND</text>
<text>G15</text>
<text>G14</text>
<text>G13</text>
<text>G12</text>
<text>5V</text>
<text>G11</text>
<text>GND</text>
<text>G10</text>
<text>G9</text>
<text>G8</text>
<text>G7</text>
<text>G6</text>
<text>G5</text>
<text>G4</text>
<text>G3</text>
<text>G2</text>
<text>G1</text>
<text>3V3</text>
<text>G46</text>
<text>G43</text>
<text>G42</text>
<text>G44</text>
<text>G41</text>
<text>EN</text>
<text>G40</text>
<text>G0</text>
<text>G39</text>
<text>GND</text>
<text>M5 StampS3</text>
<text>M5 StampS3
FlexyPin Adapter
by Evil Genius Labs</text>
<text>M5 StampS3
FlexyPin Adapter
by Evil Genius Labs</text>
</plain>
<libraries>
<library name="flexy-pin">
<packages>
<package name="FLEXY-PIN-M5-STAMP-S3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X17_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -17 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:17&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_17&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -11 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="flexy-pin" package="FLEXY-PIN-M5-STAMP-S3" value="FLEXY-PIN-M5-STAMP-S3"/>
<element name="J1" library="SparkFun-Connectors" package="1X17_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X11_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="G15">
<contactref element="U$1" pad="G15-2"/>
<contactref element="U$1" pad="G15-1"/>
<contactref element="U$1" pad="G15-3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="G14">
<contactref element="U$1" pad="G14-1"/>
<contactref element="U$1" pad="G14-2"/>
<contactref element="U$1" pad="G14-3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="G13">
<contactref element="U$1" pad="G13-3"/>
<contactref element="U$1" pad="G13-2"/>
<contactref element="U$1" pad="G13-1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="G12">
<contactref element="U$1" pad="G12-2"/>
<contactref element="U$1" pad="G12-1"/>
<contactref element="U$1" pad="G12-3"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="G11">
<contactref element="U$1" pad="G11-1"/>
<contactref element="U$1" pad="G11-2"/>
<contactref element="U$1" pad="G11-3"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="G10">
<contactref element="U$1" pad="G10-2"/>
<contactref element="U$1" pad="G10-1"/>
<contactref element="U$1" pad="G10-3"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="G9">
<contactref element="U$1" pad="G9-1"/>
<contactref element="U$1" pad="G9-3"/>
<contactref element="U$1" pad="G9-2"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="G8">
<contactref element="U$1" pad="G8-3"/>
<contactref element="U$1" pad="G8-2"/>
<contactref element="U$1" pad="G8-1"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="G7">
<contactref element="U$1" pad="G7-2"/>
<contactref element="U$1" pad="G7-1"/>
<contactref element="U$1" pad="G7-3"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="G6">
<contactref element="U$1" pad="G6-3"/>
<contactref element="U$1" pad="G6-2"/>
<contactref element="U$1" pad="G6-1"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="G5">
<contactref element="U$1" pad="G5-2"/>
<contactref element="U$1" pad="G5-1"/>
<contactref element="U$1" pad="G5-3"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="G4">
<contactref element="U$1" pad="G4-3"/>
<contactref element="U$1" pad="G4-2"/>
<contactref element="U$1" pad="G4-1"/>
<contactref element="J1" pad="14"/>
</signal>
<signal name="G3">
<contactref element="U$1" pad="G3-3"/>
<contactref element="U$1" pad="G3-2"/>
<contactref element="U$1" pad="G3-1"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="G2">
<contactref element="U$1" pad="G2-3"/>
<contactref element="U$1" pad="G2-2"/>
<contactref element="U$1" pad="G2-1"/>
<contactref element="J1" pad="16"/>
</signal>
<signal name="G1">
<contactref element="U$1" pad="G1-3"/>
<contactref element="U$1" pad="G1-2"/>
<contactref element="U$1" pad="G1-1"/>
<contactref element="J1" pad="17"/>
</signal>
<signal name="3V3">
<contactref element="U$1" pad="3V3-3"/>
<contactref element="U$1" pad="3V3-2"/>
<contactref element="U$1" pad="3V3-1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="G46">
<contactref element="U$1" pad="G46-3"/>
<contactref element="U$1" pad="G46-2"/>
<contactref element="U$1" pad="G46-1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="G43">
<contactref element="U$1" pad="G43-2"/>
<contactref element="U$1" pad="G43-1"/>
<contactref element="U$1" pad="G43-3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="G42">
<contactref element="U$1" pad="G42-3"/>
<contactref element="U$1" pad="G42-2"/>
<contactref element="U$1" pad="G42-1"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="G44">
<contactref element="U$1" pad="G44-1"/>
<contactref element="U$1" pad="G44-3"/>
<contactref element="U$1" pad="G44-2"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="G41">
<contactref element="U$1" pad="G41-3"/>
<contactref element="U$1" pad="G41-2"/>
<contactref element="U$1" pad="G41-1"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="EN">
<contactref element="U$1" pad="EN-1"/>
<contactref element="U$1" pad="EN-3"/>
<contactref element="U$1" pad="EN-2"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="G40">
<contactref element="U$1" pad="G40-3"/>
<contactref element="U$1" pad="G40-2"/>
<contactref element="U$1" pad="G40-1"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="G0">
<contactref element="U$1" pad="G0-2"/>
<contactref element="U$1" pad="G0-1"/>
<contactref element="U$1" pad="G0-3"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="G39">
<contactref element="U$1" pad="G39-3"/>
<contactref element="U$1" pad="G39-2"/>
<contactref element="U$1" pad="G39-1"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND1-1"/>
<contactref element="U$1" pad="GND1-2"/>
<contactref element="U$1" pad="GND1-3"/>
<contactref element="J1" pad="7"/>
<contactref element="U$1" pad="GND2-1"/>
<contactref element="U$1" pad="GND2-3"/>
<contactref element="U$1" pad="GND2-2"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="5V-2"/>
<contactref element="U$1" pad="5V-3"/>
<contactref element="U$1" pad="5V-1"/>
<contactref element="J1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
