<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>ATTinier84
AVR ISP Shield</text>
<text>&gt;REVISION</text>
<text>&gt;REVISION</text>
<wire x1="29" y1="0" x2="2" y2="0" width="0" layer="20"/>
<wire x1="2" y1="0" x2="0" y2="2" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="2" x2="0" y2="27" width="0" layer="20"/>
<wire x1="0" y1="27" x2="2" y2="29" width="0" layer="20" curve="-90"/>
<wire x1="2" y1="29" x2="29" y2="29" width="0" layer="20"/>
<wire x1="29" y1="29" x2="31" y2="27" width="0" layer="20" curve="-90"/>
<wire x1="31" y1="27" x2="31" y2="2" width="0" layer="20"/>
<wire x1="31" y1="2" x2="29" y2="0" width="0" layer="20" curve="-90"/>
<text>ATTinier84
AVR ISP Shield</text>
<text>ATTinier84
AVR ISP Shield</text>
<text>&gt;REVISION</text>
<text>&gt;REVISION</text>
</plain>
<libraries>
<library name="A_butts">
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
<package name="DTS-6-SMALL-PADS">
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="ATTINIER84_SHIELD2">
</package>
<package name="CC-BY-SA-4.0-NO-URL">
</package>
<package name="COW_SMALL">
</package>
<package name="OSHWLOGO_BOT_0.2_A">
</package>
<package name="2X3-SHROUDED">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REVISION" value="v1.0"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="A_butts" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="VERSION" value=""/>
<attribute name="DESIGNER" value="Nobody"/>
</element>
<element name="C1" library="A_butts" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="A_butts" package="DTS-6-SMALL-PADS" value="SPST-NO-TACT6MM-PTH-SMALL-PADS">
<attribute name="NAME"/>
</element>
<element name="U1" library="A_butts" package="ATTINIER84_SHIELD2" value="ATTINIER84_SHIELD1551G"/>
<element name="U$1" library="A_butts" package="CC-BY-SA-4.0-NO-URL" value=""/>
<element name="U$2" library="A_butts" package="COW_SMALL" value=""/>
<element name="U$4" library="A_butts" package="OSHWLOGO_BOT_0.2_A" value=""/>
<element name="AVRISP" library="A_butts" package="2X3-SHROUDED" value="AVR_SPI_PRG_6PTH-SHROUD">
<attribute name="NAME"/>
</element>
<element name="U$3" library="A_butts" package="OSHWLOGO_BOT_0.2_A" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="RESET" pad="3"/>
<contactref element="U1" pad="GND@2"/>
<contactref element="U1" pad="GND@1"/>
<contactref element="AVRISP" pad="6"/>
<contactref element="RESET" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="VCC"/>
<contactref element="AVRISP" pad="2"/>
</signal>
<signal name="RST">
<contactref element="RESET" pad="1"/>
<contactref element="AVRISP" pad="5"/>
<contactref element="RESET" pad="2"/>
<contactref element="U1" pad="RST"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="PA6"/>
<contactref element="AVRISP" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="PA5"/>
<contactref element="AVRISP" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="PA4"/>
<contactref element="AVRISP" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
