<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>GND</text>
<text>5VDC</text>
<text>IR+</text>
<text>IR-</text>
<text>dhunter v0</text>
<text>ir 
stereo
remote</text>
<wire x1="3.81" y1="39.37" x2="5.08" y2="40.64" width="0" layer="20"/>
<wire x1="5.08" y1="40.64" x2="7.62" y2="40.64" width="0" layer="20"/>
<wire x1="7.62" y1="40.64" x2="8.89" y2="39.37" width="0" layer="20"/>
<wire x1="8.89" y1="39.37" x2="41.91" y2="39.37" width="0" layer="20"/>
<wire x1="41.91" y1="39.37" x2="43.18" y2="40.64" width="0" layer="20"/>
<wire x1="43.18" y1="40.64" x2="45.72" y2="40.64" width="0" layer="20"/>
<wire x1="45.72" y1="40.64" x2="46.99" y2="39.37" width="0" layer="20"/>
<wire x1="46.99" y1="39.37" x2="46.99" y2="36.83" width="0" layer="20"/>
<wire x1="46.99" y1="36.83" x2="45.72" y2="35.56" width="0" layer="20"/>
<wire x1="45.72" y1="35.56" x2="45.72" y2="8.89" width="0" layer="20"/>
<wire x1="45.72" y1="8.89" x2="46.99" y2="7.62" width="0" layer="20"/>
<wire x1="46.99" y1="7.62" x2="46.99" y2="5.08" width="0" layer="20"/>
<wire x1="46.99" y1="5.08" x2="45.72" y2="3.81" width="0" layer="20"/>
<wire x1="45.72" y1="3.81" x2="43.18" y2="3.81" width="0" layer="20"/>
<wire x1="43.18" y1="3.81" x2="41.91" y2="5.08" width="0" layer="20"/>
<wire x1="41.91" y1="5.08" x2="31.75" y2="5.08" width="0" layer="20"/>
<wire x1="31.75" y1="5.08" x2="29.21" y2="2.54" width="0" layer="20"/>
<wire x1="29.21" y1="2.54" x2="21.59" y2="2.54" width="0" layer="20"/>
<wire x1="21.59" y1="2.54" x2="19.05" y2="5.08" width="0" layer="20"/>
<wire x1="19.05" y1="5.08" x2="8.89" y2="5.08" width="0" layer="20"/>
<wire x1="8.89" y1="5.08" x2="7.62" y2="3.81" width="0" layer="20"/>
<wire x1="7.62" y1="3.81" x2="5.08" y2="3.81" width="0" layer="20"/>
<wire x1="5.08" y1="3.81" x2="3.81" y2="5.08" width="0" layer="20"/>
<wire x1="3.81" y1="5.08" x2="3.81" y2="7.62" width="0" layer="20"/>
<wire x1="3.81" y1="7.62" x2="5.08" y2="8.89" width="0" layer="20"/>
<wire x1="5.08" y1="8.89" x2="5.08" y2="21.59" width="0" layer="20"/>
<wire x1="5.08" y1="21.59" x2="3.81" y2="22.86" width="0" layer="20"/>
<wire x1="3.81" y1="22.86" x2="3.81" y2="31.75" width="0" layer="20"/>
<wire x1="3.81" y1="31.75" x2="5.08" y2="33.02" width="0" layer="20"/>
<wire x1="5.08" y1="33.02" x2="5.08" y2="35.56" width="0" layer="20"/>
<wire x1="5.08" y1="35.56" x2="3.81" y2="36.83" width="0" layer="20"/>
<wire x1="3.81" y1="36.83" x2="3.81" y2="39.37" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ROTARY_ENC_PLAIN">
<description>Simple rotary encoder, no LED, push center&lt;br&gt;
COM-09117</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL28-3">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
</packages>
</library>
<library name="LilyPad-Wearables">
<packages>
<package name="SIMPLE_HOLE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SW1" library="SparkFun-Electromechanical" package="ROTARY_ENC_PLAIN" value="ROTARTY_ENCODER"/>
<element name="U1" library="SparkFun-DigitalIC" package="DIL28-3" value="ATMEGA_328">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="100">
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49US" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="100uF">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="10k">
<attribute name="VALUE"/>
</element>
<element name="H1" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H2" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H3" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H4" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="R2" pad="P$2"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="SW1" pad="SW-"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="U1" pad="8"/>
<contactref element="SW1" pad="C"/>
<contactref element="H4" pad="P$1"/>
<contactref element="H3" pad="P$1"/>
<contactref element="H2" pad="P$1"/>
<contactref element="H1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="25"/>
<contactref element="SW1" pad="SW+"/>
</signal>
<signal name="ROTA">
<contactref element="U1" pad="26"/>
<contactref element="SW1" pad="A"/>
</signal>
<signal name="ROTB">
<contactref element="SW1" pad="B"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="10"/>
<contactref element="Y1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="9"/>
<contactref element="Y1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="15"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="1"/>
<contactref element="R2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
