<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="43.18" y2="0" width="0" layer="20"/>
<wire x1="43.18" y1="0" x2="43.18" y2="25.4" width="0" layer="20"/>
<wire x1="43.18" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<text> 2-LRCKT</text>
<text> 3-OCLK</text>
<text> 5-VSS</text>
<text> 6-VDD</text>
<text> 7-VSS</text>
<text> 8-VDD</text>
<text>NC</text>
<text>NC</text>
<text>10-PVDD</text>
<text>11-PVSS</text>
<text>12-FILT</text>
<text>13-XTO</text>
<text>15-XTI</text>
<text>19-VSS</text>
<text>21-VDD</text>
<text>22-!TESTEN</text>
<text>SCANEN-24</text>
<text>!RESET!-25</text>
<text>VSS-26</text>
<text>OUT_CLK-27</text>
<text>VDD-29</text>
<text>VSS-30</text>
<text>SDA-31</text>
<text>SCL-32</text>
<text>SDI-34</text>
<text>SCKR-36</text>
<text>BIT_EN-38</text>
<text>!SRC_INT!-40</text>
<text>SDO-42</text>
<text>SCKT-44</text>
<text>NC</text>
<text>NC</text>
<text> 1-GPIN7</text>
<text> 2-VL</text>
<text> 3-GND</text>
<text> 4-GPOUT0</text>
<text> 5-GPOUT1</text>
<text> 6-GPOUT2</text>
<text> 7-GPOUT3</text>
<text> 8-GPOUT4</text>
<text> 9-GPOUT5</text>
<text>10-GPOUT6</text>
<text>11-GPOUT7</text>
<text>12-!RES</text>
<text>13-SCLK</text>
<text>14-!SS</text>
<text>15-MISO</text>
<text>16-MOSI</text>
<text>17-GPX</text>
<text>18-INT</text>
<text>19-GND</text>
<text>20-D-</text>
<text>21-D+</text>
<text>22-VBCOMP</text>
<text>23-VCC</text>
<text>24-XI</text>
<text>25-XO</text>
<text>26-GPIN0</text>
<text>27-GPIN1</text>
<text>28-GPIN2</text>
<text>29-GPIN3</text>
<text>30-GPIN4</text>
<text>31-GPIN5</text>
<text>32-GPIN6</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X16">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-5MM">
</package>
</packages>
</library>
<library name="st-microelectronics">
<description>&lt;b&gt;ST Microelectronics Devices&lt;/b&gt;&lt;p&gt;
Microcontrollers,  I2C components, linear devices&lt;p&gt;
http://www.st.com&lt;p&gt;
&lt;i&gt;Include st-microelectronics-2.lbr, st-microelectronics-3.lbr.&lt;p&gt;&lt;/i&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP44">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X16" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X16" value=""/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-5MM" value="MAX3421E"/>
<element name="IC1" library="st-microelectronics" package="TQFP44" value="STA013TS">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value="STA013T$"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="57P0492"/>
</element>
</elements>
<signals>
<signal name="10">
<contactref element="J2" pad="10"/>
<contactref element="U1" pad="10"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="26">
<contactref element="U1" pad="26"/>
<contactref element="J1" pad="7"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="27">
<contactref element="U1" pad="27"/>
<contactref element="J1" pad="6"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="28">
<contactref element="U1" pad="28"/>
<contactref element="J1" pad="5"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="29">
<contactref element="U1" pad="29"/>
<contactref element="J1" pad="4"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="30">
<contactref element="U1" pad="30"/>
<contactref element="J1" pad="3"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="31">
<contactref element="U1" pad="31"/>
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="32">
<contactref element="U1" pad="32"/>
<contactref element="J1" pad="1"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="1">
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="4">
<contactref element="U1" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="6">
<contactref element="U1" pad="6"/>
<contactref element="J2" pad="6"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="7">
<contactref element="U1" pad="7"/>
<contactref element="J2" pad="7"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="8">
<contactref element="U1" pad="8"/>
<contactref element="J2" pad="8"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="9">
<contactref element="U1" pad="9"/>
<contactref element="J2" pad="9"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="11">
<contactref element="U1" pad="11"/>
<contactref element="J2" pad="11"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="23">
<contactref element="U1" pad="23"/>
<contactref element="J1" pad="10"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="2">
<contactref element="U1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="21">
<contactref element="U1" pad="21"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="20">
<contactref element="U1" pad="20"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="22">
<contactref element="U1" pad="22"/>
<contactref element="J1" pad="11"/>
<contactref element="IC1" pad="38"/>
</signal>
<signal name="25">
<contactref element="U1" pad="25"/>
<contactref element="J1" pad="8"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="24">
<contactref element="U1" pad="24"/>
<contactref element="J1" pad="9"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="18">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="15"/>
<contactref element="IC1" pad="42"/>
</signal>
<signal name="12">
<contactref element="U1" pad="12"/>
<contactref element="J2" pad="12"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="17">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="16"/>
<contactref element="IC1" pad="44"/>
</signal>
<signal name="16">
<contactref element="U1" pad="16"/>
<contactref element="J2" pad="16"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="15">
<contactref element="U1" pad="15"/>
<contactref element="J2" pad="15"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="13">
<contactref element="U1" pad="13"/>
<contactref element="J2" pad="13"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="14">
<contactref element="U1" pad="14"/>
<contactref element="J2" pad="14"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="3">
<contactref element="U1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="19">
<contactref element="U1" pad="19"/>
<contactref element="J1" pad="14"/>
<contactref element="IC1" pad="40"/>
</signal>
<signal name="5">
<contactref element="U1" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
