<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="45.7" y2="0" width="0" layer="20"/>
<wire x1="45.7" y1="0" x2="45.7" y2="60.63" width="0" layer="20"/>
<wire x1="45.7" y1="60.63" x2="0" y2="60.63" width="0" layer="20"/>
<wire x1="0" y1="60.63" x2="0" y2="0" width="0" layer="20"/>
<text>SPINE TAPE
   2024</text>
<text>DESIGNED BY
AARON ROSEN</text>
<text>G4</text>
<text>G5</text>
<text>microSD</text>
<text>VCC</text>
<text>(microUSB end)</text>
<text>VCC</text>
<text>VCC</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>7</text>
<text>6</text>
<text>5</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD-FEMALE">
<description>&lt;h3&gt;Header - 6 pin Female SMD&lt;/h3&gt;
Right angle 0.1"
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/19686.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="ABX00027">
<packages>
<package name="MODULE_ABX00027">
</package>
</packages>
</library>
<library name="ConnectorLib">
<packages>
<package name="PAD.03X.05">
<description>&lt;h3&gt;Electrically Conductive Pad 0.25" Circle&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.25" x 0.25"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="R-1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="AI-1223-TWT-3V-2-R">
<packages>
<package name="XDCR_AI-1223-TWT-3V-2-R">
</package>
</packages>
</library>
<library name="2024-01-22_03-34-57_Library">
<packages>
<package name="CONN_1989764_PXC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MICROSD_SMD" library="SparkFun-Connectors" package="1X06-SMD-FEMALE" value="">
<attribute name="PROD_ID" value="CONN-09668"/>
<attribute name="VALUE"/>
</element>
<element name="NANO_33_IOT" library="ABX00027" package="MODULE_ABX00027" value="ABX00027">
<attribute name="AVAILABILITY" value="Not in stock"/>
<attribute name="DESCRIPTION" value=" An IoT connected IMU sensor in the Nano form factor. "/>
<attribute name="MF" value="Arduino"/>
<attribute name="MP" value="Arduino Nano 33 IoT"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="TP1" library="ConnectorLib" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP2" library="ConnectorLib" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP3" library="ConnectorLib" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP4" library="ConnectorLib" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP5" library="ConnectorLib" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP6" library="ConnectorLib" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP7" library="ConnectorLib" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="R1" library="resistors" package="R-1206" value="10R(1206)">
<attribute name="MOUSER" value="660-RK73H2BTTD10R0F"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="resistors" package="R-1206" value="10R(1206)">
<attribute name="MOUSER" value="660-RK73H2BTTD10R0F"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="resistors" package="R-1206" value="10R(1206)">
<attribute name="MOUSER" value="660-RK73H2BTTD10R0F"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="resistors" package="R-1206" value="10R(1206)">
<attribute name="MOUSER" value="660-RK73H2BTTD10R0F"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="resistors" package="R-1206" value="10R(1206)">
<attribute name="MOUSER" value="660-RK73H2BTTD10R0F"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="resistors" package="R-1206" value="10R(1206)">
<attribute name="MOUSER" value="660-RK73H2BTTD10R0F"/>
<attribute name="NAME"/>
</element>
<element name="R_BUZZ" library="resistors" package="R-1206" value="10R(1206)">
<attribute name="MOUSER" value="660-RK73H2BTTD10R0F"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
<attribute name="VALUE"/>
</element>
<element name="LS1" library="AI-1223-TWT-3V-2-R" package="XDCR_AI-1223-TWT-3V-2-R" value="AI-1223-TWT-3V-2-R">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" AUDIO INDICATOR 82 DB 3 VDC 2300 HZ "/>
<attribute name="MF" value="PUI Audio,"/>
<attribute name="MP" value="AI-1223-TWT-3V-2-R"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/AI-1223-TWT-3V-2-R/?ref=eda"/>
</element>
<element name="J2" library="2024-01-22_03-34-57_Library" package="CONN_1989764_PXC" value="1989764CONN_1989764_PXC">
<attribute name="COPYRIGHT" value="Copyright (C) 2024 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1989764"/>
<attribute name="MFR_NAME" value="Phoenix Contact"/>
<attribute name="NAME"/>
</element>
<element name="J3" library="2024-01-22_03-34-57_Library" package="CONN_1989764_PXC" value="1989764CONN_1989764_PXC">
<attribute name="COPYRIGHT" value="Copyright (C) 2024 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1989764"/>
<attribute name="MFR_NAME" value="Phoenix Contact"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="COM1">
<contactref element="NANO_33_IOT" pad="5"/>
<contactref element="TP1" pad="P$1"/>
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="COM2">
<contactref element="NANO_33_IOT" pad="6"/>
<contactref element="TP2" pad="P$1"/>
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="COM3">
<contactref element="NANO_33_IOT" pad="7"/>
<contactref element="TP3" pad="P$1"/>
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="COM5">
<contactref element="TP4" pad="P$1"/>
<contactref element="R4" pad="2"/>
<contactref element="NANO_33_IOT" pad="4"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="COM6">
<contactref element="NANO_33_IOT" pad="10"/>
<contactref element="TP5" pad="P$1"/>
<contactref element="R5" pad="2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="COM7">
<contactref element="NANO_33_IOT" pad="11"/>
<contactref element="TP6" pad="P$1"/>
<contactref element="R6" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="NANO_33_IOT" pad="14"/>
<contactref element="NANO_33_IOT" pad="19"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="MICROSD_SMD" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="LS1" pad="N"/>
</signal>
<signal name="N$7">
<contactref element="NANO_33_IOT" pad="25"/>
<contactref element="R_BUZZ" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="MICROSD_SMD" pad="2"/>
<contactref element="NANO_33_IOT" pad="2"/>
<contactref element="TP7" pad="P$1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="MICROSD_SMD" pad="3"/>
<contactref element="NANO_33_IOT" pad="30"/>
</signal>
<signal name="MOSI">
<contactref element="MICROSD_SMD" pad="4"/>
<contactref element="NANO_33_IOT" pad="29"/>
</signal>
<signal name="SCK">
<contactref element="MICROSD_SMD" pad="5"/>
<contactref element="NANO_33_IOT" pad="1"/>
</signal>
<signal name="CS">
<contactref element="MICROSD_SMD" pad="6"/>
<contactref element="NANO_33_IOT" pad="28"/>
</signal>
<signal name="VUSB">
<contactref element="NANO_33_IOT" pad="12"/>
</signal>
<signal name="N$2">
<contactref element="NANO_33_IOT" pad="15"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R_BUZZ" pad="2"/>
<contactref element="LS1" pad="P"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
