<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.78" y2="0" width="0" layer="20"/>
<wire x1="17.78" y1="0" x2="17.78" y2="10.16" width="0" layer="20"/>
<wire x1="17.78" y1="10.16" x2="0" y2="10.15" width="0" layer="20"/>
<wire x1="0" y1="10.15" x2="0" y2="0" width="0" layer="20"/>
<text>DFN12-BOB</text>
<text>PUGBUTT.COM</text>
</plain>
<libraries>
<library name="LinearTechnology">
<packages>
<package name="DFN12-DD-3X3">
</package>
</packages>
</library>
<library name="ThruHole">
<packages>
<package name="PINHEAD_1X7">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="LinearTechnology" package="DFN12-DD-3X3" value="LT3652_DFN"/>
<element name="J1" library="ThruHole" package="PINHEAD_1X7" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="ThruHole" package="PINHEAD_1X7" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VFB">
<contactref element="IC1" pad="7"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="NTC">
<contactref element="IC1" pad="8"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="BAT">
<contactref element="IC1" pad="9"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="BOOST">
<contactref element="IC1" pad="11"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="SW">
<contactref element="IC1" pad="12"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="TIMER">
<contactref element="IC1" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="/FAULT">
<contactref element="IC1" pad="5"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="/CHRG">
<contactref element="IC1" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="/SHDN">
<contactref element="IC1" pad="3"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="VINREG">
<contactref element="IC1" pad="2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="VIN">
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="7"/>
</signal>
<signal name="SENSE">
<contactref element="IC1" pad="10"/>
<contactref element="J2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
