<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="36" width="0.4064" layer="20"/>
<wire x1="0" y1="36" x2="38.4" y2="36" width="0.4064" layer="20"/>
<wire x1="38.4" y1="36" x2="38.4" y2="0" width="0.4064" layer="20"/>
<wire x1="38.4" y1="0" x2="0" y2="0" width="0.4064" layer="20"/>
<text>electricityforprogress 2015</text>
<text>electricityforprogress 2015</text>
<text>RGB Timer</text>
<hole x="35" y="21" drill="2.8"/>
<hole x="3" y="21" drill="2.8"/>
<text>VCC</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>TX</text>
<text>RX</text>
<text>10-pwm</text>
<text>RGB Timer</text>
<text>V+</text>
<text>GND</text>
<text>V+</text>
<text>GND</text>
<text>A0</text>
<text>V</text>
<text>GND</text>
<text>GND</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X03-CLEANBIG">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL28-3">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rgb_encoder">
<packages>
<package name="RGB_ENCODER">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.0 mm, square</description>
</package>
<package name="3,0-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.0 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CTZ3">
<description>CTZ3 Series land pattern for variable capacitor - CTZ3E-50C-W1-PF</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="DIL28-3" value="ATMEGA328P_PDIP">
<attribute name="VALUE"/>
</element>
<element name="ICSP" library="SparkFun-Connectors" package="2X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ASSORTED" library="pinhead" package="1X10" value="">
<attribute name="VALUE"/>
</element>
<element name="CHIME" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="rgb_encoder" package="RGB_ENCODER" value="RGB_ENCODER"/>
<element name="H1" library="holes" package="3,0-PAD-SQUARE" value="MOUNT-PAD-SQUARE3.0"/>
<element name="H2" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="C1" library="SparkFun-Passives" package="CTZ3" value="0.1uf"/>
<element name="R1" library="adafruit" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="8"/>
<contactref element="ICSP" pad="6"/>
<contactref element="CHIME" pad="3"/>
<contactref element="H1" pad="B3,0"/>
<contactref element="ASSORTED" pad="10"/>
<contactref element="C1" pad="-"/>
<contactref element="U$1" pad="C"/>
</signal>
<signal name="RED">
<contactref element="U1" pad="15"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="BLUE">
<contactref element="U1" pad="11"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="GREEN">
<contactref element="U1" pad="12"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="20"/>
<contactref element="ICSP" pad="2"/>
<contactref element="CHIME" pad="1"/>
<contactref element="H2" pad="B3,0"/>
<contactref element="C1" pad="+"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="KNOB">
<contactref element="ASSORTED" pad="8"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="3"/>
<contactref element="ASSORTED" pad="2"/>
</signal>
<signal name="RX">
<contactref element="ASSORTED" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="ICSP" pad="1"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="SCK">
<contactref element="ICSP" pad="3"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="RESET">
<contactref element="ICSP" pad="5"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="ICSP" pad="4"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$4">
</signal>
<signal name="10-PWM">
<contactref element="U1" pad="16"/>
<contactref element="ASSORTED" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="ASSORTED" pad="3"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="N$3">
<contactref element="ASSORTED" pad="4"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="N$5">
<contactref element="ASSORTED" pad="5"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="N$6">
<contactref element="ASSORTED" pad="6"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$7">
<contactref element="ASSORTED" pad="7"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="A">
<contactref element="U1" pad="4"/>
<contactref element="U$1" pad="A"/>
</signal>
<signal name="B">
<contactref element="U$1" pad="B"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="SPEAKER">
<contactref element="CHIME" pad="2"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="SWITCH">
<contactref element="U1" pad="13"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
