<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="14.224" y1="13.716" x2="1.27" y2="13.716" width="0" layer="20"/>
<wire x1="1.27" y1="13.716" x2="0" y2="12.446" width="0" layer="20" curve="90"/>
<wire x1="0" y1="12.446" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="14.224" y2="0" width="0" layer="20"/>
<wire x1="14.224" y1="0" x2="15.494" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="15.494" y1="1.27" x2="15.494" y2="12.446" width="0" layer="20"/>
<wire x1="15.494" y1="12.446" x2="14.224" y2="13.716" width="0" layer="20" curve="90"/>
<text>VCC</text>
<text>SDA</text>
<text>SCL</text>
<text>INT</text>
<text>GND</text>
<text>Si1141 Breakout Board
Cirkyt Inc.</text>
</plain>
<libraries>
<library name="silabs-si1411">
<packages>
<package name="QFN10">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA05-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="silabs-si1411" package="QFN10" value="SI1141">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="696-SMLFM0603SRCTR">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="30 Ohm">
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08390"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="15uF">
<attribute name="PROD_ID" value="CAP-08390"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-lstb" package="MA05-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="1"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="2"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="INT">
<contactref element="U1" pad="4"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
