<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="177.8" y2="0" width="1.5748" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="87.63" width="1.5748" layer="20"/>
<wire x1="0" y1="87.63" x2="177.8" y2="87.63" width="1.5748" layer="20"/>
<wire x1="177.8" y1="0" x2="177.8" y2="87.63" width="1.5748" layer="20"/>
<text>CH1</text>
<text>CH2</text>
<text>CH3</text>
<text>CH4</text>
<text>CH5</text>
<text>CH6</text>
<text>CH7</text>
<text>CH8</text>
<text>Serial Data</text>
<text>CH1</text>
<text>CH2</text>
<text>CH3</text>
<text>CH4</text>
<text>CH5</text>
<text>CH6</text>
<text>CH7</text>
<text>CH8</text>
<text>Serial Data Output</text>
<text>Serial</text>
<text>CLK In</text>
<text>Out 1</text>
<text>Out 2</text>
<text>Out 3</text>
<text>Serial Clk</text>
<text>+5v</text>
<text>Com</text>
<text>Power In</text>
<text>Fiber Optic I/O - 8 Channel</text>
<text>Revision 2</text>
<text>3/18/16</text>
<text>RX1</text>
<text>TX1</text>
<text>RX2</text>
<text>TX2</text>
<text>RX3</text>
<text>TX3</text>
<text>RX4</text>
<text>TX4</text>
<text>RX5</text>
<text>TX5</text>
<text>RX6</text>
<text>TX6</text>
<text>RX7</text>
<text>TX7</text>
<text>RX8</text>
<text>TX8</text>
</plain>
<libraries>
<library name="ap_opto">
<description>Opto-electronics</description>
<packages>
<package name="HFBR_HORZ">
<description>HFBR Horizontal Package</description>
</package>
<package name="DIP20">
<description>DIP20, 20 Pin Dual Inline Package</description>
</package>
</packages>
</library>
<library name="ap_ti">
<description>Texas Instruments ICs</description>
<packages>
<package name="DIP08">
<description>DIP08, 8 Pin Dual Inline Package</description>
</package>
<package name="DIP20">
<description>DIP20, 20 Pin Dual Inline Package</description>
</package>
</packages>
</library>
<library name="ap_capacitor_thru">
<description>Through-Hole Capacitors</description>
<packages>
<package name="10UF_TANT_0.2">
</package>
<package name="C100">
<description>Capacitor, 0.1 inch Spacing, Through-Hole</description>
</package>
<package name="C400">
<description>Capacitor, 0.4 inch Spacing, Through-Hole</description>
</package>
<package name="POLAR_0.35DIA_0.2LEAD">
</package>
<package name="47UF_TANTALUM">
<description>47uF Tantalum Capacitor</description>
</package>
<package name="C200">
<description>Capacitor, 0.2 inch Spacing, Through-Hole</description>
</package>
</packages>
</library>
<library name="ap_resistor_thru">
<description>Through-Hole Resistors</description>
<packages>
<package name="R400">
<description>Resistor, 0.4 inch Spacing, Through Hole</description>
</package>
<package name="SIP9">
</package>
</packages>
</library>
<library name="ap_conn_Phoenix">
<description>Phoneix Connectors</description>
<packages>
<package name="1777138_8PIN">
<description>Header, 8 Position, 12A, Screw Down</description>
</package>
<package name="1777219_16PIN">
</package>
<package name="1777073_2PIN">
<description>Header, 2 Position, 12A, Screw Down</description>
</package>
</packages>
</library>
<library name="ap_inductor">
<description>Inductors and Ferrite Beads</description>
<packages>
<package name="RCR875">
<description>Sumida RCR875 Inductor, Radial Leaded, Shielded</description>
</package>
</packages>
</library>
<library name="ap_misc">
<packages>
<package name="ISO_MOUNT">
<description>Isolated Mounting Hole, 0.125" Hole</description>
</package>
<package name="MAGLAB_SYMBOL_1/2">
<description>Maglab Logo 0.625" Width</description>
</package>
</packages>
</library>
<library name="ap_jumpers">
<description>Jumpers, Solder and Pin</description>
<packages>
<package name="JMP400">
<description>Jumper. 0.4" Spacing</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TX1" library="ap_opto" package="HFBR_HORZ" value="HFBR-1521Z">
<attribute name="VENDOR_PART#" value="71K0263"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-1521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX1" library="ap_opto" package="HFBR_HORZ" value="HFBR-2521Z">
<attribute name="VENDOR_PART#" value="71K0280"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-2521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="ap_ti" package="DIP08" value="">
<attribute name="VENDOR_PART#" value="60K6936"/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value="SN75452B"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ap_resistor_thru" package="R400" value="66.5">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="POWER" value=""/>
<attribute name="TC" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="ap_capacitor_thru" package="C100" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX2" library="ap_opto" package="HFBR_HORZ" value="HFBR-1521Z">
<attribute name="VENDOR_PART#" value="71K0263"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-1521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX2" library="ap_opto" package="HFBR_HORZ" value="HFBR-2521Z">
<attribute name="VENDOR_PART#" value="71K0280"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-2521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="ap_resistor_thru" package="R400" value="66.5">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="POWER" value=""/>
<attribute name="TC" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="ap_capacitor_thru" package="C100" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX3" library="ap_opto" package="HFBR_HORZ" value="HFBR-1521Z">
<attribute name="VENDOR_PART#" value="71K0263"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-1521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX3" library="ap_opto" package="HFBR_HORZ" value="HFBR-2521Z">
<attribute name="VENDOR_PART#" value="71K0280"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-2521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="ap_ti" package="DIP08" value="">
<attribute name="VENDOR_PART#" value="60K6936"/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value="SN75452B"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="ap_resistor_thru" package="R400" value="66.5">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="POWER" value=""/>
<attribute name="TC" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="ap_capacitor_thru" package="C100" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX4" library="ap_opto" package="HFBR_HORZ" value="HFBR-1521Z">
<attribute name="VENDOR_PART#" value="71K0263"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-1521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX4" library="ap_opto" package="HFBR_HORZ" value="HFBR-2521Z">
<attribute name="VENDOR_PART#" value="71K0280"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-2521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="ap_resistor_thru" package="R400" value="66.5">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="POWER" value=""/>
<attribute name="TC" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="ap_capacitor_thru" package="C100" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX5" library="ap_opto" package="HFBR_HORZ" value="HFBR-1521Z">
<attribute name="VENDOR_PART#" value="71K0263"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-1521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX5" library="ap_opto" package="HFBR_HORZ" value="HFBR-2521Z">
<attribute name="VENDOR_PART#" value="71K0280"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-2521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="ap_ti" package="DIP08" value="">
<attribute name="VENDOR_PART#" value="60K6936"/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value="SN75452B"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="ap_resistor_thru" package="R400" value="66.5">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="POWER" value=""/>
<attribute name="TC" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="ap_capacitor_thru" package="C100" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX6" library="ap_opto" package="HFBR_HORZ" value="HFBR-1521Z">
<attribute name="VENDOR_PART#" value="71K0263"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-1521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX6" library="ap_opto" package="HFBR_HORZ" value="HFBR-2521Z">
<attribute name="VENDOR_PART#" value="71K0280"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-2521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="ap_resistor_thru" package="R400" value="66.5">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="POWER" value=""/>
<attribute name="TC" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="ap_capacitor_thru" package="C100" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX7" library="ap_opto" package="HFBR_HORZ" value="HFBR-1521Z">
<attribute name="VENDOR_PART#" value="71K0263"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-1521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX7" library="ap_opto" package="HFBR_HORZ" value="HFBR-2521Z">
<attribute name="VENDOR_PART#" value="71K0280"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-2521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="ap_ti" package="DIP08" value="">
<attribute name="VENDOR_PART#" value="60K6936"/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value="SN75452B"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="ap_resistor_thru" package="R400" value="66.5">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="POWER" value=""/>
<attribute name="TC" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="ap_capacitor_thru" package="C100" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX8" library="ap_opto" package="HFBR_HORZ" value="HFBR-1521Z">
<attribute name="VENDOR_PART#" value="71K0263"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-1521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX8" library="ap_opto" package="HFBR_HORZ" value="HFBR-2521Z">
<attribute name="VENDOR_PART#" value="71K0280"/>
<attribute name="SERIES" value="Horizontal"/>
<attribute name="PART_NUMBER" value="HFBR-2521Z"/>
<attribute name="MANUFACTURER" value="Avago"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="ap_resistor_thru" package="R400" value="66.5">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="POWER" value=""/>
<attribute name="TC" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="ap_capacitor_thru" package="C100" value="0.1uF">
<attribute name="VENDOR_PART#" value="12M6471"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="P20"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="P20R104K5-F"/>
<attribute name="MANUFACTURER" value="Cornell Dubilier"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="ap_ti" package="DIP20" value="">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="ap_conn_Phoenix" package="1777138_8PIN" value="">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="ap_ti" package="DIP20" value="">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="ap_ti" package="DIP20" value="">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="ap_capacitor_thru" package="10UF_TANT_0.2" value="10uF">
<attribute name="VENDOR_PART#" value="57K9411"/>
<attribute name="SERIES" value="Tatalum"/>
<attribute name="PART_NUMBER" value="T356G106K035AT"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="Newark"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="ap_conn_Phoenix" package="1777219_16PIN" value="1777219">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="ap_resistor_thru" package="SIP9" value="330">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="ap_opto" package="DIP20" value="">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="ap_conn_Phoenix" package="1777073_2PIN" value="1777073">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="ap_inductor" package="RCR875" value="22uF">
<attribute name="VENDOR_PART#" value="851-RCR875DNP-220L"/>
<attribute name="SERIES" value="Shielded"/>
<attribute name="PART_NUMBER" value="RCR875DNP-220L"/>
<attribute name="MANUFACTURER" value="Sumida"/>
<attribute name="VENDOR" value="Mouser"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="ap_capacitor_thru" package="POLAR_0.35DIA_0.2LEAD" value="100uF">
<attribute name="VENDOR_PART#" value="1189-1887-ND"/>
<attribute name="SERIES" value="Electrolytic"/>
<attribute name="PART_NUMBER" value="100ZLH100MEFC10X20"/>
<attribute name="PACKAGE" value="Through Hole"/>
<attribute name="MANUFACTURER" value="Rubycon"/>
<attribute name="VENDOR" value="DigiKey"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="ap_capacitor_thru" package="47UF_TANTALUM" value="47uF">
<attribute name="VOLTAGE" value="10v"/>
<attribute name="VENDOR_PART#" value="478-6063-ND"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="TAP"/>
<attribute name="PART_NUMBER" value="TAP107K010CCS"/>
<attribute name="MANUFACTURER" value="AVX"/>
<attribute name="VENDOR" value="DigiKey"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="ap_capacitor_thru" package="C200" value="1uF">
<attribute name="VENDOR_PART#" value="445-8517-ND"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="FK"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="FK24X7R1H105K"/>
<attribute name="MANUFACTURER" value="TDK"/>
<attribute name="VENDOR" value="DigiKey"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="ap_capacitor_thru" package="C400" value="0.1uF">
<attribute name="VENDOR_PART#" value="399-4491-1-ND"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="SERIES" value="400"/>
<attribute name="TYPE" value="Ceramic"/>
<attribute name="TC" value="X7R"/>
<attribute name="PART_NUMBER" value="C420C104K5R5TA7200"/>
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="VENDOR" value="DigiKey"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$75" library="ap_misc" package="ISO_MOUNT" value=""/>
<element name="U$76" library="ap_misc" package="ISO_MOUNT" value=""/>
<element name="U$77" library="ap_misc" package="ISO_MOUNT" value=""/>
<element name="U$78" library="ap_misc" package="ISO_MOUNT" value=""/>
<element name="U$79" library="ap_misc" package="MAGLAB_SYMBOL_1/2" value=""/>
<element name="JMP1" library="ap_jumpers" package="JMP400" value="">
<attribute name="VENDOR_PART#" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="VENDOR" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="P$2"/>
<contactref element="C3" pad="2"/>
<contactref element="TX1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="RX1" pad="2"/>
<contactref element="C10" pad="P$2"/>
<contactref element="C12" pad="2"/>
<contactref element="TX2" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="RX2" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="C5" pad="P$2"/>
<contactref element="C6" pad="2"/>
<contactref element="TX3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="RX3" pad="2"/>
<contactref element="C11" pad="P$2"/>
<contactref element="C13" pad="2"/>
<contactref element="TX4" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="RX4" pad="2"/>
<contactref element="U4" pad="4"/>
<contactref element="C20" pad="P$2"/>
<contactref element="C24" pad="2"/>
<contactref element="TX5" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="RX5" pad="2"/>
<contactref element="C30" pad="P$2"/>
<contactref element="C31" pad="2"/>
<contactref element="TX6" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="RX6" pad="2"/>
<contactref element="U5" pad="4"/>
<contactref element="C21" pad="P$2"/>
<contactref element="C26" pad="2"/>
<contactref element="TX7" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="RX7" pad="2"/>
<contactref element="C32" pad="P$2"/>
<contactref element="C33" pad="2"/>
<contactref element="TX8" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="RX8" pad="2"/>
<contactref element="C9" pad="P$2"/>
<contactref element="U3" pad="10"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="8"/>
<contactref element="C29" pad="P$2"/>
<contactref element="C22" pad="P$2"/>
<contactref element="U6" pad="10"/>
<contactref element="U7" pad="10"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="16"/>
<contactref element="J3" pad="4"/>
<contactref element="J3" pad="6"/>
<contactref element="J3" pad="8"/>
<contactref element="J3" pad="10"/>
<contactref element="J3" pad="12"/>
<contactref element="J3" pad="14"/>
<contactref element="R9" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="P$2"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="JMP1" pad="P$1"/>
<contactref element="JMP1" pad="P$2"/>
</signal>
<signal name="+5V">
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="P$1"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="1"/>
<contactref element="RX1" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C10" pad="P$1"/>
<contactref element="R3" pad="2"/>
<contactref element="RX2" pad="3"/>
<contactref element="C14" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="P$1"/>
<contactref element="R2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="1"/>
<contactref element="RX3" pad="3"/>
<contactref element="C8" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C11" pad="P$1"/>
<contactref element="R4" pad="2"/>
<contactref element="RX4" pad="3"/>
<contactref element="C15" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C20" pad="P$1"/>
<contactref element="R5" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="6"/>
<contactref element="U4" pad="1"/>
<contactref element="RX5" pad="3"/>
<contactref element="C27" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C30" pad="P$1"/>
<contactref element="R7" pad="2"/>
<contactref element="RX6" pad="3"/>
<contactref element="C34" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C21" pad="P$1"/>
<contactref element="R6" pad="2"/>
<contactref element="C25" pad="1"/>
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="1"/>
<contactref element="RX7" pad="3"/>
<contactref element="C28" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C32" pad="P$1"/>
<contactref element="R8" pad="2"/>
<contactref element="RX8" pad="3"/>
<contactref element="C35" pad="1"/>
<contactref element="U3" pad="20"/>
<contactref element="C9" pad="P$1"/>
<contactref element="U3" pad="19"/>
<contactref element="U3" pad="1"/>
<contactref element="C29" pad="P$1"/>
<contactref element="C22" pad="P$1"/>
<contactref element="U7" pad="20"/>
<contactref element="U7" pad="1"/>
<contactref element="U7" pad="19"/>
<contactref element="U6" pad="20"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="19"/>
<contactref element="L1" pad="P$2"/>
<contactref element="C17" pad="P$1"/>
<contactref element="C18" pad="1"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="TX1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="RX1" pad="1"/>
<contactref element="RX1" pad="4"/>
<contactref element="U6" pad="9"/>
<contactref element="U7" pad="9"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="5"/>
<contactref element="TX2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="TX3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="RX4" pad="1"/>
<contactref element="RX4" pad="4"/>
<contactref element="U6" pad="6"/>
<contactref element="U7" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="5"/>
<contactref element="TX4" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="TX5" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="U4" pad="5"/>
<contactref element="TX6" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="TX7" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="U5" pad="5"/>
<contactref element="TX8" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="9"/>
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="18"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U3" pad="17"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="U3" pad="16"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="U3" pad="15"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="2"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="N$23">
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="N$24">
<contactref element="U3" pad="12"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="N$25">
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="2"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="N$26">
<contactref element="LED1" pad="13"/>
<contactref element="R9" pad="9"/>
</signal>
<signal name="N$27">
<contactref element="LED1" pad="14"/>
<contactref element="R9" pad="8"/>
</signal>
<signal name="N$28">
<contactref element="LED1" pad="15"/>
<contactref element="R9" pad="7"/>
</signal>
<signal name="N$29">
<contactref element="LED1" pad="16"/>
<contactref element="R9" pad="6"/>
</signal>
<signal name="N$30">
<contactref element="LED1" pad="17"/>
<contactref element="R9" pad="5"/>
</signal>
<signal name="N$31">
<contactref element="LED1" pad="18"/>
<contactref element="R9" pad="4"/>
</signal>
<signal name="N$32">
<contactref element="LED1" pad="19"/>
<contactref element="R9" pad="3"/>
</signal>
<signal name="N$33">
<contactref element="LED1" pad="20"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="LED1" pad="1"/>
<contactref element="U7" pad="18"/>
</signal>
<signal name="N$43">
<contactref element="LED1" pad="2"/>
<contactref element="U7" pad="17"/>
</signal>
<signal name="N$44">
<contactref element="LED1" pad="3"/>
<contactref element="U7" pad="16"/>
</signal>
<signal name="N$45">
<contactref element="LED1" pad="4"/>
<contactref element="U7" pad="15"/>
</signal>
<signal name="N$46">
<contactref element="LED1" pad="5"/>
<contactref element="U7" pad="14"/>
</signal>
<signal name="N$47">
<contactref element="LED1" pad="6"/>
<contactref element="U7" pad="13"/>
</signal>
<signal name="N$48">
<contactref element="LED1" pad="7"/>
<contactref element="U7" pad="12"/>
</signal>
<signal name="N$49">
<contactref element="LED1" pad="8"/>
<contactref element="U7" pad="11"/>
</signal>
<signal name="N$54">
<contactref element="U6" pad="2"/>
<contactref element="RX8" pad="1"/>
<contactref element="RX8" pad="4"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="RX3" pad="1"/>
<contactref element="RX3" pad="4"/>
<contactref element="U6" pad="7"/>
<contactref element="U7" pad="7"/>
</signal>
<signal name="N$51">
<contactref element="RX2" pad="1"/>
<contactref element="RX2" pad="4"/>
<contactref element="U6" pad="8"/>
<contactref element="U7" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="U6" pad="4"/>
<contactref element="RX6" pad="1"/>
<contactref element="RX6" pad="4"/>
<contactref element="U7" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U6" pad="5"/>
<contactref element="RX5" pad="1"/>
<contactref element="RX5" pad="4"/>
<contactref element="U7" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="U6" pad="3"/>
<contactref element="RX7" pad="1"/>
<contactref element="RX7" pad="4"/>
<contactref element="U7" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="U6" pad="11"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="J3" pad="3"/>
<contactref element="U6" pad="12"/>
</signal>
<signal name="N$15">
<contactref element="U6" pad="13"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="N$34">
<contactref element="U6" pad="14"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="N$36">
<contactref element="U6" pad="15"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="N$37">
<contactref element="U6" pad="16"/>
<contactref element="J3" pad="11"/>
</signal>
<signal name="N$38">
<contactref element="U6" pad="17"/>
<contactref element="J3" pad="13"/>
</signal>
<signal name="N$39">
<contactref element="U6" pad="18"/>
<contactref element="J3" pad="15"/>
</signal>
<signal name="N$40">
<contactref element="L1" pad="P$1"/>
<contactref element="C16" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
