<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<text>M1</text>
<text>M0</text>
<text>M3</text>
<text>M2</text>
<text>+</text>
<text>-</text>
<text>ZER0</text>
<text>alienwhoop</text>
<text>F0</text>
<text>M3</text>
<text>M1</text>
<text>M2</text>
<text>M0</text>
<text>ZER0</text>
<text>alienwhoop.us</text>
<text>g20180815A</text>
<text>LICENSED UNDER
CC BY SA 4.0 INTL</text>
<wire x1="6.19125" y1="-0.15875" x2="0" y2="6.35" width="0.1524" layer="20" curve="-105.359338"/>
<wire x1="-0.15875" y1="22.70125" x2="0" y2="6.35" width="0.1524" layer="20" curve="-128.21614"/>
<wire x1="-0.15875" y1="22.70125" x2="6.35" y2="29.05125" width="0.1524" layer="20" curve="-106.947683"/>
<wire x1="22.70125" y1="29.05125" x2="6.35" y2="29.05125" width="0.1524" layer="20" curve="-128.212706"/>
<wire x1="22.70125" y1="29.05125" x2="29.05125" y2="22.70125" width="0.1524" layer="20" curve="-106.260205"/>
<wire x1="29.05125" y1="6.35" x2="29.05125" y2="22.70125" width="0.1524" layer="20" curve="-128.212706"/>
<wire x1="29.05125" y1="6.35" x2="22.70125" y2="-0.15875" width="0.1524" layer="20" curve="-106.947683"/>
<wire x1="6.19125" y1="-0.15875" x2="22.70125" y2="-0.15875" width="0.1524" layer="20" curve="-131.361383"/>
<text>GND</text>
<text>CLK</text>
<text>DAT</text>
<text>M2</text>
<text>M3</text>
<text>M0</text>
<text>M1</text>
<text>0</text>
<text>0</text>
<text>5V</text>
<text>3V3</text>
<text>GND</text>
<text>RX1</text>
<text>TX1</text>
<text>K</text>
<text>SPI</text>
<text>DIY MIX</text>
<text>DIY MIX</text>
</plain>
<libraries>
<library name="micro-stm_v2">
<description>&lt;b&gt;ARM 32-bit Cortex™ MCUs&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by jb@jenszuhause.de&lt;/author&gt;&lt;p&gt;
&lt;b&gt;You are using this libary by your own risk.&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Make sure to check everything well due to this libary before using it.&lt;/b&gt;</description>
<packages>
<package name="TSSOP20-I">
<description>&lt;b&gt;TSSOP20-I&lt;/b&gt;&lt;p&gt;
20-pin thin shrink small outline package</description>
</package>
</packages>
</library>
<library name="AlienWhoop">
<packages>
<package name="53047-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
<package name="DFE201612E-INDUCTOR">
<description>Fixed Inductors 0806 2.2uH 20% 2.4A RDC=0.116ohms</description>
</package>
<package name="TPS6306X">
</package>
<package name="TESTPAD">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="SOT-23">
<description>SOT23</description>
</package>
<package name="FE03-1">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Perfect_0402">
<packages>
<package name="0402">
<description>0402 (1005 Metric)  

Nick Garner - TeleSense</description>
</package>
</packages>
</library>
<library name="alienflight">
<packages>
<package name="MICROFET-2X2">
<description>MICROFET-2x2&lt;hr&gt;
&lt;a href="https://www.fairchildsemi.com/datasheets/FD/FDMA410NZ.pdf"&gt;View Datasheet&lt;/a&gt;</description>
</package>
<package name="S2B-PH-K-S">
<description>Battery Connector&lt;br&gt;
JST PH S2B-PH-K-S&lt;hr&gt;
&lt;a href="http://www.jst-mfg.com/product/pdf/eng/ePH.pdf"&gt;View Datasheet&lt;/a&gt;</description>
</package>
<package name="YUDEN-CAP-0805">
<description>Yuden Capacitor</description>
</package>
<package name="SMD-CHIP-LED-0805">
<description>SMD CHIP LED - APHCM2012QBC/D-F01 &lt;hr&gt;
&lt;br&gt;
&lt;a href="https://www.kingbrightusa.com/images/catalog/spec/APHCM2012QBC-D-F01.pdf"&gt;View Datasheet&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="alienflight">
<packages>
<package name="YUDEN-CAP-0805">
<description>Yuden Capacitor</description>
</package>
</packages>
</library>
<library name="Sparkfun">
<packages>
<package name="QFN24_PAD">
<description>SparkFun IMU Breakout - MPU-9250; https://github.com/sparkfun/MPU-9250_Breakout; https://www.sparkfun.com/products/13762; Built for the MPU-9250 using guidelines found in http://cds.linear.com/docs/en/packaging/Carsem%20MLP%20users%20guide.pdf</description>
</package>
</packages>
</library>
<library name="holes">
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="micro-stm_v2" package="TSSOP20-I" value="STM32F030F4P">
<attribute name="PARTNO" value="STM32F030F4P6TR"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="Perfect_0402" package="0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GCM155R71C104KA55D"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Perfect_0402" package="0402" value="1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GRM155C71A105KE11D"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Perfect_0402" package="0402" value="10nF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GCM155R71H103KA55D"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Perfect_0402" package="0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GCM155R71C104KA55D"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Perfect_0402" package="0402" value="10K">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RC0402FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Perfect_0402" package="0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GCM155R71C104KA55D"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="alienflight" package="MICROFET-2X2" value="FDMA410NZ">
<attribute name="MF" value="Fairchild"/>
<attribute name="MPN" value="FDMA410NZ"/>
</element>
<element name="Q2" library="alienflight" package="MICROFET-2X2" value="FDMA410NZ">
<attribute name="MF" value="Fairchild"/>
<attribute name="MPN" value="FDMA410NZ"/>
</element>
<element name="Q0" library="alienflight" package="MICROFET-2X2" value="FDMA410NZ">
<attribute name="MF" value="Fairchild"/>
<attribute name="MPN" value="FDMA410NZ"/>
</element>
<element name="Q3" library="alienflight" package="MICROFET-2X2" value="FDMA410NZ">
<attribute name="MF" value="Fairchild"/>
<attribute name="MPN" value="FDMA410NZ"/>
</element>
<element name="M1" library="AlienWhoop" package="53047-02" value="53047-02">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="OC_NEWARK" value="57H4701"/>
</element>
<element name="M2" library="AlienWhoop" package="53047-02" value="53047-02">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="OC_NEWARK" value="57H4701"/>
</element>
<element name="M0" library="AlienWhoop" package="53047-02" value="53047-02">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="OC_NEWARK" value="57H4701"/>
</element>
<element name="M3" library="AlienWhoop" package="53047-02" value="53047-02">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="OC_NEWARK" value="57H4701"/>
</element>
<element name="R6" library="Perfect_0402" package="0402" value="10K">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RC0402FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Perfect_0402" package="0402" value="10K">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RC0402FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="Perfect_0402" package="0402" value="10K">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RC0402FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="Perfect_0402" package="0402" value="10K">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RC0402FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="VBAT" library="alienflight" package="S2B-PH-K-S" value="JST 2.0 PH">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
<attribute name="MF" value="JST"/>
<attribute name="MPN" value="S2B-PH-K-S"/>
</element>
<element name="L1" library="AlienWhoop" package="DFE201612E-INDUCTOR" value="1uH">
<attribute name="MF" value="Murata"/>
<attribute name="MPN" value="DFE201612E-1R0M=P2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="alienflight" package="YUDEN-CAP-0805" value="10uF">
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="JMK212AB7106KG-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="alienflight" package="YUDEN-CAP-0805" value="10uF">
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="JMK212AB7106KG-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="AlienWhoop" package="TPS6306X" value="TPS63061DSC5V">
<attribute name="PARTNO" value="TPS63061DSCR"/>
</element>
<element name="C24" library="Perfect_0402" package="0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GCM155R71C104KA55D"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="alienflight" package="YUDEN-CAP-0805" value="22uF">
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="JMK212BJ226MG-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="alienflight" package="YUDEN-CAP-0805" value="22uF">
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="JMK212BJ226MG-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="alienflight" package="YUDEN-CAP-0805" value="22uF">
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="JMK212BJ226MG-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="Perfect_0402" package="0402" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GRM155R60G475ME47J"/>
<attribute name="VALUE"/>
</element>
<element name="LED0" library="alienflight" package="SMD-CHIP-LED-0805" value="BLUE">
<attribute name="MF" value="Kingbright"/>
<attribute name="MPN" value="APHCM2012QBC/D-F01"/>
</element>
<element name="Q5" library="AlienWhoop" package="SOT-23" value="3.3V">
<attribute name="PARTNO" value="AP2210N-3.3TRG1"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="Perfect_0402" package="0402" value="1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GRM155C71A105KE11D"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="Perfect_0402" package="0402" value="2.2uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GRM155C70J225KE11D"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="Perfect_0402" package="0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GCM155R71C104KA55D"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="Perfect_0402" package="0402" value="10nF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GCM155R71H103KA55D"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="Perfect_0402" package="0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="GCM155R71C104KA55D"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Sparkfun" package="QFN24_PAD" value="MPU-6881">
<attribute name="NAME"/>
<attribute name="PARTNO" value="MPU-6881"/>
<attribute name="VALUE"/>
</element>
<element name="+" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="-" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="U$1" library="holes" package="3,2" value=""/>
<element name="U$2" library="holes" package="3,2" value=""/>
<element name="U$3" library="holes" package="3,2" value=""/>
<element name="U$4" library="holes" package="3,2" value=""/>
<element name="R2" library="Perfect_0402" package="0402" value="2K7">
<attribute name="NAME"/>
<attribute name="PARTNO" value="AC0402JR-072K7L"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Perfect_0402" package="0402" value="2K7">
<attribute name="NAME"/>
<attribute name="PARTNO" value="AC0402JR-072K7L"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO3" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="R4" library="Perfect_0402" package="0402" value="200R">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RC0402JR-7D200RL"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Perfect_0402" package="0402" value="1K">
<attribute name="NAME"/>
<attribute name="PARTNO" value="AT0402BRD071KL"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="Perfect_0402" package="0402" value="2K">
<attribute name="NAME"/>
<attribute name="PARTNO" value="AT0402BRE072KL"/>
<attribute name="VALUE"/>
</element>
<element name="U$13" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="U$14" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="5V2" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="3.3V2" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="GND23" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="STM32" library="AlienWhoop" package="FE03-1" value="PROG">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="A13" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="A14" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="DFU" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
<attribute name="NAME"/>
</element>
<element name="SPI_CS" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
<element name="GND@2" library="AlienWhoop" package="TESTPAD" value="TESTPAD">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNP" value="T"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="M1" pad="1"/>
<contactref element="M2" pad="1"/>
<contactref element="M0" pad="1"/>
<contactref element="M3" pad="1"/>
<contactref element="U7" pad="2"/>
<contactref element="U7" pad="3"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="VBAT" pad="1"/>
<contactref element="+" pad="TP"/>
<contactref element="R10" pad="2"/>
<contactref element="U7" pad="4"/>
<contactref element="M1" pad="1S"/>
<contactref element="M2" pad="1S"/>
<contactref element="M0" pad="1S"/>
<contactref element="M3" pad="1S"/>
</signal>
<signal name="NRST">
<contactref element="U2" pad="4"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="Q1" pad="S"/>
<contactref element="Q1" pad="S1"/>
<contactref element="R6" pad="1"/>
<contactref element="Q2" pad="S"/>
<contactref element="Q2" pad="S1"/>
<contactref element="R7" pad="1"/>
<contactref element="Q0" pad="S"/>
<contactref element="Q0" pad="S1"/>
<contactref element="R8" pad="1"/>
<contactref element="Q3" pad="S"/>
<contactref element="Q3" pad="S1"/>
<contactref element="R9" pad="1"/>
<contactref element="U7" pad="P$18"/>
<contactref element="U7" pad="P$4"/>
<contactref element="U7" pad="P$21"/>
<contactref element="U7" pad="P$1"/>
<contactref element="U7" pad="P$2"/>
<contactref element="U7" pad="P$3"/>
<contactref element="U7" pad="P$17"/>
<contactref element="U7" pad="P$22"/>
<contactref element="U7" pad="P$5"/>
<contactref element="C24" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="VBAT" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="Q5" pad="1"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="-" pad="TP"/>
<contactref element="LED0" pad="C"/>
<contactref element="U2" pad="6"/>
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="U2" pad="15"/>
<contactref element="GND23" pad="TP"/>
<contactref element="STM32" pad="1"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="20"/>
<contactref element="C9" pad="2"/>
<contactref element="U1" pad="11"/>
<contactref element="C10" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U7" pad="7"/>
<contactref element="GND@2" pad="TP"/>
</signal>
<signal name="PROG_SCL">
<contactref element="U2" pad="20"/>
<contactref element="STM32" pad="2"/>
<contactref element="A14" pad="TP"/>
</signal>
<signal name="PROG_SDA">
<contactref element="U2" pad="19"/>
<contactref element="STM32" pad="3"/>
<contactref element="A13" pad="TP"/>
</signal>
<signal name="GYRO_SDA">
<contactref element="U2" pad="18"/>
<contactref element="U1" pad="24"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GYRO_SCL">
<contactref element="U2" pad="17"/>
<contactref element="U1" pad="23"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="BOOT">
<contactref element="U2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="DFU" pad="TP"/>
</signal>
<signal name="M1G">
<contactref element="M1" pad="2"/>
<contactref element="Q1" pad="D3"/>
<contactref element="Q1" pad="D1"/>
<contactref element="Q1" pad="D"/>
<contactref element="Q1" pad="D2"/>
<contactref element="Q1" pad="D4"/>
<contactref element="M1" pad="2S"/>
</signal>
<signal name="M0G">
<contactref element="M0" pad="2"/>
<contactref element="Q0" pad="D3"/>
<contactref element="Q0" pad="D1"/>
<contactref element="Q0" pad="D"/>
<contactref element="Q0" pad="D2"/>
<contactref element="Q0" pad="D4"/>
<contactref element="M0" pad="2S"/>
</signal>
<signal name="M3G">
<contactref element="M3" pad="2"/>
<contactref element="Q3" pad="D3"/>
<contactref element="Q3" pad="D1"/>
<contactref element="Q3" pad="D"/>
<contactref element="Q3" pad="D2"/>
<contactref element="Q3" pad="D4"/>
<contactref element="M3" pad="2S"/>
</signal>
<signal name="L1A">
<contactref element="L1" pad="P$1"/>
<contactref element="U7" pad="1"/>
</signal>
<signal name="L1B">
<contactref element="L1" pad="P$2"/>
<contactref element="U7" pad="10"/>
</signal>
<signal name="VAUX">
<contactref element="U7" pad="6"/>
<contactref element="C24" pad="1"/>
</signal>
<signal name="LED0">
<contactref element="U2" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="Q5" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="16"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="3.3V2" pad="TP"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="5V-REG">
<contactref element="C22" pad="1"/>
<contactref element="Q5" pad="3"/>
<contactref element="U7" pad="9"/>
<contactref element="U7" pad="8"/>
<contactref element="C25" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="5V2" pad="TP"/>
</signal>
<signal name="LED">
<contactref element="R4" pad="1"/>
<contactref element="LED0" pad="A"/>
</signal>
<signal name="VOLTDIV">
<contactref element="U2" pad="11"/>
<contactref element="R10" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="USART1_RX">
<contactref element="U2" pad="9"/>
<contactref element="U$13" pad="TP"/>
</signal>
<signal name="USART1_TX">
<contactref element="U2" pad="8"/>
<contactref element="U$14" pad="TP"/>
</signal>
<signal name="REGOUT">
<contactref element="U1" pad="10"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="M0">
<contactref element="R8" pad="2"/>
<contactref element="Q0" pad="G"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="M3">
<contactref element="R9" pad="2"/>
<contactref element="Q3" pad="G"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="M2">
<contactref element="R7" pad="2"/>
<contactref element="Q2" pad="G"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="SPI_CS">
<contactref element="U2" pad="7"/>
<contactref element="SPI_CS" pad="TP"/>
</signal>
<signal name="M1">
<contactref element="U2" pad="14"/>
<contactref element="Q1" pad="G"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="M2G">
<contactref element="M2" pad="2S"/>
<contactref element="M2" pad="2"/>
<contactref element="Q2" pad="D3"/>
<contactref element="Q2" pad="D"/>
<contactref element="Q2" pad="D1"/>
<contactref element="Q2" pad="D2"/>
<contactref element="Q2" pad="D4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
