<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="3.81" y1="0" x2="89.9414" y2="0" width="0" layer="20"/>
<wire x1="93.7514" y1="3.81" x2="93.7514" y2="62.23" width="0" layer="20"/>
<wire x1="89.9414" y1="65.8622" x2="3.81" y2="65.8622" width="0" layer="20"/>
<wire x1="0" y1="62.23" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="3.81" y1="65.8622" x2="0" y2="62.23" width="0" layer="20" curve="-90"/>
<wire x1="89.9414" y1="65.8622" x2="93.7514" y2="62.23" width="0" layer="20" curve="90"/>
<wire x1="89.9414" y1="0" x2="93.7514" y2="3.81" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0" layer="20" curve="-90"/>
<text>well-siting-meter</text>
<text>v2</text>
<text>danwahl.github.io/</text>
<text>BATT</text>
<text>GND</text>
<text>I1</text>
<text>I2</text>
<text>V1</text>
<text>V2</text>
<text>BATT</text>
<text>GND</text>
<text>I1</text>
<text>I2</text>
<text>V1</text>
<text>V2</text>
<text>rev A</text>
<text>sn:</text>
</plain>
<libraries>
<library name="ec2">
<packages>
<package name="EC2">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_PRO_MINI">
</package>
</packages>
</library>
<library name="ad623">
<packages>
<package name="DIP08">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="DIODE-1N4001">
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="BANANA_CONN">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LCD-16X2_NOHOLES">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="max1771">
<packages>
<package name="DIP-08">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TRIM-3386">
</package>
</packages>
</library>
<library name="misc">
<packages>
<package name="1415">
</package>
</packages>
</library>
<library name="murata1400">
<packages>
<package name="MURATA1400">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U3" library="ec2" package="EC2" value="EC2">
<attribute name="NAME"/>
<attribute name="PN" value="399-11029-5-ND"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="ec2" package="EC2" value="EC2">
<attribute name="NAME"/>
<attribute name="PN" value="399-11029-5-ND"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-Boards" package="ARDUINO_PRO_MINI" value="ARDUINO_PRO_MINI">
<attribute name="NAME"/>
<attribute name="PN" value="1568-1055-ND"/>
</element>
<element name="U5" library="ad623" package="DIP08" value="AD623">
<attribute name="NAME"/>
<attribute name="PN" value="AD623ANZ-ND"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="ad623" package="DIP08" value="AD623">
<attribute name="NAME"/>
<attribute name="PN" value="AD623ANZ-ND"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="PN" value="PN2222AFS-ND"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="PN" value="PN2222AFS-ND"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="">
<attribute name="NAME"/>
<attribute name="PN" value="1N4001-TPMSCT-ND"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="">
<attribute name="NAME"/>
<attribute name="PN" value="1N4001-TPMSCT-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="10K">
<attribute name="NAME"/>
<attribute name="PN" value="10.0KXBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="10K">
<attribute name="NAME"/>
<attribute name="PN" value="10.0KXBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value="392R">
<attribute name="NAME"/>
<attribute name="PN" value="392XBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value="392R">
<attribute name="NAME"/>
<attribute name="PN" value="392XBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.4" value="2.05K">
<attribute name="NAME"/>
<attribute name="PN" value="2.05KXBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.4" value="100K">
<attribute name="NAME"/>
<attribute name="PN" value="100KXBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.6" value="0R050">
<attribute name="NAME"/>
<attribute name="PN" value="696-1731-ND"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03" value="7805">
<attribute name="NAME"/>
<attribute name="PN" value="811-2196-5-ND"/>
<attribute name="PN2" value="LM7805CT-ND"/>
</element>
<element name="C7" library="SparkFun-Passives" package="CAP-PTH-5MM" value="10uF">
<attribute name="NAME"/>
<attribute name="PN" value="445-173437-1-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="CAP-PTH-5MM" value="10uF">
<attribute name="NAME"/>
<attribute name="PN" value="445-173437-1-ND"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-Displays" package="LCD-16X2_NOHOLES" value="LCD-16X2NOHOLES">
<attribute name="PN" value="1528-1502-ND"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="BANANA_CONN" value="">
<attribute name="PN" value="1568-1665-ND"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="BANANA_CONN" value="">
<attribute name="PN" value="1568-1664-ND"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="BANANA_CONN" value="">
<attribute name="PN" value="1568-1665-ND"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="BANANA_CONN" value="">
<attribute name="PN" value="1568-1664-ND"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="BANANA_CONN" value="">
<attribute name="PN" value="1568-1665-ND"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="BANANA_CONN" value="">
<attribute name="PN" value="1568-1664-ND"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="NAME"/>
<attribute name="PN" value="SW406-ND"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="NAME"/>
<attribute name="PN" value="SW406-ND"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-1000UF-25V" value="100uF">
<attribute name="NAME"/>
<attribute name="PN" value="1572-1306-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="CAP-PTH-5MM" value="0.1uf">
<attribute name="NAME"/>
<attribute name="PN" value="BC2665CT-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="CAP-PTH-5MM" value="0.1uf">
<attribute name="NAME"/>
<attribute name="PN" value="BC2665CT-ND"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-NCHANNELFQP30N06L">
<attribute name="NAME"/>
<attribute name="PN" value="FDP33N25-ND"/>
<attribute name="PROD_ID" value="TRANS-10060"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="">
<attribute name="NAME"/>
<attribute name="PN" value="EGP20FCT-ND"/>
<attribute name="VALUE"/>
</element>
<element name="RSENSE" library="SparkFun-Passives" package="AXIAL-0.6" value="0R010">
<attribute name="NAME"/>
<attribute name="PN" value="696-1729-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.4" value="10K">
<attribute name="NAME"/>
<attribute name="PN" value="10.0KXBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.4" value="1M">
<attribute name="NAME"/>
<attribute name="PN" value="1.00MXBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="CAP-PTH-5MM" value="0.1uf">
<attribute name="NAME"/>
<attribute name="PN" value="445-173449-1-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="CPOL-RADIAL-1000UF-25V" value="4u7">
<attribute name="NAME"/>
<attribute name="PN" value="399-6091-ND"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="max1771" package="DIP-08" value="MAX1771">
<attribute name="NAME"/>
<attribute name="PN" value="MAX1771CPA+-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="AXIAL-0.4" value="31.6K">
<attribute name="NAME"/>
<attribute name="PN" value="31.6KXBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Passives" package="AXIAL-0.4" value="31.6K">
<attribute name="NAME"/>
<attribute name="PN" value="31.6KXBK-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Passives" package="CAP-PTH-5MM" value="0.1uf">
<attribute name="NAME"/>
<attribute name="PN" value="BC2665CT-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Passives" package="CAP-PTH-5MM" value="0.1uf">
<attribute name="NAME"/>
<attribute name="PN" value="BC2665CT-ND"/>
<attribute name="VALUE"/>
</element>
<element name="TM1" library="adafruit" package="TRIM-3386" value="">
<attribute name="NAME"/>
<attribute name="PN" value="1528-1997-ND "/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="misc" package="1415" value="22uH">
<attribute name="NAME"/>
<attribute name="PN" value="732-7163-ND"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="murata1400" package="MURATA1400" value="47uH">
<attribute name="NAME"/>
<attribute name="PN" value="811-2633-ND"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U5" pad="4"/>
<contactref element="U6" pad="4"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="J2" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="J8" pad="P$1"/>
<contactref element="S1" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="RSENSE" pad="P$2"/>
<contactref element="U7" pad="6"/>
<contactref element="U7" pad="7"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="21"/>
<contactref element="U5" pad="7"/>
<contactref element="U6" pad="7"/>
<contactref element="R1" pad="P$1"/>
<contactref element="J2" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$1">
<contactref element="Q2" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="P$2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="VSW">
<contactref element="R4" pad="P$1"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="P$2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="ISW">
<contactref element="R3" pad="P$1"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="I1">
<contactref element="U3" pad="9"/>
<contactref element="J9" pad="P$1"/>
</signal>
<signal name="I2">
<contactref element="U3" pad="4"/>
<contactref element="J10" pad="P$1"/>
</signal>
<signal name="IRET">
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="8"/>
<contactref element="U5" pad="3"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="V+">
<contactref element="U6" pad="3"/>
<contactref element="U4" pad="10"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="V-">
<contactref element="U6" pad="2"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="N$24">
<contactref element="U5" pad="1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$25">
<contactref element="R5" pad="P$2"/>
<contactref element="U5" pad="8"/>
</signal>
<signal name="N$26">
<contactref element="U6" pad="1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$27">
<contactref element="R6" pad="P$2"/>
<contactref element="U6" pad="8"/>
</signal>
<signal name="IOUT">
<contactref element="U2" pad="17"/>
<contactref element="R10" pad="P$2"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="U2" pad="18"/>
<contactref element="C10" pad="1"/>
<contactref element="R11" pad="P$2"/>
</signal>
<signal name="VIN">
<contactref element="U3" pad="10"/>
<contactref element="U3" pad="5"/>
<contactref element="D3" pad="C"/>
<contactref element="C4" pad="1"/>
<contactref element="R9" pad="P$1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="V2">
<contactref element="U4" pad="4"/>
<contactref element="J12" pad="P$1"/>
</signal>
<signal name="V1">
<contactref element="U4" pad="9"/>
<contactref element="J11" pad="P$1"/>
</signal>
<signal name="VREF">
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="U5" pad="5"/>
<contactref element="U6" pad="5"/>
</signal>
<signal name="V_BATT">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="J2" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="J7" pad="P$1"/>
<contactref element="C1" pad="1"/>
<contactref element="U7" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="L1" pad="P1"/>
<contactref element="L2" pad="P$1"/>
<contactref element="U3" pad="12"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="RS">
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="E">
<contactref element="U1" pad="6"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="DB7">
<contactref element="U1" pad="14"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="DB6">
<contactref element="U1" pad="13"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="DB5">
<contactref element="U1" pad="12"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="DB4">
<contactref element="U1" pad="11"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="VO">
<contactref element="U1" pad="3"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$3">
</signal>
<signal name="B1">
<contactref element="U2" pad="7"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="B2">
<contactref element="U2" pad="8"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C3" pad="1"/>
<contactref element="U7" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="T1" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="L1" pad="P2"/>
<contactref element="L2" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="T1" pad="1"/>
<contactref element="U7" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="T1" pad="3"/>
<contactref element="RSENSE" pad="P$1"/>
<contactref element="U7" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="R9" pad="P$2"/>
<contactref element="TM1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="P$1"/>
<contactref element="TM1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U7" pad="3"/>
<contactref element="TM1" pad="2"/>
</signal>
<signal name="SHDN">
<contactref element="U7" pad="4"/>
<contactref element="U2" pad="19"/>
</signal>
<signal name="N$12">
<contactref element="U5" pad="6"/>
<contactref element="R10" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="U6" pad="6"/>
<contactref element="R11" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
