<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="31.496" y1="0" x2="95.428" y2="0" width="0" layer="20"/>
<wire x1="95.428" y1="0" x2="95.428" y2="48.25" width="0" layer="20"/>
<wire x1="95.428" y1="48.25" x2="31.496" y2="48.25" width="0" layer="20"/>
<wire x1="31.496" y1="48.25" x2="31.496" y2="0" width="0" layer="20"/>
<text>Monitor</text>
<text>2 Ports</text>
<text>Female</text>
<text>Female</text>
<text>Male</text>
<text>Male</text>
<text>Paterson Technology</text>
<text>Dual Serial / Monitor V 1.1</text>
<text>Enhanced</text>
<text>Standard</text>
</plain>
<libraries>
<library name="Tim's Parts">
<packages>
<package name="TSSOP16">
<description>TSSOP-16, 0.65mm pitch, 4.5mm body width</description>
</package>
<package name="QF24">
<description>QFN 24 4x4mm</description>
</package>
<package name="CONN-2.54X2-6">
</package>
<package name="0603">
<description>Generic 0603
Same as ExpressPCB</description>
</package>
<package name="LED-DUAL-1206">
</package>
</packages>
</library>
<library name="Connectors">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="USB_MICRO-B_FCI">
</package>
<package name="DE-9F-RA-.318">
</package>
<package name="DE-9M-RA-.318">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="Tim's Parts" package="TSSOP16" value="MAX202">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Connectors" package="USB_MICRO-B_FCI" value="USB_MINI-B-MICRO-B_FCI">
<attribute name="NAME"/>
</element>
<element name="J4" library="Connectors" package="DE-9F-RA-.318" value="DE-9F-RA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Connectors" package="DE-9F-RA-.318" value="DE-9F-RA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="Connectors" package="DE-9M-RA-.318" value="DE-9M-RA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="Connectors" package="DE-9M-RA-.318" value="DE-9M-RA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Tim's Parts" package="QF24" value="CP2105">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="Tim's Parts" package="CONN-2.54X2-6" value=""/>
<element name="C1" library="Tim's Parts" package="0603" value=".1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Tim's Parts" package="0603" value=".1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Tim's Parts" package="0603" value=".1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Tim's Parts" package="0603" value=".1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Tim's Parts" package="0603" value=".1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="Tim's Parts" package="0603" value=".1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="Tim's Parts" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="Tim's Parts" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="Tim's Parts" package="LED-DUAL-1206" value="LED-DUAL">
<attribute name="NAME"/>
</element>
<element name="LED2" library="Tim's Parts" package="LED-DUAL-1206" value="LED-DUAL">
<attribute name="NAME"/>
</element>
<element name="R1" library="Tim's Parts" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Tim's Parts" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Tim's Parts" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Tim's Parts" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U2" pad="15"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="EXP"/>
<contactref element="J1" pad="5"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="5"/>
<contactref element="J4" pad="5"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="5"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="C2" pad="2"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="V-">
<contactref element="U2" pad="6"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="V+">
<contactref element="U2" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="U2" pad="16"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="6"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="SW1" pad="4"/>
</signal>
<signal name="N$27">
<contactref element="J2" pad="3"/>
<contactref element="U2" pad="13"/>
<contactref element="J3" pad="2"/>
<contactref element="SW1" pad="5"/>
</signal>
<signal name="N$28">
<contactref element="J4" pad="3"/>
<contactref element="J5" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="SW1" pad="6"/>
</signal>
<signal name="N$29">
<contactref element="J5" pad="3"/>
<contactref element="J4" pad="2"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="11"/>
<contactref element="U1" pad="13"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="10"/>
<contactref element="U1" pad="21"/>
<contactref element="LED2" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="12"/>
<contactref element="U1" pad="12"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="9"/>
<contactref element="U1" pad="20"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="7"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="14"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R4" pad="2"/>
<contactref element="LED2" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="R3" pad="2"/>
<contactref element="LED2" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R2" pad="1"/>
<contactref element="LED1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
