<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.7645" y2="0" width="0" layer="20"/>
<wire x1="20.7645" y1="0" x2="20.7645" y2="36.83" width="0" layer="20"/>
<wire x1="20.7645" y1="36.83" x2="0" y2="36.83" width="0" layer="20"/>
<wire x1="0" y1="36.83" x2="0" y2="0" width="0" layer="20"/>
<text>AT28C64 to 2716</text>
<text>Georgian Borca - 2022</text>
<text>AT28C64B</text>
</plain>
<libraries>
<library name="memory">
<description>&lt;b&gt;Generic Memories&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL24">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P1524X482-28">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="ANARCHY_LOGO">
<description>Anarchy Logo by BrK</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="memory" package="DIL24" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="DIP254P1524X482-28" value="AT28C64B-15PU">
<attribute name="PACKAGE" value="PCDIP-28"/>
<attribute name="MPN" value="AT28C64B-15PU"/>
<attribute name="SUPPLIER" value="ATMEL"/>
<attribute name="DESCRIPTION" value="Parallel EEPROM"/>
<attribute name="OC_FARNELL" value="1095784"/>
<attribute name="OC_NEWARK" value="96K6557"/>
</element>
<element name="U$1" library="dp_devices" package="ANARCHY_LOGO" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC1" pad="24"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="12"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="11"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="12"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="11"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="15"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="14"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="17"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="16"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="19"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="8"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="7"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="6"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="5"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="4"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="3"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="23"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="22"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="19"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="22"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="20"/>
<contactref element="IC1" pad="18"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
