<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.53" y1="9.26" x2="20.365" y2="9.26" width="0" layer="20"/>
<wire x1="20.365" y1="9.26" x2="20.365" y2="24.47" width="0" layer="20"/>
<wire x1="20.365" y1="24.47" x2="0.53" y2="24.45" width="0" layer="20"/>
<wire x1="0.53" y1="24.45" x2="0.53" y2="9.26" width="0" layer="20"/>
<text>EZ-I2C Charger V1</text>
<text>EZ-I2C Charger V1</text>
</plain>
<libraries>
<library name="UniqueInteractionsLib">
<packages>
<package name="EZ-I2CHEADERV1">
</package>
</packages>
</library>
<library name="MiniWear_LOGO">
<packages>
<package name="LOGO2">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-PTH-NS">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="LED-0603">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="serial">
<packages>
<package name="ZX62-B-5PA">
<description>&lt;b&gt;Hirose ZX62-B-5PA(11)&lt;/b&gt;&lt;br&gt;
Micro B - Standard (Bottom Mount), Shell SMT</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="UniqueInteractionsLib" package="EZ-I2CHEADERV1" value="EZ-I2CHEADERV1"/>
<element name="U$6" library="MiniWear_LOGO" package="LOGO2" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="M02-JST-2-PTH-NO_SILK">
<attribute name="NAME"/>
</element>
<element name="U$2" library="MiniWear_LOGO" package="LOGO2" value=""/>
<element name="D11" library="SparkFun" package="LED-0603" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0402-RES" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun" package="SOT23-5" value="MCP73831">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0402-RES" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0402-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="0402-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="serial" package="ZX62-B-5PA" value="MICRO-USB-ZX62-B-5PA"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="USB1" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="SDA"/>
<contactref element="U$1" pad="SDA1"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="SCL"/>
<contactref element="U$1" pad="SCL1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="VCC"/>
<contactref element="U$1" pad="VCC1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="LPOW"/>
<contactref element="U$1" pad="LPOW1"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="USB1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D11" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="PROG">
<contactref element="U1" pad="5"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="STAT">
<contactref element="D11" pad="C"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="BAT">
<contactref element="U1" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="BAT"/>
<contactref element="U$1" pad="BAT1"/>
</signal>
<signal name="GND1">
<contactref element="USB1" pad="GND@1"/>
</signal>
<signal name="GND2">
<contactref element="USB1" pad="GND@2"/>
</signal>
<signal name="GND3">
<contactref element="USB1" pad="GND@3"/>
</signal>
<signal name="GND4">
<contactref element="USB1" pad="GND@4"/>
</signal>
<signal name="GND5">
<contactref element="USB1" pad="GND@5"/>
</signal>
<signal name="GND6">
<contactref element="USB1" pad="GND@6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
