<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="27.5" x2="0" y2="1.5" width="0" layer="20"/>
<wire x1="0" y1="1.5" x2="1.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.5" y1="0" x2="53" y2="0" width="0" layer="20"/>
<wire x1="53" y1="0" x2="54.5" y2="1.5" width="0" layer="20" curve="90"/>
<wire x1="54.5" y1="1.5" x2="54.5" y2="27.5" width="0" layer="20"/>
<wire x1="54.5" y1="27.5" x2="53" y2="29" width="0" layer="20" curve="90"/>
<wire x1="53" y1="29" x2="1.5" y2="29" width="0" layer="20"/>
<wire x1="1.5" y1="29" x2="0" y2="27.5" width="0" layer="20" curve="90"/>
<text>GND</text>
<text>VCC</text>
<text>H/L</text>
<text>PD</text>
<text>PTT</text>
<text>AF_OUT</text>
<text>SQ</text>
<text>MIC_IN</text>
<text>TXD</text>
<text>RXD</text>
<text>SQ</text>
<text>AF</text>
<text>PTT</text>
<text>PD</text>
<text>H/L</text>
<text>MIC</text>
<text>TXD</text>
<text>RXD</text>
<text>ANT</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>LOW</text>
<text>IO PIN</text>
<text>DRA818U/V</text>
<text>Prototype Board v1.0
I. McLinden 2017</text>
<text>DRA818U/V</text>
<text>DRA818U/V</text>
<text>Prototype Board v1.0
I. McLinden 2017</text>
<text>ANT</text>
<text>ANT</text>
<text>GND</text>
<text>VCC</text>
<text>H/L</text>
<text>PD</text>
<text>PTT</text>
<text>AF_OUT</text>
<text>SQ</text>
<text>MIC_IN</text>
<text>TXD</text>
<text>RXD</text>
<text>Jumper IO PIN to pass H/L control to breakout pins.
Jumper LOW to pull H/L pin LOW/GND.

H/L LOW    -&gt; 0.5W TX
H/L FLOAT -&gt; 1.0W TX</text>
<text>IO PIN</text>
<text>LOW</text>
<text>VCC    3.3  -  4.5   V-DC
Freq   134  -  174   MHz
Temp   -20  -   70   °C
CH_w        25       MHz
T_sw        20       ms
Z           50       Ohm
P_low       26  27   dBm
P_high      29  31   dBm
F_dev          2.5   KHz</text>
<text>DRA818U/V Spec</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
<description>&lt;h3&gt;Plated Through Hole -10 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="dorji">
<packages>
<package name="DRA818U/V">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMA_EDGELAUNCH">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BRKOUT" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="H/LBP" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="dorji" package="DRA818U/V" value="DRA818U/V"/>
<element name="X1" library="adafruit" package="SMA_EDGELAUNCH" value="SMACONNECTOR_EDGE">
<attribute name="LABEL" value=""/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
</elements>
<signals>
<signal name="ANT">
<contactref element="U$1" pad="12"/>
<contactref element="X1" pad="P"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="GND@2"/>
<contactref element="X1" pad="GND@1"/>
<contactref element="X1" pad="GND@4"/>
<contactref element="X1" pad="GND@3"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="10"/>
<contactref element="H/LBP" pad="3"/>
<contactref element="BRKOUT" pad="10"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="BRKOUT" pad="9"/>
</signal>
<signal name="PD">
<contactref element="BRKOUT" pad="7"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="PTT">
<contactref element="BRKOUT" pad="6"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="AF_OUT">
<contactref element="BRKOUT" pad="5"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="SQ">
<contactref element="BRKOUT" pad="4"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="MIC_IN">
<contactref element="BRKOUT" pad="3"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="TXD">
<contactref element="U$1" pad="17"/>
<contactref element="BRKOUT" pad="2"/>
</signal>
<signal name="RXD">
<contactref element="BRKOUT" pad="1"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="BK_H/L">
<contactref element="BRKOUT" pad="8"/>
<contactref element="H/LBP" pad="1"/>
</signal>
<signal name="H/L">
<contactref element="U$1" pad="7"/>
<contactref element="H/LBP" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
