<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="47.93" y2="0" width="0" layer="20"/>
<wire x1="47.93" y1="0" x2="47.93" y2="48.25" width="0" layer="20"/>
<wire x1="47.93" y1="48.25" x2="0" y2="48.25" width="0" layer="20"/>
<wire x1="0" y1="48.25" x2="0" y2="0" width="0" layer="20"/>
<text>DB9M</text>
<text>DB9F</text>
<text>CD</text>
<text>RX</text>
<text>TX</text>
<text>DTR</text>
<text>DSR</text>
<text>RTS</text>
<text>CTS</text>
<text>RI</text>
<text>RS232 Tester</text>
<text>CFS 2015</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB9">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="DB9_MALE">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor-sil">
<description>&lt;b&gt;Resistors in Single Inline Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SIL9">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="LED3MM" value="RD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED3MM" value="GN"/>
<element name="JP1" library="SparkFun-Connectors" package="DB9" value="">
<attribute name="PROD_ID" value="CONN-08194"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="DB9_MALE" value="">
<attribute name="PROD_ID" value="CONN-09904"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED3MM" value="RD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED3MM" value="GN"/>
<element name="D5" library="SparkFun-LED" package="LED3MM" value="RD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-LED" package="LED3MM" value="GN"/>
<element name="D7" library="SparkFun-LED" package="LED3MM" value="RD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="SparkFun-LED" package="LED3MM" value="GN"/>
<element name="D9" library="SparkFun-LED" package="LED3MM" value="RD"/>
<element name="D10" library="SparkFun-LED" package="LED3MM" value="GN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="SparkFun-LED" package="LED3MM" value="RD"/>
<element name="D12" library="SparkFun-LED" package="LED3MM" value="GN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="SparkFun-LED" package="LED3MM" value="RD"/>
<element name="D14" library="SparkFun-LED" package="LED3MM" value="GN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D15" library="SparkFun-LED" package="LED3MM" value="RD"/>
<element name="D16" library="SparkFun-LED" package="LED3MM" value="GN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-sil" package="SIL9" value="2.2K">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="K"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="K"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="D6" pad="A"/>
<contactref element="D5" pad="K"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="D8" pad="A"/>
<contactref element="D7" pad="K"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="D10" pad="A"/>
<contactref element="D9" pad="K"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$29">
<contactref element="D14" pad="A"/>
<contactref element="D13" pad="K"/>
<contactref element="JP1" pad="8"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="D16" pad="A"/>
<contactref element="D15" pad="K"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="N$7">
<contactref element="D16" pad="K"/>
<contactref element="D15" pad="A"/>
<contactref element="RN1" pad="9"/>
</signal>
<signal name="N$12">
<contactref element="D14" pad="K"/>
<contactref element="D13" pad="A"/>
<contactref element="RN1" pad="8"/>
</signal>
<signal name="N$13">
<contactref element="D11" pad="A"/>
<contactref element="D12" pad="K"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="D10" pad="K"/>
<contactref element="D9" pad="A"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="D7" pad="A"/>
<contactref element="D8" pad="K"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="K"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="K"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="D2" pad="K"/>
<contactref element="D1" pad="A"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D12" pad="A"/>
<contactref element="D11" pad="K"/>
<contactref element="JP2" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="5"/>
<contactref element="JP1" pad="5"/>
<contactref element="RN1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
