<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.198" y2="0" width="0" layer="20"/>
<wire x1="33.198" y1="0" x2="33.198" y2="38.09" width="0" layer="20"/>
<wire x1="33.198" y1="38.09" x2="0" y2="38.09" width="0" layer="20"/>
<wire x1="0" y1="38.09" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>P0.25</text>
<text>P0.26</text>
<text>P0.27</text>
<text>P0.28</text>
<text>P0.29</text>
<text>P0.30</text>
<text>P0.31</text>
<text>DEC4</text>
<text>DCC</text>
<text>VDD</text>
<text>G</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>P0.03</text>
<text>P0.04</text>
<text>P0.05</text>
<text>P0.06</text>
<text>P0.07</text>
<text>P0.08</text>
<text>P0.09</text>
<text>P0.10</text>
<text>GND</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>P0.15</text>
<text>P0.16</text>
<text>P0.17</text>
<text>P0.18</text>
<text>P0.19</text>
<text>P0.20</text>
<text>21/RST</text>
<text>SWDCL</text>
<text>SWDIO</text>
<text>P0.22</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X15">
<description>&lt;h3&gt;Plated Through Hole -15 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:15&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_15&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="MDBT42Q_170329">
<description>Raytac MDBT42Q Eagle Library</description>
<packages>
<package name="MDBT42Q">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X15" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X09" value=""/>
<element name="J4" library="SparkFun-Connectors" package="1X15" value=""/>
<element name="MDBT42Q1" library="MDBT42Q_170329" package="MDBT42Q" value="MDBT42Q"/>
</elements>
<signals>
<signal name="N$16">
<contactref element="MDBT42Q1" pad="16"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="N$17">
<contactref element="MDBT42Q1" pad="17"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$21">
<contactref element="MDBT42Q1" pad="21"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="MDBT42Q1" pad="22"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="MDBT42Q1" pad="23"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="MDBT42Q1" pad="24"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="MDBT42Q1" pad="25"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="N$26">
<contactref element="MDBT42Q1" pad="26"/>
<contactref element="J1" pad="14"/>
</signal>
<signal name="N$27">
<contactref element="MDBT42Q1" pad="27"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="N$28">
<contactref element="MDBT42Q1" pad="28"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="N$29">
<contactref element="MDBT42Q1" pad="29"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="N$30">
<contactref element="MDBT42Q1" pad="30"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="N$31">
<contactref element="MDBT42Q1" pad="31"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="N$32">
<contactref element="MDBT42Q1" pad="32"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$33">
<contactref element="MDBT42Q1" pad="33"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$34">
<contactref element="MDBT42Q1" pad="34"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$35">
<contactref element="MDBT42Q1" pad="35"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$36">
<contactref element="MDBT42Q1" pad="36"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$37">
<contactref element="MDBT42Q1" pad="37"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$38">
<contactref element="MDBT42Q1" pad="38"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="MDBT42Q1" pad="39"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="MDBT42Q1" pad="1"/>
<contactref element="J4" pad="15"/>
</signal>
<signal name="N$2">
<contactref element="J4" pad="14"/>
<contactref element="MDBT42Q1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J4" pad="13"/>
<contactref element="MDBT42Q1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J4" pad="12"/>
<contactref element="MDBT42Q1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="11"/>
<contactref element="MDBT42Q1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="J4" pad="10"/>
<contactref element="MDBT42Q1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="J4" pad="9"/>
<contactref element="MDBT42Q1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="J4" pad="8"/>
<contactref element="MDBT42Q1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="J4" pad="7"/>
<contactref element="MDBT42Q1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="J4" pad="6"/>
<contactref element="MDBT42Q1" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="J4" pad="5"/>
<contactref element="MDBT42Q1" pad="11"/>
</signal>
<signal name="N$12">
<contactref element="J4" pad="4"/>
<contactref element="MDBT42Q1" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="MDBT42Q1" pad="13"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="MDBT42Q1" pad="14"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="J4" pad="1"/>
<contactref element="MDBT42Q1" pad="15"/>
</signal>
<signal name="N$18">
<contactref element="J2" pad="5"/>
<contactref element="MDBT42Q1" pad="20"/>
</signal>
<signal name="N$19">
<contactref element="J2" pad="6"/>
<contactref element="MDBT42Q1" pad="19"/>
</signal>
<signal name="N$20">
<contactref element="J2" pad="7"/>
<contactref element="MDBT42Q1" pad="18"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
