<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.0">
<drawing>
<board>
<plain>
<text>Phantomic Labs
BlueDevil Toneworks Division
Full Frontal Fuzz v1.0
2018</text>
<text>Phantomic Labs
BlueDevil Toneworks Division
Full Frontal Fuzz v1.0
2018</text>
</plain>
<libraries>
<library name="battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AB9V">
<description>&lt;B&gt;9-V BATTERY CLIP&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="radiotubes">
<packages>
<package name="POTI">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="E2,5-6E">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="0805-THM-7">
</package>
<package name="6MM">
</package>
</packages>
</library>
<library name="cap-master.rpt">
<description>&lt;b&gt;CAP MASTER! v4.02 - Electrolytic, Film and Tantalum&lt;/b&gt;&lt;br&gt;
&lt;p&gt;This library is a collection of SMD and through hole capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CNP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
&lt;small&gt;DISCLAIMER: The author does not warrant that this library is free from error or that it will meet your specific requirements.&lt;/small&gt;&lt;/p&gt;
&lt;author&gt;by Bob Starr (rtzaudio@mindspring.com)&lt;br&gt;
Updated 05/28/2005 - Rev 4.02&lt;/author&gt;&lt;br&gt;&lt;br&gt;</description>
<packages>
<package name="ENP-020-050">
<description>&lt;b&gt;BIPOLAR ELECTROLYTIC&lt;/b&gt;&lt;p&gt;
2.0 mm lead spacing, 5 mm diameter, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="Seeed-Diode">
<packages>
<package name="DO-214AC">
<description>http://www.sycelectronica.com.ar/semiconductores/1N4007-SMD.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors_custom">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO_JACK_0.25&quot;_TRS_PTH_RA">
<description>&lt;h3&gt;Right Angle -1/4" Stereo Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Components/General/JP-611%20DD.jpg”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;AUDIO_JACK_TRS_0.25"_PTH_RA&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3PDT">
<description>&lt;b&gt;3PDT 9 pin footswitch&lt;/b&gt; SF17020F-0302-21R-L&lt;p&gt;
Source: 3PDT.jpg</description>
</package>
</packages>
</library>
<library name="dp_pcb">
<packages>
<package name="DP9056_V1">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH_BREAD">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector Breadboard Compatible&lt;/h3&gt;
Breadboard-friendly pins. 
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/18742.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BAT9V" library="battery" package="AB9V" value="9V"/>
<element name="BIAS" library="radiotubes" package="POTI" value="50K B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="E2,5-6E" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="E2,5-6E" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="E2,5-6E" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="cap-master.rpt" package="ENP-020-050" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="SparkFun-Connectors" package="POWER_JACK_PTH_BREAD" value="9V">
<attribute name="PROD_ID" value="PRT-10811"/>
<attribute name="VALUE"/>
</element>
<element name="CONTOUR" library="radiotubes" package="POTI" value="1K B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Seeed-Diode" package="DO-214AC" value="1N4007">
<attribute name="MPN" value="1N4007"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FUZZ" library="radiotubes" package="POTI" value="1K B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors_custom" package="AUDIO_JACK_0.25&quot;_TRS_PTH_RA" value="AUDIO_JACK_TRS_0.25&quot;_PTH_RA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-12339"/>
<attribute name="SF_ID" value="COM-11144"/>
</element>
<element name="J2" library="SparkFun-Connectors_custom" package="AUDIO_JACK_0.25&quot;_TRS_PTH_RA" value="AUDIO_JACK_TRS_0.25&quot;_PTH_RA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-12339"/>
<attribute name="SF_ID" value="COM-11144"/>
</element>
<element name="LED1" library="adafruit" package="LED3MM" value="BLUE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92" value="NKT275">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-09536"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="NKT275">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-09536"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="0805-THM-7" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0805-THM-7" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0805-THM-7" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0805-THM-7" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0805-THM-7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="switch" package="3PDT" value="3PDT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TM1" library="adafruit" package="6MM" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VOLUME" library="radiotubes" package="POTI" value="500K A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="dp_pcb" package="DP9056_V1" value=""/>
</elements>
<signals>
<signal name="PWR">
<contactref element="CONTOUR" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="+"/>
<contactref element="D1" pad="2"/>
<contactref element="CN1" pad="PWR"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="GNDBREAK">
<contactref element="CN1" pad="GNDBREAK"/>
<contactref element="BAT9V" pad="+"/>
</signal>
<signal name="NET_J1_SW1B">
<contactref element="BAT9V" pad="-"/>
<contactref element="J1" pad="RING"/>
<contactref element="SW1" pad="6"/>
<contactref element="J1" pad="RING-NORM"/>
</signal>
<signal name="GND">
<contactref element="Q2" pad="3"/>
<contactref element="J1" pad="SLEEVE"/>
<contactref element="CN1" pad="GND"/>
<contactref element="SW1" pad="8"/>
<contactref element="FUZZ" pad="3"/>
<contactref element="C1" pad="-"/>
<contactref element="D1" pad="1"/>
<contactref element="C4" pad="-"/>
<contactref element="J2" pad="SLEEVE"/>
<contactref element="VOLUME" pad="3"/>
<contactref element="J1" pad="SLEEVE-NORM"/>
<contactref element="J2" pad="SLEEVE-NORM"/>
</signal>
<signal name="NET_J1_SW1A">
<contactref element="J1" pad="TIP"/>
<contactref element="SW1" pad="1"/>
<contactref element="J1" pad="TIP-NORM"/>
</signal>
<signal name="NET_LED_SW1C">
<contactref element="SW1" pad="7"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="NET_SW1A_SW1C">
<contactref element="SW1" pad="9"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="NET_VOL_SW1B">
<contactref element="SW1" pad="4"/>
<contactref element="VOLUME" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="-"/>
<contactref element="BIAS" pad="1"/>
</signal>
<signal name="NET_BIAS_SW1A">
<contactref element="BIAS" pad="2"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="NET_J2_SW1B">
<contactref element="J2" pad="RING"/>
<contactref element="SW1" pad="5"/>
<contactref element="J2" pad="RING-NORM"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="1"/>
<contactref element="TM1" pad="S"/>
</signal>
<signal name="N$7">
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="FUZZ" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="TM1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="CONTOUR" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="FUZZ" pad="2"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$11">
<contactref element="C3" pad="2"/>
<contactref element="VOLUME" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
