<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="30.48" y1="20.32" x2="114.28" y2="20.32" width="0" layer="20"/>
<wire x1="114.28" y1="20.32" x2="114.28" y2="79.68" width="0" layer="20"/>
<wire x1="114.28" y1="79.68" x2="30.48" y2="79.68" width="0" layer="20"/>
<wire x1="30.48" y1="79.68" x2="30.48" y2="20.32" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-SHROUDED-NS">
</package>
<package name="1X02_BIG">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
<library name="DUElib130425">
<packages>
<package name="DUE(NORMAL)">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="10PIN" library="SparkFun-Connectors" package="2X5-SHROUDED-NS" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="">
<attribute name="PROD_ID" value="RES-9435"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="">
<attribute name="PROD_ID" value="RES-9435"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="">
<attribute name="PROD_ID" value="RES-9435"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="">
<attribute name="PROD_ID" value="RES-9435"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="">
<attribute name="PROD_ID" value="RES-9435"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="">
<attribute name="PROD_ID" value="RES-9435"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X02_BIG" value=""/>
<element name="J5" library="SparkFun-Connectors" package="1X02_BIG" value=""/>
<element name="J6" library="SparkFun-Connectors" package="1X02_BIG" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X02_BIG" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X02_BIG" value=""/>
<element name="J1" library="SparkFun-Connectors" package="1X02_BIG" value=""/>
<element name="U$1" library="DUElib130425" package="DUE(NORMAL)" value="DUE(NORMAL)"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="P$2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="P$2"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="J3" pad="P$2"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="J4" pad="P$2"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="J5" pad="P$2"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="J6" pad="P$2"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="PIN1">
<contactref element="10PIN" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="PIN3">
<contactref element="10PIN" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="PIN2">
<contactref element="10PIN" pad="2"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="PIN4">
<contactref element="10PIN" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="PIN6">
<contactref element="10PIN" pad="6"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="PIN8">
<contactref element="10PIN" pad="8"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J6" pad="P$1"/>
<contactref element="J5" pad="P$1"/>
<contactref element="J4" pad="P$1"/>
<contactref element="J3" pad="P$1"/>
<contactref element="J2" pad="P$1"/>
<contactref element="J1" pad="P$1"/>
<contactref element="10PIN" pad="10"/>
<contactref element="10PIN" pad="5"/>
<contactref element="10PIN" pad="7"/>
<contactref element="10PIN" pad="9"/>
<contactref element="U$1" pad="GND_2"/>
<contactref element="U$1" pad="GND_1"/>
<contactref element="U$1" pad="5V_ICSP"/>
<contactref element="U$1" pad="GND_B"/>
<contactref element="U$1" pad="GND_A"/>
<contactref element="U$1" pad="GND1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="P$2"/>
<contactref element="U$1" pad="52"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="P$2"/>
<contactref element="U$1" pad="50"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="P$2"/>
<contactref element="U$1" pad="48"/>
</signal>
<signal name="N$8">
<contactref element="R4" pad="P$2"/>
<contactref element="U$1" pad="46"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="P$2"/>
<contactref element="U$1" pad="44"/>
</signal>
<signal name="N$12">
<contactref element="R6" pad="P$2"/>
<contactref element="U$1" pad="42"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
