<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="76.2" y2="0" width="0" layer="20"/>
<wire x1="76.2" y1="0" x2="76.2" y2="76.2" width="0" layer="20"/>
<wire x1="76.2" y1="76.2" x2="0" y2="76.2" width="0" layer="20"/>
<wire x1="0" y1="76.2" x2="0" y2="0" width="0" layer="20"/>
<text>CONTROLLER
THIS SIDE</text>
<text>github.com/dvdfreitag/4x4</text>
</plain>
<libraries>
<library name="Cherry-MX">
<packages>
<package name="CHERRY-MX">
</package>
</packages>
</library>
<library name="Passives">
<packages>
<package name="DIODE-PTH">
</package>
<package name="TWITTER">
</package>
<package name="OSHW">
</package>
<package name="0603-LED">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="Connectors">
<packages>
<package name="M01X1_100MIL-PTH">
</package>
<package name="M12X1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S2" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S3" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S4" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S5" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S6" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S7" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S8" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S9" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S10" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S11" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S12" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S13" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S14" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S15" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S16" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="D1" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D2" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D3" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D4" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D5" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D6" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D7" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D8" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D9" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D10" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D11" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D12" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D13" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D14" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D15" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D16" library="Passives" package="DIODE-PTH" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="J1" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J2" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J3" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J4" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J5" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J6" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J7" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J8" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J9" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J10" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J11" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J12" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J13" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J14" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J15" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J16" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J17" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J21" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J18" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J22" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J19" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J23" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J20" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J24" library="Connectors" package="M01X1_100MIL-PTH" value="M01X1-100MIL-PTH"/>
<element name="J25" library="Connectors" package="M12X1" value="M12-100MIL">
<attribute name="NAME"/>
</element>
<element name="J26" library="Connectors" package="M12X1" value="M12-100MIL">
<attribute name="NAME"/>
</element>
<element name="U$1" library="Passives" package="TWITTER" value=""/>
<element name="U$2" library="Passives" package="OSHW" value=""/>
<element name="D17" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="D18" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="D19" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="D20" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="D21" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="D22" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="D23" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="D24" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="D25" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="R1" library="Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
</element>
<element name="R2" library="Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
</element>
<element name="R3" library="Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
</element>
<element name="R4" library="Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
</element>
<element name="R5" library="Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
</element>
<element name="R6" library="Passives" package="0603-CAP" value=""/>
<element name="R7" library="Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
</element>
<element name="R8" library="Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
</element>
<element name="R9" library="Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="ROW0">
<contactref element="D4" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="J1" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J26" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="S3" pad="S2"/>
<contactref element="S3" pad="S3"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="S4" pad="S2"/>
<contactref element="S4" pad="S3"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="S2" pad="S2"/>
<contactref element="S2" pad="S3"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="S1" pad="S2"/>
<contactref element="S1" pad="S3"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="ROW1">
<contactref element="D8" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="J2" pad="1"/>
<contactref element="J6" pad="1"/>
<contactref element="J25" pad="5"/>
</signal>
<signal name="ROW2">
<contactref element="D12" pad="C"/>
<contactref element="D11" pad="C"/>
<contactref element="D10" pad="C"/>
<contactref element="D9" pad="C"/>
<contactref element="J3" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="J25" pad="6"/>
</signal>
<signal name="ROW3">
<contactref element="D16" pad="C"/>
<contactref element="D13" pad="C"/>
<contactref element="D14" pad="C"/>
<contactref element="D15" pad="C"/>
<contactref element="J4" pad="1"/>
<contactref element="J8" pad="1"/>
<contactref element="J25" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="S9" pad="S2"/>
<contactref element="S9" pad="S3"/>
<contactref element="D9" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="S10" pad="S2"/>
<contactref element="S10" pad="S3"/>
<contactref element="D10" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="S11" pad="S2"/>
<contactref element="S11" pad="S3"/>
<contactref element="D11" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="S12" pad="S2"/>
<contactref element="S12" pad="S3"/>
<contactref element="D12" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="S16" pad="S2"/>
<contactref element="S16" pad="S3"/>
<contactref element="D16" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="S15" pad="S2"/>
<contactref element="S15" pad="S3"/>
<contactref element="D15" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="S14" pad="S2"/>
<contactref element="S14" pad="S3"/>
<contactref element="D14" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="S13" pad="S2"/>
<contactref element="S13" pad="S3"/>
<contactref element="D13" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="S5" pad="S2"/>
<contactref element="S5" pad="S3"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="S6" pad="S2"/>
<contactref element="S6" pad="S3"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="S7" pad="S2"/>
<contactref element="S7" pad="S3"/>
<contactref element="D7" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="S8" pad="S2"/>
<contactref element="S8" pad="S3"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="COL0">
<contactref element="S13" pad="S4"/>
<contactref element="S13" pad="S1"/>
<contactref element="S1" pad="S4"/>
<contactref element="S1" pad="S1"/>
<contactref element="S5" pad="S4"/>
<contactref element="S5" pad="S1"/>
<contactref element="S9" pad="S4"/>
<contactref element="S9" pad="S1"/>
<contactref element="J9" pad="1"/>
<contactref element="J25" pad="8"/>
</signal>
<signal name="COL1">
<contactref element="S14" pad="S4"/>
<contactref element="S14" pad="S1"/>
<contactref element="S10" pad="S4"/>
<contactref element="S10" pad="S1"/>
<contactref element="S6" pad="S4"/>
<contactref element="S6" pad="S1"/>
<contactref element="S2" pad="S4"/>
<contactref element="S2" pad="S1"/>
<contactref element="J10" pad="1"/>
<contactref element="J25" pad="9"/>
</signal>
<signal name="COL2">
<contactref element="S15" pad="S4"/>
<contactref element="S15" pad="S1"/>
<contactref element="S11" pad="S4"/>
<contactref element="S11" pad="S1"/>
<contactref element="S7" pad="S4"/>
<contactref element="S7" pad="S1"/>
<contactref element="S3" pad="S4"/>
<contactref element="S3" pad="S1"/>
<contactref element="J11" pad="1"/>
<contactref element="J25" pad="10"/>
</signal>
<signal name="COL3">
<contactref element="S16" pad="S4"/>
<contactref element="S16" pad="S1"/>
<contactref element="S4" pad="S4"/>
<contactref element="S4" pad="S1"/>
<contactref element="S8" pad="S4"/>
<contactref element="S8" pad="S1"/>
<contactref element="S12" pad="S4"/>
<contactref element="S12" pad="S1"/>
<contactref element="J12" pad="1"/>
<contactref element="J25" pad="11"/>
</signal>
<signal name="N$1">
</signal>
<signal name="COL8">
<contactref element="J26" pad="8"/>
<contactref element="J21" pad="1"/>
</signal>
<signal name="COL9">
<contactref element="J26" pad="7"/>
<contactref element="J22" pad="1"/>
</signal>
<signal name="COL10">
<contactref element="J26" pad="6"/>
<contactref element="J23" pad="1"/>
</signal>
<signal name="COL11">
<contactref element="J24" pad="1"/>
<contactref element="J26" pad="5"/>
</signal>
<signal name="COL4">
<contactref element="J13" pad="1"/>
<contactref element="J17" pad="1"/>
<contactref element="J25" pad="12"/>
</signal>
<signal name="COL5">
<contactref element="J14" pad="1"/>
<contactref element="J26" pad="12"/>
<contactref element="J18" pad="1"/>
</signal>
<signal name="COL6">
<contactref element="J15" pad="1"/>
<contactref element="J26" pad="10"/>
<contactref element="J19" pad="1"/>
</signal>
<signal name="COL7">
<contactref element="J16" pad="1"/>
<contactref element="J26" pad="9"/>
<contactref element="J20" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J25" pad="3"/>
<contactref element="J25" pad="4"/>
<contactref element="J26" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="J26" pad="4"/>
<contactref element="D22" pad="A"/>
<contactref element="D20" pad="A"/>
<contactref element="D21" pad="A"/>
<contactref element="D19" pad="A"/>
<contactref element="D17" pad="A"/>
<contactref element="D18" pad="A"/>
<contactref element="D25" pad="A"/>
<contactref element="D23" pad="A"/>
<contactref element="D24" pad="A"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$21">
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="D17" pad="C"/>
</signal>
<signal name="N$22">
<contactref element="R2" pad="2"/>
<contactref element="D18" pad="C"/>
</signal>
<signal name="N$23">
<contactref element="R3" pad="2"/>
<contactref element="D19" pad="C"/>
</signal>
<signal name="N$24">
<contactref element="R4" pad="2"/>
<contactref element="D20" pad="C"/>
</signal>
<signal name="N$25">
<contactref element="R5" pad="2"/>
<contactref element="D21" pad="C"/>
</signal>
<signal name="N$26">
<contactref element="R6" pad="2"/>
<contactref element="D22" pad="C"/>
</signal>
<signal name="N$27">
<contactref element="R7" pad="2"/>
<contactref element="D23" pad="C"/>
</signal>
<signal name="N$28">
<contactref element="R8" pad="2"/>
<contactref element="D24" pad="C"/>
</signal>
<signal name="N$29">
<contactref element="R9" pad="2"/>
<contactref element="D25" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
